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1 
introduction

The aim of this document is to provide the necessary information to connect client systems with the OTE system for the needs of automated communications of trading markets and to support the diostribution of financial reports (IS OTE).

It is both the technical part, i.e. a configuration of communication, which is mostly made up of links to documents containing detailed description of communication matters for all parts of the CS OTE system, and a part of the content, which specifies the data exchange, including the meaning of individual items.

This document describes the external interface that will be supported by the system after upgrade implementation that will take place on 1.1.2010. With regard to the ongoing implementation of the CS OTE Upgrade, further partial alterations and updates may occur in the specifications referred to this document. We will keep all participants informed shoud any changes take place. 

2 connecting the client system to the system operator

The aim of this chapter is to provide the users with the recommended process to connect to the CS OTE through the WEB services.

Each participant that wishes to connect to the Operator through the WEB service must realize that the Operator ensures only a certain part of the communication (from the point of view of the whole technological chain). The second part means the implementation of certain interventions on the side of the customer, including the eventual intervention to the client’s own infrastructure (especially for the server-server type of communication). 

The client must follow the following steps when establishing the automatic communication:

· Prepare a client infrastructure for the requested mode of communication. For the variants client-server (lower requirements on the side of the client) such a system must be prepared that will be configured to access the communication server of OTE (the client system may be in a security zone).  For the server-server variants (higher requirements on the client side) such a system must be created that will be configured to access the communication server of OTE and also the other way around to enable the access of the OTE communication server to the client system (the client system must be placed in a demilitarized zone).

· Prepare the client application, which would ensure the communication with the OTE server. This activity consists of a number of sub steps:

· Generation of data files for the individual instructions/processes of incoming messages. The structure of data files is published by the operator and it is available on the public web of the Operator (http://www.ote-cr.cz) in the document D1.4.2_ D1.4.2_Formaty_XML.doc (last version), for communication within BM, DM, IM&BalM, RRD and financial reports are relevant only for the description of the following messages:

· ISOTEDATA

· ISOTEREQ

· RESPONSE 

· SFVOTREQ

· SFVOTCLAIM

· SFVOTCLAIMSUM

· SFVOTBILLING

· SFVOTBILLINGEMO

· SFVOTBILLINGSUM

· SFVOTTDD

· SFVOTCONFDATA

· SFVOTDTEXPIMP

· Implementation of signing in/signing out routines 

· Pass data to appropriate web service with WS-Security header. The detailed description of the web service interface is stated in the document of external interface of the CS OTE system: HTTPS/SOAP. This document will be available on the public OTE web. 

· Creation/configuration of an application that ensures the exchange of data through the WEB services.

· Execution of the modification in the very trading system that enables the processing of data provided by OTE (in simpler cases it may be only the generation of instructions on the basis of manual activation; in a more complicated case the system may generate instructions by itself on the basis of the results of previous instructions, eventually on the basis of for example a selected model in the trading system of the client). 

· If the partner system is ready for communication, then the configuration of the Operator’s infrastructure (acc. to the type of communication) must take place. Eventually, to enable the communication between the parties, there might be a need to configure the client’s infrastructure, as well – the request must be escalated to the Operator. The Operator with the support of Logica, ensures for each communication type, within https communication the following activities:

	Step
	Description
	Executor

	1
	Retrieval of the request on the formats of outgoing messages for the respective external subject (individual message identifiers):

Data IM&BalM, DM, BM (input/output) – currently only in xml format (message ISOTEDATA*)

Outgoing confirmation messages:

· Format XML – message RESPONSE*

Request for data IM&BalM, DM, BM, RRD:

· Format XML – message ISOTEREQ*

Request for financial report data

· Format XML – message SFVOTREQ
Outgoing confirmation messages of financial reports

· Format XML – message RESPONSE

Outgoing reports

· Format XML – SFVOTCLAIM

· Format XML – SFVOTCLAIMSUM

· Format XML – SFVOTBILLING

· Format XML – SFVOTBILLINGEMO

· Format XML – SFVOTBILLINGSUM

· Format XML – SFVOTTDD

· Format XML – SFVOTCONFDATA

· Format XML – SFVOTDTEXPIMP
	OTE

	2
	Setup of the communication server WAS for the respective external subject acc. to point 1
	OTE

	3
	Retrieval of necessary information for the setup of CS OTE infrastructure (only for server-server type of communication):

· Socket (IP address and port) of the partner’s system

· Access certificate


	OTE

	4
	Certificate registration for https communication:

· SSL authentication

· Data signature
	OTE

	5
	Setup of the CS OTE infrastructure (only for server-server type of communication):

· Setup of security rules for the particular connection (setup of firewall for outgoing and incoming communication),

· Setup of the callback web services parameters
	Logica on the basis of the order

	6
	Verification of the communication format (SOAP communication)
	Logica on the basis of the order


3 Principle of Communication

3.1 Means of communication

To ensure the system-system type of automatic communication the principle of CDS communication, with all its benefits, is used (especially the possibility to communicate through more channels SMTP, HTTPs). 

As the communication server on the side of IS OTE the communication portal SAP WAS is used, which the part of CDS.

For the entire communication system relating to the IS OTE, new communication scenarios are defined, i.e. messages with unique identifiers (MSG_CODE). Definition and description of the individual scenarios is further specified in Chapter 4 Communication scenarios. 

At the same time there is a communication portal SAP WAS that is used as an outgoing gate for the distribution of messages of the EMTAS module (for those markets, where the AC is implemented).

All communication tasks that are ensured by the communication portal WAS are divided into 2 groups on the basis of processing:

· Synchronous communication – the exchange of data between CS OTE and the external system that runs with the help of the HTTPs channel and with the use of web services, for which an answer may be, and it is advisable, provided within one HTTPs session.
· Asynchronous communication – the exchange of data between CS OTE and the external system, which runs either through the HTTPs or the SMTP channel, within which there is no need (and in the case of the SMTP channel it is not even possible) to maintain a synchronous communication. The asynchronous communication through the HTTPs is possible in the case of client-server communication.

The following schemes describe the modes of communications for each mentioned case above:
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Figure 1 Synchronous request

In the case of a connection failure between the client (the participant’s system) and the server (WAS) the respective messages will be sent on the basis of previously agreed rules (asynchronous way through the use of the SMTP channel).  


[image: image2.emf]Client OTE com server CS OTE application

Message transfer

Response()

Service call -pick up()

Data

return code

Service call()

Pick up from the queue

Save to queue


Figure 2 Asynchronous request in client-server mode

The existence of web services is assumed solely for WAS (used only for IS OTE)
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Figure 3 Asynchronous request in server-server mode

Assumes the processing of requests through EMTAS, while the message on the evaluation of the process is send through the mail service WAS.

For detail description of web services formats and communication methods see the document D1.4.3 Web services interface.

3.2 Realization of communication channels

3.2.1 Description of the realization of synchronous processing through the WAS portal 

Synchronous processing through the HTTPs channel is used solely for a communication within the frame of the receipt of business instructions from external subjects, i.e. :

· Bid entry (MSG_CODE 851)

· Bid cancellation (MSG_CODE 861)

· Bid acceptance (MSG_CODE 871)

· DM bid entry (MSG_CODE 811)
· DM bid cancellation (MSG_CODE 821)
· BM order entry (MSG_CODE 854)
· BM order cancellation (MSG_CODE 857)
The reason for the use of synchronous communication for these requests is the necessity to immediately obtain the results of the EMTAS system processing. Thus for communication purposes through the http(s) channel solely synchronous communication is used (asynchronous communication with the http(s) channel is in this case insignificant). 

Synchronous processing of all messages will be done in ETSO format.

Processing plan of synchronous communication:

· The request is received through the http(s) handler through the SSL protocol. At the receipt of the handler the message is automatically encrypted.

· Through the PKI interface the signature is verified.

· From the body of the message the message code is ascertained and the respective transformation takes place. A message about the performed activities is created as a new object in the application log.

·  The final data after the transformation has been carried out, it is processed by the operator’s system according to the individual business instructions and the result of the request execution is ready for the external system.

· After the transformation of the process results the message is checked, whether it serves as an output for the open connection or the request falls under the sphere of asynchronous communication (in the case of such requests the final message is saved in the system until the withdrawal of the enquiry „921- Request for data handover IS OTE”). 
· After the transformation of all the blocks the output data is sent with the help of the output parameters of the function. Unsent messages (messages destined for other participants than for the partner of the open connection) are sent asynchronously. 
In the case of errors during data processing the following three statuses may arise:

1) Connection error during processing of requests within transactions. In this case the cancellation of all executed activities takes place. The reason value of the function called through SOSP is a nonzero one.  

2) Connection error after the finalization of the transaction in the business module (the instruction is successfully processed, the business position is changed). The request is arranged through standard asynchronous processing. 

3) Connection error when sending own output data. In this case the data is sent automatically with the WAS module through standard asynchronous processing.

The above mentioned error statuses 2 and 3, however, always signal such a situation for the external subject, where the HTTPs connection is interrupted and the external subject must manually confirm the result of the request. If the external system reacts in such a way that the previous request is repeated, then an unintentional change of the participant’s business position might take place. 
3.2.2 Description of the realization of asynchronous processing with the WAS portal through e-mail 

Asynchronous processing through the SMTP channel is used for all incoming requests concerning the communication within the IM&BalM, RRD, DM, BM and Settlement. For the communication within the IM&BalM, RRD, DM, BM and Settlement a new e-mail address is defined csote@csote.ote-cr.cz. 

Processing plan:

· The request is received by a standard way through the SMTP handler. 

· First the messages are encoded and the signature is verified, then the messages are sorted as CDS and IM&BalM. From the message body the message code is uncovered and the respective transformation takes place. The message created about the executed activities is saved by the system as a new object in the application log under a specific object for IM&BalM processing. 

· The final data for the execution of transformation is processed by the system operator, on the basis of individual enquiries and the result of the request processing is ready for the external system.  

· The request is closed after successful execution.

· Other processes correspond to standard request execution through asynchronous communication, which is elaborated on in Chapter 3.2.6 Data sending process within asynchronous communication.

The following statuses may arise in the case of errors during receipt of data:

1) Connection error during request processing (receipt) (process of requests within transactions). In this case all executed activities will be cancelled. Error message is sent – message type CONTROL.

3.2.3 Description of the realization of asynchronous processing with the WAS portal through https 

Asynchronous processing through the HTTPS channel is used solely for the communication within data request on the IM&BalM, DM, BM or trading results and financial reports, i.e. :

· Bid status determination
· Notice board data
· Market results
· Trading hours data
· DM bid status determination
· BM order status determination
· BM trade status determination
· BM instance (product) data 

· Data request - Final plan
· Data request – Hourly settlement
· Data request – Daily settlement
· Data request – Billing Report

· Data request – Billing Report – summary

· Data request – Billing Report OTE

· Data request – Billing Report OTE – summary

· Data request – Report of Claims
· Data request – Report of Claims – summary

· Data request – Report of Claims OTE
· Data request – Report of Claims OTE – summary

· Data request – Clearing of Load Profiles (TDD) Differences
· Data request – Clearing of Load Profiles (TDD) Differences OTE
· Data request – Billing Report PXE - OTE

· Data request – Billing Report OTE - PXE

· Data request – List of included receivables and payables

· Data request – List of included receivables and payables

· Results of DM by area
· Results of DM by SS
Processing of data handover IS OTE - MSG_CODE 921 (relevant solely for asynchronous communication HTTPs client-server type) is elaborated on in chapter 3.2.4 Receipt of special claims Request for data distribution IS OTE (MSG_CODE 921) asynchronous through https and requests for financial reports in chapter Receipt of special claims Request for financial report data asynchronously through https.

Processing plan: 

· The request is received through the http(s) handler through the SSL protocol. After the receipt of the handler the system automatically decodes the message. 

· With the PKI interface the signature is verified

· From the message body the message code is uncovered and the respective transformation takes place. The message created about the executed activities is saved by the system as a new object in the application log under a specific object for automatic communication processing. 

· After the successful receipt of the message by the integration platform the message RESPONSE is generated with identification for the recipient. The message RESPONSE is sent as an output parameter of the function. 

· After the transformation the final data is processed by the system operator on the basis of the individual requests and the result about the processing of the request is prepared for the external system.

· Further processing corresponds to the standard implementation of the request through asynchronous communication, which is described in 3.2.6 Data sending process within asynchronous communication .
In the case of errors during data reception the following status may arise: 

1) Connection error during processing (receipt) of requests (request processing within transaction). In this case all executed activities are cancelled. Error message is distributed.
3.2.4 Receipt of special claims Request for data distribution IS OTE (MSG_CODE 921) asynchronous through https 

Special type of claim for data is the Request for data distribution IS OTE  (MSG_CODE 921), which is solely used for asynchronous communication, type Client-Server for the withdrawal of process results of the previous data request. 

Processing plan:

· The request is received through the http(s) handler through the SSL protocol. After the receipt of the handler the message is automatically decoded.

· With the help of PKI interface the signature is validated.

· From the message body the message code is obtained and the respective transformation takes place.

· From the calling the identification of the message and from the PKI interface the RMP identification is obtained.

Afterwards the Table of unsent messages is checked, whether the request has been resolved (the receipt of requests is specified in chapter 3.2.3 Description of the realization of asynchronous processing with the WAS portal through https). If the check of tables is successful then the system sends the data to the respective MSG_ID. On the other hand, if the result of the checking process is negative, then a RESPONSE is sent with an error reason code – The request has not been executed yet.

In the case of an error during processing the following status may arise:

1) Connection failure during request processing. Reason value of the function that is called through SOAP will be nonzero. 

3.2.5 Receipt of special claims Request for financial report data asynchronously through https 

Special type of claim for data is the Request for report that is used solely for asynchronous communication, type Client-Server for the purposes of financial data withdrawal.

Processing plan:

· The request is received through http(s) handler through SSL protocol. After the receipt of the handler the system automatically decodes the message.

· With the PKI interface the signature is verified

· From the message body the message code is uncovered and the respective transformation takes place.

· From the calling the identification of the message and from the PKI interface the RMP identification is obtained.

Afterwards the Table of unsent messages is checked, whether the request has been resolved yet (the receipt of requests is specified in chapter 3.2.3 Description of the realization of asynchronous processing with the WAS portal through https 


). If the check of tables is successful then the system sends the data to the respective MSG_ID. On the other hand, if the result of the checking process is negative, then a RESPONSE is sent with an error reason code – The request has not been executed yet.

In the case of an error during processing the following status may arise:

2) Connection failure during request processing. Reason value of the function that is called through SOAP will be nonzero. 

3.2.6 Data sending process within asynchronous communication 

The process of sending output data means the asynchronous communication with the WAS system. 

Messages that have not been sent in a synchronous mode within the open connection are sent in a 5 minute cycle as follows:

· The table of unsent messages will be browsed and those messages that are waiting for sending will be tracked through the ID RMP and MSG_CODE from the table ZWAS_RUT_MAIL the mode and address of sending. Consequently these messages are sent by the system. 

· If the sending of the message was unsuccessful (in the case of sending data through https to the partner’s server), then the number of trials will be documented in the table of unsent messages. 

· In the case of 3 unsuccessful trials an electronic message will be sent to the default address of the RMP.

3.3 Identification of the time stamp for the receipt of business instructions through the communication portal WAS 

The need to set up a time stamp is relevant and it relates to all input messages that manipulate with business data:

· Bid entry (MSG_CODE 851)

· Bid cancellation (MSG_CODE 861)

· Bid acceptance (MSG_CODE 871)

· DM bid entry (MSG_CODE 811)
· DM bid cancellation (MSG_CODE 821)
· BM order entry (MSG_CODE 854)
· BM order cancellation (MSG_CODE 857)
· Submission of RD
When submitting instructions through the WAS portal the time stamp, which is being evaluated for request validity, is taken from the entry wall of the WAS portal.  

The time stamp is allocated to incoming messages as the system time of the WAS server (it is synchronized with the IS OTE time) as soon as:

· The incoming message has been received (after handover to the SMTP handler of the WAS system)


Warning: the time stamp is not relevant in the case of eventual queries from external subjects, because in the case of communication with an SMTP channel the period from sending the message to the external participant until receiving the message by the central system is not guaranteed. This point must be taken into account in the contractual relations between OTE and the external participant.

· The incoming message has been received by the HTTPs channel, the time stamp will be allocated in the second of invocation of the web service, thus before deciphering and verifying the signature. 

· The WAS system withdraws the data from the integration interface (outgoing message)

By the time stamp, specified above, the trabsactions are processed. With respect to the length of the technological chain, when processing requests through the WAS portal, one must count with a longer time of transaction completion in the business module. 

4 COMMUNICATION SCRIPTS

This Section describes the communication scripts for particular jobs, which can be performed within automatic communication.

4.1 Communication scripts  notification

Communication script when trade system give notice to surrounding systems about some actions or events. Notification will be send by using messages RESPONSE for all participiants who have access to respective market trade in relative trade day. 

4.1.1 Meaning of structure notification items – RESPONSE

	RESPONSE
	Meaning/Comment

	Message identifier
	In case of client – server comunication is using for request of process result 

	Message code
	Identification of message type – three alfa-numeric string

	Message create time
	precise creation time of message in format : 

yyyy-mm-ddThh:mm:ss

	Sender Identification
	Sender Identification. 

Market trade for Elektricity : EAN OTE (generally Operator)

Market trade for Gas: EIC OTE (generally Operator)

	Receiver Identification
	Receiver Identification. 

Market trade for Elektricity : EAN code

Market trade for Gas: EIC code

	Reason (message body)
	Text of reason, notification or error

	Reason Code (internal code)
	Internal identification of message type – three alfa-numeric string 

	Reason Type
	Number of notification or error


Structure of response is presented in chapter Summary of notification structure – RESPONSE - 5.11.1
4.2 IM&BalM Communication scripts 

Single items of this section are defined in the maximum classification, which means that some of them might be never used. 

4.2.1 Bid structure items meaning – ISOTEDATA/ISOTEREQ

Sentence-like command structure will consist of the following items (fields):

	ISOTEDATA
	Meaning/Comment
	ISOTEREQ

	Message code
	Message code that identifies message type.
	Yes

	ISOTEDATA/Trade
	Meaning/Comment
	

	Delivery day
	The date determined for the particular bid. Must be entered in the form  of YYYY-MM-DD.
	Yes

	Bid type
	Identifies the type of bid: Sell (P) or Buy (N).

Any trading is always a coupled action of a buy bid and a sell bid. Thus the acceptance bid is always of the opposite type than the accepted bid. So, in the balancing market it means:

· Supplier Party (offered on the notice board – accepted bid) – sell = RE+; buy = RE-

· Accepting party (accepts data on the notice board - acceptance bid) – sell = RE-; buy= RE+
	Yes

	Bid order
	The identification of the bid order within the delivery day, participant and bid type. In the case of replacing the bid, the item is filled with the order number of the replaced bid. In case of a new bid to be entered, the item is left blank.
	n/a

	Bid withdrawal time
	The time mark that defines the time of the bid withdraw from the notice board (in the form of  YYYY-MM-DDTHH:MI) 
	n/a

	Bid withdrawal time - attribute
	Identifies whether the specified time of the offer withdrawal applies to winter (Z) or summer (L) time. This item is taken into account only for the day of the transition from summer to winter time, and at the same time, exclusively for the real-time of the duplication (2:00 – 2:59). If specified, the item „Bid withdrawal time” must be filled in.
	n/a

	Total bid acceptance
	Identifies, whether the offer is considered as a whole - time indivisible (A), thus all trading hours must be traded simultaneously, or not (N), which means time divisible - each bid hour can be traded separately.
	n/a

	Comment
	Description, which the offer will be provided with. Maximum item length is 100 characters.
	n/a

	Bid cancellation time
	The time mark of the bid cancellation in the form of YYYY-MM-DDThh:mm:ss.
	n/a

	Bid ID
	Bid ID (identifier) used within EMTAS. This is a ten-digit number (code), which along with the bid version creates a unique bid identifier in the CS OTE system.
	Yes

	Bid version
	Bid version within EMTAS. This is a five-digit number, which along with the bid ID creates a unique bid identifier in the CS OTE system.
	Yes

	Replaced
	The attribute that indicates whether the bid was replaced.  

Then the existing bid, for which no energy has been traded, can be replaced with a new version (A – the bid was replaced, therefore no trade could be made with such a bid, N – not replaced with any other bid).
	n/a

	Bid origin
	In terms of the IM&BalM trading system all offers should be considered as an identical object, regardless of whether they were entered into the system as bids sent to be displayed on notice boards, or appeared as the result of the acceptance of an offer already displayed on the notice board. This attribute identifies the origin of the offer (A – acceptance bid – the bid appeared by acceptance of an existing bid on the notice board, N – bid – the bid was entered into the system to be displayed on the notice board).
	Yes

	Bid entry time
	The time mark, which indicates that the bid was entered into the system in the form of YYYY-MM-DDThh:mm:ss.
	n/a

	Error code
	Identification of errors that can occur during processing the request. Individual identifiers will be defined by a dial (section 4.14.3). If the item is not completed, the result of processing will be error-free.
	n/a

	Error reaction
	Identification of the system reaction rate during mass command data processing. A - apply changes only to the correctly processed commands, N – in case of error cancel the changes for all commands. The current version always processes only one command.
	n/a

	Market type
	Identification of the market for which the processing will be carried out; VDT – intraday market, VT – balancing market.
	Yes

	Participant – counterparty
	Identification of the Participant (EAN) in the role of a counterpart during bid acceptance in BalM – displayed only for TSO participants.
	n/a

	Settlement version
	Settlement version identification (2 - Daily Imbalance Settlement, 3 - Interim Monthly Settlement, 4 - Final Monthly Settlement).
	Yes

	ISOTEDATA/Trade/ProfileData
	Meaning/Comment
	

	Hour
	Identification of the trading hour for which the required action will be performed. The defined interval is 1 to 25, depending on the number of hours of a trading day. (winter/summer time shift – 23; summer/winter time shift – 25). Detailed records for each item must be clear and must be sorted in ascending order.
	Yes

	Volume
	Volume is determined for a specified trading hour. Volume is specified in tenth of MWh (the system can be switched to accept only whole MWh).
	n/a

	Price
	Price for one MWh. Price is defined in whole CZK.
	n/a

	Divisibility
	Volume divisibility of a specified bid’s trading hour (A – volume is divisible, N – volume is not divisible).
	n/a

	IM accepted
	Volume accepted within a specific trading hour on the IM. Volume is specified in tenth of MWh (the system can be switched to accept only whole MWh).
	n/a

	BalM accepted
	Volume accepted on the BalM within a specific trading hour. Volume is specified in tenth of MWh (the system can be switched to accept only whole MWh). In the event that it is a copy of the accepted bid data and the owner of this bid is a TSO Participant, there is a space for the sum of all already accepted volume, specifically the BalM accepted volume.
	n/a

	Open from
	The time mark, which indicates the trading hours open in the form of YYYY-MM-DDThh:mm:ss.
	n/a

	Open from - attribute
	Identifies whether the specified time of opening of trading hours apply to winter (Z) or summer (L) time.
	n/a

	Closed from
	The time mark, which indicates the trading hours close in the form of YYYY-MM-DDThh:mm:ss.
	n/a

	Closed from - attribute
	Identifies whether the specified time of closing of trading hours apply to winter (Z) or summer (L) time.
	n/a

	Cancelled
	The attribute of a trading hour cancel.
	n/a

	Aggregated
	The attribute of a trading hour aggregation.
	n/a

	ISOTEDATA/Trade/Party
	Meaning/Comment
	

	Participant (EAN)
	The unique Participant identifier within IS OTE (EAN). It will be transformed into RMP after being accepted by the system, and will be transformed into EAN again by data output.
	n/a


Ascertainment of the bid to IM&BalM, of whether it is valid in the sense of "it is possible to deal with it" is based on the following conditions:

1) The bid was successfully entered – the „Error code“ is blank.

2) The bid is not replaced with a different version – the „Replaced“ has the value „N“.

3) Within open trading hours the untraded energy volume is available.
4) The bid is not cancelled – the items „Bid cancellation time“ are blank.

5) The bid is not withdrawn from trading – the value of the „Bid withdrawal time“ item is higher than the current time or the items are blank.

4.2.2 Bid entry

The command will allow the entry/replacement of the bid in the trading module EMTAS. One command will contain exactly one bid entry.

4.2.2.1 Command – 851 (ISOTEDATA) 

The meaning of items is entirely consistent with the meanings specified in section 4.1.1 and in the structure set out in section 5.1.1. Mandatory fields are marked with hatching. Other items are optional. 

Additionally the following rules are valid: 

	ISOTEDATA/Trade
	Meaning/Comment

	Bid order
	In the case of replacing the bid, the item is filled with the order number of the replaced bid. In case of a new bid to be entered, the item is left blank.

	Bid withdrawal time - attribute
	This item is taken into account only for the day of the transition from summer to winter time, and at the same time, exclusively for the real-time of the duplication (2:00 – 2:59). If specified, the item „Bid withdrawal time” must be filled in.


4.2.2.2 Response – 852 (RESPONSE) 

The response structure is specified in section 4.14.1 with the general formats. 

4.2.2.3 Data transcript – 853 (ISOTEDATA) 

The data transcript structure is specified in section 4.2.11. with the general formats. Data transcript is created only if the command comes from the CDS and the bid was created. If the command comes from the EMTAS, then data transcript will be not created.

4.2.3 Bid cancellation

The request will allow cancellation of the EMTAS business module bid. The meaning of individual items is described below and is identical to cancellation through EMTAS.
One command will initiate cancellation of just one bid.

4.2.3.1 Command – 861 (ISOTEDATA) - Structure

The meaning of items is entirely consistent with the meanings specified in section 4.1.1 and in the structure set out in section 5.1.1. Mandatory fields are marked with hatching. Other items are optional. 

Additionally the following rules are valid: 

	ISOTEDATA/Trade
	Meaning/Comment

	Error reaction
	The entry must have the entire set of identical values in the whole file. The item is ready for mass cancellation, which is not supported in the automatic communication mode.


4.2.3.2 Response – 862 (RESPONSE) 

The response structure is specified in section 4.14.1 with the general formats. 

4.2.3.3 Data transcript – 863 (ISOTEDATA) 

The data transcript structure is specified in section 4.2.11. with the general formats. Data transcript is created only if the command comes from the CDS and the bid was cancelled. If the command comes from the EMTAS, then data transcript will be not created.
4.2.4 Bid acceptance

The command will allow the bid acceptance in the EMTAS business module. The meaning of individual items is shown below and is identical to acceptance through EMTAS.
One command will include the cancellation of just one bid.

4.2.4.1 Command – 871 (ISOTEDATA) - Structure

The meaning of items is entirely consistent with the meanings specified in section 4.1.1 and in the structure set out in section 5.1.1. Mandatory fields are marked with hatching. Other items are optional. 

4.2.4.2 Response – 872 (RESPONSE) 

The response structure is specified in section 4.14.1 with the general formats. 

4.2.4.3 Data transcript – 873 (ISOTEDATA) 

The data transcript structure is specified in section 4.2.11. with the general formats. Data transcript is created only if the command comes from the CDS and the acceptance bid was created. If the command comes from the EMTAS, then data transcript will be not created.
4.2.5 Bid status determination

The request will allow determining the bid status in the EMTAS module. One operation will process just one request to identify the bid status, the resulting response may contain none, one or a set of bids.

4.2.5.1 Request – 881 (ISOTEREQ)

The meaning of items is entirely consistent with the meanings specified in section 4.1.1 and in the structure set out in section 5.1.2. Mandatory fields are marked with hatching. Other items are optional. 

The query can be considered in two variants:

A – request for a specific bid: 

	ISOTEREQ/Trade
	Meaning/Comment

	Bid ID
	Mandatory field

	Bid version
	Mandatory field


B – request for all bids in a specified interval:
	ISOTEREQ/Trade
	Meaning/Comment

	Delivery day
	Mandatory field

	Bid origin
	Optional item – If the item is not specified, all bids will be selected. If specified, only that type of the offer will be selected.

	Hour
	Optional field – If the item is specified, the bid’s details for the particular hour will be selected. If not specified, all trading hours related to the specific bids will be selected.

	ISOTEREQ/Document
	Meaning/Comment

	Market type
	Optional field – If the item is specified, the bids, having traded for at least part of the energy on the specified market, will be selected. If the item is not specified, all bids are taken into account regardless of traded energy volume on both markets (including the bids that were not even partially accepted on any market).


If the request would contain completed items of both variants, option A is always preferred.
4.2.5.2 Response  – 882 (RESPONSE) 

The response structure is specified in section 4.14.1 with the general formats. 

4.2.5.3 Data transcript – 883 (ISOTEDATA) 

The data transcript structure is specified in section 4.2.11. with the general formats. 

The data transcript may generate several bids for a single request. This assumption is valid for variant B.

4.2.6 Resultant BalM prices 

The request will allow determining resultant prices of the traded bids on BalM. One operation will contain just one request to identify the resultant prices; the resulting response may be none, one or a set of results.

4.2.6.1 Command – 884 (ISOTEREQ)

The meaning of items is entirely consistent with the meanings specified in section 4.1.1 and in the structure set out in section 5.1.2. Mandatory fields are marked with hatching. Other items are optional. 

The query can be considered in two variants:

A – request for a specific bid and a settlement version: 

	ISOTEREQ/Trade
	Meaning/Comment

	Bid ID
	Mandatory field

	Bid version
	Mandatory field

	Settlement version
	Mandatory field (may contain following values: 2 - Daily Imbalance Settlement, 3 - Interim Monthly Settlement, 4 - Final Monthly Settlement)


B – request for all bids related to a specific day and a settlement version: 

	ISOTEREQ/Trade
	Meaning/Comment

	Delivery day
	Mandatory field

	Settlement version
	Mandatory field (may contain following values: 2 - Daily Imbalance Settlement, 3 - Interim Monthly Settlement, 4 - Final Monthly Settlement)


A combination of all parameters is allowed, anyway, if only the Settlement version field would be filled up in the request, the resulting response will contain an error message for incorrect parameters. 

If the request would contain completed items of both variants; the resulting response will contain a combination of all items.

4.2.6.2 Response – 885 (RESPONSE) 

The response structure is specified in section 4.14.1 with the general formats. 

4.2.6.3 Data transcript – 886 (ISOTEDATA) 

The data transcript structure is specified in section 4.2.11. with the general formats. 

The data transcript may generate several bids for a single request. This assumption is valid for variant B.
4.2.7 Notice board data 

The request will allow identifying notice board data in the EMTAS module. One operation will process just one request to identify the notice board status; the resulting response may contain none, one or a set of bids depending on the request type and on the open trading hours.

4.2.7.1 Request – 891 (ISOTEREQ)

The meaning of items is entirely consistent with the meanings specified in section 4.1.1 and in the structure set out in section 5.1.2. Mandatory fields are marked with hatching. Other items are optional.

	ISOTEREQ/Trade
	Meaning/Comment

	Hour
	Optional field – If the item is specified, the bid’s details for the particular hour will be selected (for time indivisible bids all open trading hours will be selected). If not specified, all trading hours related to the specific bids will be selected.

	Delivery day
	Mandatory field

	ISOTEREQ/Document
	Meaning/Comment

	Market type
	Mandatory field – defines the notice board, from which the required data were requested:

· “VDT“ – shows Notice board data of the IM market

· “VT“ – shows Notice board data of the BalM market


4.2.7.2 Response – 892 (RESPONSE) 

The response structure is specified in section 4.14.1 with the general formats. 

Additionally the following rules are valid for this part: 

	ISOTEDATA/Trade
	Meaning/Comment

	Bid ID
	The item is not indicated.

	Bid version
	The item is not indicated.


4.2.7.3 Data transcript – 893 (ISOTEDATA) 

The data transcript structure is specified in section 4.2.11. with the general formats. 

	ISTOTEDATA
	Meaning/Comment

	Participant (EAN)
	Identification of a participant that is the bid owner. The field would be filled up if the TSO owns the bid. Identification of the RMP is available only to a TSO participant, if at the same time, access to this item is available in the EMTAS module on the specific market.


The data transcript may generate several bids for a single request.
4.2.8 Market results 

As a result, we receive the total market (summary) data for the entire market. For the IM market The matter is referred to the total energy traded in the individual trading hours and the weighted average price mean of the energy traded in the individual trading hours.

For the BalM market the matter is referred to the total energy traded in the individual trading hours, divided up according to the type of the regulating energy RE+/RE- and the weighted average price (limit prices) mean submitted to the TSO. Data are similar to public groups WEB_20 and WEB_21. The request for BalM results is considered separately for the RE + and RE-.

4.2.8.1 Request – 901 (ISOTEREQ)

The meaning of items is entirely consistent with the meanings specified in section 4.1.1 and in the structure set out in section 5.1.2. Mandatory fields are marked with hatching. Other items are optional.

	ISOTEREQ/Trade
	Meaning/Comment

	Bid type
	This field is mandatory, if it is a question on the BalM market. Regulating energy is always considered on part of the supplier (SS) but not the ČEPS. It applies to the buy (N) that is negative regulating energy and the positive regulating energy – sell (P).

	Delivery day
	Mandatory field

	Hour
	Optional field – If the item is specified, the trading results for the particular hour will be selected. If not specified, all trading hours related to the specific market will be selected.

	ISOTEREQ/Document
	Meaning/Comment

	Market type
	Mandatory field – defines the notice board, from which the required data were requested:

· “VDT“ – shows Notice board data of the IM market

· “VT“ – shows Notice board data of the BalM market


4.2.8.2 Response – 902 (RESPONSE) 

The response structure is specified in section 4.14.1 with the general formats. 

Additionally the following rules are valid for this part: 

	ISOTEDATA/Trade
	Meaning/Comment

	Bid ID
	The item is not indicated.

	Bid version
	The item is not indicated.


4.2.8.3 Data transcript – 903 (ISOTEDATA) 

The data transcript structure is specified in section 4.2.11. 

For this request to the following items have an amended meaning:

	ISOTEDATA/Trade/ProfileData
	Meaning/Comment

	Volume
	Volume traded throughout the market

Volume is specified in tenth of MWh (the system can be switched to accept only whole MWh).

	Price
	The weighted average energy price (limit price) mean on the entire market is related to the traded volume.  Price stated in whole CZK.


4.2.9 Trading hours data

The request will identify the data of open trading hours in the EMTAS module. One task will contain just one requirement to identify the state of trading hours.

 One operation will process just one request to identify the trading hour’s status.

4.2.9.1 Request – 911 (ISOTEREQ)

The meaning of items is entirely consistent with the meanings specified in section 4.1.1 and in the structure set out in section 5.1.2. Mandatory fields are marked with hatching. Other items are optional.

	ISOTEREQ/Trade
	Meaning/Comment

	Hour
	Optional field – If the item is specified, the data for the particular hour will be selected. If not specified, all trading hours related to the specific delivery day will be selected.

	ISOTEREQ/Document
	Meaning/Comment

	Market type
	Mandatory field – defines the notice board, from which the required data were requested:

· “VDT“ – shows Notice board data of the IM market

· “VT“ – shows Notice board data of the BalM market


4.2.9.2 Response – 912 (RESPONSE) 

The response structure is specified in section 4.14.1 with the general formats. 

Additionally the following rules are valid for this part: 

	ISOTEDATA/Trade
	Meaning/Comment

	Bid ID
	The item is not indicated.

	Bid version
	The item is not indicated.


4.2.9.3 Data transcript – 913 (ISOTEDATA) 

The data transcript structure is specified in section 4.2.11. 

4.2.10 The IM&BalM data notice boards change message.

This is a communication script where the trade system transmits information to neighboring systems related the change of the IM&BalM notice boards that occurs after the transactions listed below:

· Bid Enter/Update

· Bid replacement

· Bid cancellation

· Bid modification with cancellation

· Bid acceptance

· IM&BalM trading hours open

· IM&BalM trading hours close

· Bid withdrawal

Notification will be sent in the form of RESPONSE message, together with a copy of the notice board data (ISOTEDATA) for all SS, who have the right to accept bids on the IM&BalM market. Notification will be generated automatically as part of the processing of registered data distribution requests of the amended notice board.

4.2.10.1 Response – 932 (RESPONSE)

The response structure is specified in section 4.14.1 with the general formats. 

Additionally the following rules are valid for this part: 

	RESPONSE/Reason
	Meaning/Comment

	Bid ID
	The item is not indicated.

	Bid version
	The item is not indicated.


4.2.10.2 Data transcript – 933 (ISOTEDATA)

The data transcript structure is specified in section 4.2.11. with the general formats.
The notice board can generate more bids in the data transcript.

4.2.11 Bid transcript general format (ISOTEDATA - 853, 863, 873, 883, 886)

The meaning of items is entirely consistent with the meanings specified in section 4.1.1 and in the structure set out in section 5.1.1. Mandatory fields are marked with hatching. Other items are optional.

4.3 DM communication scripts 

Single items of this section are defined in the maximum classification, which means that some items may be accumulated in a common format of the data into one item (e.g. items of a date type), or may not be used at all.

4.3.1 DM bid structure items meaning – ISOTEDATA/ISOTEREQ

The sentence structure will consist of the following items:

	ISOTEDATA
	Meaning/Comment
	ISOTEREQ

	Message code
	Message code that identifies a message type.
	Yes

	ISOTEDATA/Trade
	Meaning/Comment
	

	Delivery day
	Delivery day for which the bid was generated.  It means a date in the form of  YYYY-MM-DD.
	Yes

	Bid type
	Identifies whether it is a buy (N) or a sell (P) bid.
	Yes

	Block 1 total acceptance
	Identifies whether the participant agreed to accept the condition to apply overall acceptance of the first block (A) or not (N). This option applies only to selling (sell) bids. In case of buying (buy) bids only the value (N) is allowed.
	n/a

	Comment
	DM bid description. Maximum length is 30 characters.
	n/a

	Bid cancellation time
	The time mark of the bid cancellation in the form of YYYY-MM-DDThh:mm:ss.
	n/a

	Bid ID
	Bid ID (identifier) used within EMTAS. This is a seven-digit number. Along with bid version it is a unique bid identifier in the CS OTE system.
	Yes

	Bid version
	Bid version within EMTAS. This is a three-digit number. Along with bid ID it is a unique bid identifier in the CS OTE system.
	Yes

	Replaced
	Attribute that indicates, whether the bid was replaced with a new version (A – replaced, N – not replaced).
	n/a

	Default bid attribute
	Attribute that indicates, whether it was a DM default (A) bid or not (N). Currently, the system does not support default bids.
	n/a

	Bid entry time
	Time mark of the bid entry into the source system in form of YYYY-MM-DDThh:mm:ss. It is mandatory for bids intended for DM coordination.
	n/a

	Error code
	Identification of errors that can occur during processing the request. Individual identifiers will be defined by a dial (section 4.14.3). 
	n/a

	Settlement currency code
	Currency for Day-ahead market settlement (CZK/EUR).
	n/a

	Data source
	Identification of the source system, which received the bid (PXE/OTE).
	n/a

	Bid status
	Attribute that indicates, whether the bid is valid (P) or not (N). 
	n/a

	Bid cancellation attribute
	Attribute that indicates, whether the bid was cancelled (A) or not (N).
	n/a

	ISOTEDATA/Trade/ProfileData
	Meaning/Comment
	

	Hour
	Identification of the trading hour for which the required action will be performed. The defined interval is 1 to 25, depending on the number of hours of a trading day. (winter/summer time shift – 23; summer/winter time shift – 25). Detailed records for each item must be clear and must be sorted in ascending order.
	n/a

	Volume
	Volume is entered for a specified trading hour. Volume is specified in tenth of MWh.
	n/a

	Price
	Price for one MWh. Price is defined in whole EUR (historical price data can be still in CZK).
	n/a

	Block 1 volume divisibility
	Volume divisibility attribute will be taken into account only for block 1, but it must be entered for all blocks (A – volume is divisible, N – volume is not divisible).

Buy bids can only have the value A.
	n/a

	Trading block ID
	Trading block identification (BC01-25, BP01-25). For separate trading hours the item must be sorted in ascending order.
	n/a

	ISOTEDATA
	Meaning/Comment
	ISOTEREQ

	Participant (EAN)
	 

A unique identification of the participant within IS OTE (EAN). It means the participant that created a DM bid. Regarding the DM bid coordination the matter is referred to the anonymous participant code or EIC according to the anonymity settings. 
	n/a


4.3.2 DM bid entry

The request will allow the entry/replacement of the DM bid. The meaning of individual items is shown below and is identical to the entry through EMTAS.

 One operation will process exactly one bid.

4.3.2.1 Request – 811 (ISOTEDATA) 

The data sentence structure expected in the EMTAS module.

The meaning of items is entirely consistent with the meanings specified in section 4.2.1 and in the structure set out in section 5.2.1. Mandatory fields are marked with hatching. Other items are optional.

4.3.2.2 Response – 812 (RESPONSE)

The response structure is specified in section 4.14.1. with the general formats.
4.3.2.3 Data transcript – 813 (ISOTEDATA)

The data transcript structure is specified in section 4.3.5. with the general formats.
Data transcript is created only if the request comes from the automatic communication and the bid was created. If the request comes from the EMTAS, then data transcript will be not created.

4.3.3 DM bid cancellation

The request will allow the cancellation of the DM bid. The meaning of individual items is shown below and is identical to the cancellation through EMTAS.

One operation will process exactly one bid cancellation.

4.3.3.1 Request – 821 (ISOTEDATA) 

The meaning of items is entirely consistent with the meanings specified in section 4.2.1 and in the structure set out in section 5.2.1. Mandatory fields are marked with hatching. Other items are optional.

4.3.3.2 Response – 822 (RESPONSE)

The response structure is specified in section 4.14.1. with the general formats.
4.3.3.3 Data transcript – 823 (ISOTEDATA)

The data transcript structure is specified in section 4.3.5. with the general formats.
Data transcript is created only if the request comes from the automatic communication and the bid was cancelled. If the request comes from the EMTAS, then data transcript will be not created.

4.3.4 DM bid status determination

The request will allow identifying the DM bid status in the EMTAS module. One operation will process just one request to identify the bid status, the resulting response may contain none, one or a set of bids.

4.3.4.1 Request – 831 (ISOTEREQ) 

The data sentence structure expected in the EMTAS module.

The meaning of items is entirely consistent with the meanings specified in section 4.2.1 and in the structure set out in section 5.2.2. Mandatory fields are marked with hatching. Other items are optional.

The query can be considered in two variants:

A – request for a specific bid: 

	ISOTEDATA/Trade
	Meaning/Comment

	Bid ID
	Mandatory field

	Bid version
	Mandatory field


B – request for all bids related to a specific trading day:

	ISOTEDATA/Trade
	Meaning/Comment

	Delivery day
	Mandatory field


If the request would contain completed items of both variants, option A is always preferred.
4.3.4.2 Response – 832 (RESPONSE)

The response structure is specified in section 4.14.1. with the general formats.
4.3.4.3 Data transcript – 833 (ISOTEDATA)

The data transcript structure is specified in section 4.3.5. with the general formats.
The data transcript may generate several bids for a single request. This assumption is valid for the variant B.
4.3.5 DM bid transcript general format (ISOTEDATA - 813, 823, 833)

The meaning of items is entirely consistent with the meanings specified in section 4.2.1 and in the structure set out in section 5.2.1. Mandatory fields are marked with hatching. Other items are optional.

4.4 BM communication scripts 

Single items of this section are defined in the maximum classification, which means that some items may be accumulated in a common format of the data into one item (e.g. items of a date type), or may not be used at all.

4.4.1 BM order structure items meaning – ISOTEDATA/ISOTEREQ

The sentence structure will consist of the following items:

	ISTOTEDATA
	Meaning/Comment
	ISOTEREQ

	Message code
	Message code for identification of the message type.
	Yes

	ISOTEDATA/Trade
	Meaning/Comment
	

	Order type/Trade type
	Identifies whether it is a sell (P) or a buy (N) order / trade.
	n/a

	Instance title
	Maximum item length is 30 characters.
	Yes

	Order cancellation time
	Order cancellation time mark in form of YYYY-MM-DDThh:mm:ss.
	n/a

	Order code
	Order identification code used within EMTAS. This is a ten-digit number.
	Yes

	Automatic cancellation attribute
	The attribute that indicates, whether the order was automatically cancelled or cancelled by the user (A – automatically cancelled, U – cancelled by the user, if not cancelled the item is not indicated).
	n/a

	Order attribute - mode
	The attribute that indicates, whether the order was  entered in the market maker mode (T – market maker mode, not indicated for standard mode).
	n/a

	Order entry time /Trade creation time
	Order/trade entry time mark in form of YYYY-MM-DDThh:mm:ss.
	Yes

	Trading type
	Trading type, for which the order is determined (A – auction, K – continual, AK – auction and continual). Still always K.
	

	Order status
	The attribute that indicates, whether the order is valid (P) or invalid (N).
	n/a

	Trade code 
	Defines the identification code of created trade.
	Yes

	ISOTEDATA/Trade/ProfileData
	Meaning/Comment
	

	Order index 
	Identification of detail records. For the BM trading the following is valid: 1 – trade price and number of contracts, 2 – total price amount and traded volume. For the trading screen the following is valid: 1 to 5 – top 5 orders to buy, 6 to 10 – top 5 orders to sell, 11 – day statistics, 12 – product (instance) statistics.
	n/a

	Traded volume and Final price/Bottom price
	Indicates for the BM trading the specified instance traded volume. For the trading screen this indicates the latest traded order price of the specified instance (product) or the bottom price in daily statistics related to instance (product) trading.
	n/a

	Limit price, Trading price/Total price and Limit price/Ceiling price
	A limit price for one MWh in orders (price stated in whole CZK). A trade price or a total price for the BM trading. For the trading screen it means a limit price in orders  related to the specified instance (product) or a ceiling price  in daily statistics related to instance (product) trading.
	n/a

	Number of contracts
	A number of contracts in the order.
	n/a

	Number of traded contracts
	A number of BM traded contracts related to the specific instance (product).
	n/a

	ISOTEDATA/Trade/Party
	Meaning/Comment
	 

	Participant (EAN)
	A unique participant ID within IS OTE (EAN).
	n/a


A BM market order to be successful must meet following requirements:

1) The order must be successfully entered for a specific instance (product).

2) The order must be valid – the item „Order status” must have the value „P“.

3) The order must not be cancelled – the item „Automatic cancellation attribute“ must have no value - the field is blank.

4.4.2 BM order entry

This request will allow entering a new BM order with an option to cancel the order that was entered earlier. The meaning of individual items is shown below and is identical to the entry through EMTAS. 

One operation will process exactly one order entry.

4.4.2.1 Request – 854 (ISOTEDATA)

The meaning of items is entirely consistent with the meanings specified in section 4.3.1 and in the structure set out in section 5.3.1. Mandatory fields are marked with hatching. Other items are optional.

When entering a new order it is possible to specify a code of the existing order, which will be cancelled by this operation (the previously entered order will be replaced with a new one), if the existing order was not changed (already cancelled or traded). In the case that the order code is missing only a new order will be entered.

4.4.2.2 Response – 855 (RESPONSE)

The response structure is specified in section 4.14.1. with the general formats.
4.4.2.3 Data transcript – 856 (ISOTEDATA)

The data transcript structure is specified in section 4.4.13. with the general formats.
Data transcript is created only if the request comes from the automatic communication and the order was created. 
4.4.3 BM order cancellation

This request will allow cancelling a BM order. The meaning of individual items is shown below and is identical to the cancellation through EMTAS.
One operation will process exactly one order or a set of orders cancellation for a specific product (instance).

4.4.3.1 Request – 857 (ISOTEDATA) 

The meaning of items is entirely consistent with the meanings specified in section 4.3.1 and in the structure set out in section 5.3.1. Mandatory fields are marked with hatching. Other items are optional.

The cancellation can be considered in two variants:

A – cancellation of a specific order: 

	ISOTEDATA/Trade
	Meaning/Comment

	Order code
	Mandatory field


B – cancellation of all orders related to a specific instance (product):

	ISOTEDATA/Trade
	Meaning/Comment

	Instance title
	Mandatory field


4.4.3.2 Response – 858 (RESPONSE)

The response structure is specified in section 4.14.1. with the general formats.
4.4.3.3 Data transcript – 859 (ISOTEDATA)

The data transcript structure is specified in section 4.4.13. with the general formats.
Data transcript is created only if the request comes from the automatic communication and the order was cancelled. If the request comes from the EMTAS, then data transcript will be not created.
4.4.4 BM order status determination

The request will allow identifying the BM order status in the EMTAS module. One operation will process just one request to identify the order status, the resulting response may contain none, one or a set of orders.

4.4.4.1 Request – 864 (ISOTEREQ) 

The meaning of items is entirely consistent with the meanings specified in section 4.3.1 and in the structure set out in section 5.3. Mandatory fields are marked with hatching. Other items are optional.

The query can be considered in three variants:

A – request for a specific order: 

	ISOTEREQ/Trade
	Meaning/Comment

	Order code
	Mandatory field


B – request for an order related to a specific instance (product):

	ISOTEREQ/Trade
	Meaning/Comment

	Instance title
	Mandatory field


C – request for an order related to a specific order entry day:

	ISOTEREQ/Trade
	Meaning/Comment

	Order entry time 
	Mandatory field


If the request items would be filled up with two or all three variants, the request will be treated as an error query.

4.4.4.2 Response – 865 (RESPONSE)

The response structure is specified in section 4.14.1. with the general formats.
4.4.4.3 Data transcript – 866 (ISOTEDATA)

The data transcript structure is specified in section 4.4.13. with the general formats.
The data transcript may generate several orders for a single request. This assumption is valid for the variants B and C.
4.4.5 BM trade status determination

The request will allow identifying the BM trade status in the EMTAS module. One operation will process just one request to identify the trade status; the resulting response may contain none, one or a set of trades.

4.4.5.1 Request – 874 (ISOTEREQ) 

The data sentence structure expected in the EMTAS module.

The meaning of items is entirely consistent with the meanings specified in section 4.3.1 and in the structure set out in section 5.3.2. Mandatory fields are marked with hatching. Other items are optional.

The query can be considered in three variants:

A – request for a specific trade: 

	ISOTEREQ/Trade
	Meaning/Comment

	Trade code 
	Mandatory field


B – request for trades related to a specific instance (product):

	ISOTEREQ/Trade
	Meaning/Comment

	Instance title
	Mandatory field


C – request for trades related to a specific trade creation day:

	ISOTEREQ/Trade
	Meaning/Comment

	Trade creation time
	Mandatory field


If the request items would be filled up with two or all three variants, the request will be treated as an error query.

4.4.5.2 Response – 875 (RESPONSE)

The response structure is specified in section 4.14.1. with the general formats.
4.4.5.3 Data transcript – 876 (ISOTEDATA)

The data transcript structure is specified in section 4.4.13. with the general formats.
The data transcript may generate several trades for a single request. This assumption is valid for the variants B and C.
4.4.6 BM trading screen status change notification

This is a communication script where the trade system transmits information to the rest of the neighboring systems on the BM trading screen status changes that occur after the transactions listed below:

· Order entry

· Order cancellation by the user/system

Notification will be sent in the form of RESPONSE message along with the transcript trading screen status of the ISOTEDATA trading to all SS, which have the right to trade on BM.

4.4.6.1 Response – 868 (RESPONSE)

The response structure is specified in section 4.14.1 with the general formats. 

Additionally the following rules are valid for this part: 

	ISOTEDATA/Trade
	Meaning/Comment

	Order code
	The item is not indicated


4.4.6.2 Data transcript – 869 (ISOTEDATA)

The data transcript structure is specified in section 4.4.13. with the general formats.
The trading screen data transcript may generate several orders. 

4.4.7 BM notification of instance opening

This is a communication script where the trade system transmits information to the rest of the neighboring systems on a specific transaction, in this case – on the instance (product) opening. Notification will be sent in the form of RESPONSE message all SS, which have the right to trade on BM. When CDS mails are assigned to a specific message it is possible to take a decision for a separate SS, of whether such information would be transmitted to them or would remain at the CDS level in the unsent messages folder (or messages sent to the default CDS mail).

4.4.7.1 Response – 984 (RESPONSE) 

The response structure is specified in section 4.14.1 with the general formats.
4.4.8 BM notification of not opening an instance

This is a communication script where the trade system transmits information to the rest of the neighboring systems on a specific transaction, in this case – on the instance (product) not opening. Notification will be sent in the form of RESPONSE message all SS, which have the right to trade on BM. When CDS mails assigning to the specific message it is possible to take a decision for a separate SS, whether such information would be transmitted to them or would remain at the CDS level in the unsent messages folder (or messages sent to the default CDS mail).

4.4.8.1 Response – 988 (RESPONSE) 

The response structure is specified in section 4.14.1 with the general formats.
4.4.9 BM instance trading opening notification

This is a communication script where the trade system transmits information to the rest of the neighboring systems on a specific transaction, in this case – on the instance (product) trading opening. Notification will be sent in the form of RESPONSE message all SS, which have the right to trade on BM. When CDS mails assigning to the specific message it is possible to take a decision for a separate SS, whether such information would be transmitted to them or would remain at the CDS level in the unsent messages folder (or messages sent to the default CDS mail).

4.4.9.1 Response – 985 (RESPONSE) 

The response structure is specified in section 4.14.1 with the general formats.
4.4.10 BM instance trading closing notification

This is a communication script where the trade system transmits information to the rest of the neighboring systems on a specific transaction, in this case – on the instance (product) trading closing. Notification will be sent in the form of RESPONSE message all SS, which have the right to trade on BM. When CDS mails assigning to the specific message it is possible to take a decision for a separate SS, whether such information would be transmitted to them or would remain at the CDS level in the unsent messages folder (or messages sent to the default CDS mail).

4.4.10.1 Response – 986 (RESPONSE) 

The response structure is specified in section 4.14.1 with the general formats.
4.4.11 BM trading aggregation notification

This is a communication script where the trade system transmits information to the rest of the neighboring systems on a specific transaction, in this case – BM aggregation. Notification will be sent in the form of RESPONSE message all SS, which have the right to trade on BM. When CDS mails assigning to the specific message it is possible to take a decision for a separate SS, whether such information would be transmitted to them or would remain at the CDS level in the unsent messages folder (or messages sent to the default CDS mail). Notification will be generated automatically as part of the BM aggregation process in the phase next to the successful completion of aggregation.
4.4.11.1 Response – 983 (RESPONSE) 

The response structure is specified in section 4.14.1 with the general formats.
4.4.12 Instance trading results publishing notification

This is a communication script where the trade system transmits information to the rest of the neighboring systems on a specific transaction, in this case – instance trading results publishing. Notification will be sent in the form of RESPONSE message all SS, which have the right to trade on BM. When CDS mails assigning to the specific message it is possible to take a decision for a separate SS, whether such information would be transmitted to them or would remain at the CDS level in the unsent messages folder (or messages sent to the default CDS mail). 
4.4.12.1 Response – 987 (RESPONSE) 

The response structure is specified in section 4.14.1 with the general formats. 

4.4.13 BM order transcript general format (ISOTEDATA - 856, 859, 866, 869, 876)

The meaning of items is entirely consistent with the meanings specified in section 4.3.1 and in the structure set out in section 5.3.1. Mandatory fields are marked with hatching. Other items are optional.

4.5 Query communication script upon BM data instances (products)

4.5.1 BM instance (product) items structure determination – ISOTEMASTERDATA

Data structure will consist of the following items:

	ISOTEMASTERDATA
	Meaning/Comment

	Message code
	Message code that identifies a message type.

	ISOTEMASTERDATA/Instance
	Meaning/Comment

	Instance
	Product (instance) short title.

	Long instance title
	Product (instance) description.

	Instance class
	Specifies the instance (product) supply period length of the delivery of the product (a week or a day). Currently only the D (Daily) value may be selected. 

	Block type  
	Specifies the instance (product) supply period  interval (B – Baseload, P – Peakload, O – Offpeakload).

	Instance location
	Physical supply location. Assumed the Czech electricity system.

	Instance contract unit
	Contractual unit  (e.g., MWh).

	Instance currency unit
	Currency unit. This can have values in CZK and EUR (for future use).

	Settlement type
	Method of settlement of a completed trade (default PS – physical supply).

	Contract volume
	Volume of a single contract in terms of defined units. Technological limit is 0,1 – 999.

	Minimum supply volume
	Minimum supply volume is the product of the number of hours of the supply interval, number of days of the supply period and the minimum tradable unit (MWh).

	Initial delivery day
	The supply period initial day in the form of  YYYY-MM-DD.

	Final delivery day
	The supply period final day in the form of  YYYY-MM-DD.

	ISOTEMASTERDATA/Instance/Interval
	Meaning/Comment

	Order index
	The detail record order number.

	Supply interval
	The delivery day in the form of YYYY-MM-DD.

	Supply interval - initial period
	The initial trading hour index of the continuous interval of trading hours on the delivery day. It is a two-digit number, e.g. 01. The defined interval is 01 to 25 taking into account the number of hours of the day (default 24 hours, winter/summer time shift – 23; summer/winter time shift – 25).

	Supply interval – final period
	The final trading hour index of the continuous interval of trading hours on the delivery day. It is a two-digit number, e.g. 24. The defined interval is 01 to 25 taking into account the number of hours of the day (default 24 hours, winter/summer time shift – 23; summer/winter time shift – 25).

	Event title
	The time event title within the instance (product) life cycle:

· N_ISSUE – instance not opening notification,

· ISSUE - instance opening notification,

· TRC_START_MM – continual trading commencement  for the market maker,

· TRC_START_SS - continual trading commencement  for subjects of settlement,

· TRC_CLOSE - continual trading completion,

· AGGREG – data aggregation,

· PUBLICATION – data publishing

	Time of event
	The time mark of the event occurrence  in the form of YYYY-MM-DDThh:mm:ss.


4.5.2 BM instance (product) data

The request will allow identifying the instance (product) data in the EMTAS module. One operation will process just one request to identify the instance (product) data, the resulting response may contain none, one or a set of instances.

4.5.2.1 Request – 877 (ISOTEREQ) 

The meaning of items is entirely consistent with the meanings specified in section 4.4.1 and in the structure set out in section 5.4.2. Mandatory fields are marked with hatching. Other items are optional.

	ISOTEREQ/Trade
	Meaning/Comment

	Product
	Mandatory field – note: using the asterisk character as a wildcard marker (e.g., DB0801*) it is possible to enquire for more instances, then the request would process all daily baseload instances (products) related to January 2008.


4.5.2.2 Response – 878 (RESPONSE)

The response structure is specified in section 4.14.1 with the general formats. 

4.5.2.3 Data transcript – 879 (ISOTEMASTERDATA)

The meaning of items is entirely consistent with the meanings specified in section 4.4.1 and in the structure set out in section 5.4.1. Mandatory fields are marked with hatching. Other items are optional.

The data transcript may generate several instances for a single request. This assumption is valid for the variant of the use of the asterisk character as a wildcard marker in the instance title.

4.6 Communication scripts of DM results

This section describes a distribution procedure of Day-ahead market results received from the area and from the subject entities to the external organizer of the Day-ahead market, as well as the procedure of receiving the report message thereof from the external organizer of the Day-ahead market. 

This section describes particular scripts.

Single items of this section are defined in the maximum classification, which means that some items may be accumulated in a common format of the data into one item (e.g., items of a date type), or may not be used at all.

4.6.1 DM results items structure determination – ISOTEDATA

The sentence structure will consist of the following items:

	ISTOTEDATA
	Meaning/Comment

	Message code
	Message code that identifies the message type.

	ISOTEDATA/Trade
	Meaning/Comment

	Date/Delivery day
	Matching date/delivery day in the form of YYYY-MM-DD.

	Bid type
	Identifies  whether it is a buy (N) or a sell (P) bid. It is used only for the message 

 939.

	Matching ID
	A unique matching identifier within a specific day.

	Message code notification
	An identifying code for different DM trading results (states):

· RC001 – The bid was removed  by reason of complex indivisibility conditions
· RC002 - The bid was not matched by reason of optimizing the matching result (application of optimization criteria for maximizing the traded volume)

	Message text
	Only for reason code specification. The item (field) is optional.

	Bid ID
	Bid identification: 

· bids entered in the CZ – external  bid identifier (generated by a system on the part of recipient, i.e. the external Market operator system)

· bids entered in the SK – internal  bid identifier (generated by the CS OTE system)

	Bid version
	Bid version. Along with the bid ID it is a unique bid identifier. 

· bids entered in the CZ – external bid version (generated by a system on the part of recipient, i.e. the external Market operator system)

· bids entered in the SK – internal bid version (generated by the CS OTE system)

	Area
	Bid entry area identifier (CZ, SK).

	ISOTEDATA/Trade/ProfileData
	Meaning/Comment

	Hour
	A trading hour index related to a specified delivery day. The defined interval is 1 to 25 taking into account the number of hours of the trading day (winter/summer time shift – 23; summer/winter time shift – 25).

	Electricity/ Matched electricity
	The total volume of matched bids in the CZ and SK within a specified hour in MWh / matched electricity volume within a specified hour. If the item "Period matching attribute" = P, then the volume of matched electricity is less than the volume offered / demanded. If the item "Period matching attribute" = N, then the volume of matched electricity is equal to zero. If the item "Period matching attribute" = A, then the volume of matched electricity is equal to the volume offered / demanded.

	Period matching attribute
	The attribute of a total/all (A) or a partial (P) matching of the offered / demanded volume or of a not matched bid (N) within a specified hour.

	System price
	Marginal price resulted from a matching of bids in both areas within a specified hour. If during that hour the demand did not exceed the capacity profile (demand excess), items of "Price CZ", "Price SK" and "Price system" will have equal value. In case there occurred such a demand excess, values of those items may be different from each other.

	System volume 
	Marginal volume resulted from a matching of both areas within a specified hour. If during that hour the demand did not exceed the capacity profile (demand excess), the items "Total volume " and "System volume" will have equal value. In case there occurred such a demand excess, values of those items may be different from each other.

	Price CZ
	The marginal price of matched bids in the CZ within a specified hour (EUR).

	Volume CZ - sell
	Total volume of matched sell bids in the CZ within a specified hour (MWh).

	Volume CZ - buy
	Total volume of matched buy bids in the CZ within a specified hour (MWh).

	Price SK
	Marginal price of matched bids in the SK within a specified hour (EUR).

	Volume SK - sell
	Total volume of matched sell bids in the SK within a specified hour (MWh).

	Volume SK - buy
	Total volume of matched buy bids in the SK within a specified hour (MWh).

	Flow CZ => SK
	Energy flow from the CZ area to the SK area (export from the CZ). Settled as a difference between the CZ sell volume and the CZ buy volume within a specified hour. The item is specified only if the resulting value is positive or zero. Energy flow is 
specified as its absolute value.

	Requested flow CZ => SK
	Requested energy flow from the CZ area to the SK area (export from the CZ). In case that  the demand did not exceed the capacity profile (demand excess) in the appropriate direction, the item value is equal to the value of the resulting flow field (the value „Flow CZ => SK“). In case that  the demand exceeded the available capacity profile in the appropriate direction, the item value would exceed the value of the resulting flow and would also be higher than the available capacity profile in the appropriate direction.

	Flow SK => CZ
	Energy flow from the SK area to the CZ area (import into the CZ). Settled as a difference between the CZ sell volume and the CZ buy volume within a specified hour. The item is specified  only if the resulting value is negative or zero.

	Requested flow SK => CZ
	Energy flow from the SK area to the CZ area (export from the SK). In case that  the demand did not exceed the capacity profile (demand excess) in the appropriate direction, the item value is equal to the value of the resulting flow field (the item „Flow SK => CZ“). In case that  the demand exceeded the available capacity profile in the appropriate direction, the item value would exceed the value of the resulting flow and also be higher than the available capacity profile in the appropriate direction.

	Message code
	Notification or error message description specification at the level of a trading day hour (e.g. about marginal values missing by reason of buy or sell bids absence).

	Message text
	Notification or error message description specification at the level of a trading day hour. The field would be filled up in the case that it would be necessary to specify a notification or an error message, defined by the code.

	Profile ID
	Detailed information on the identification of profiles is specified in section

5.13 Allocation of profiles to IS OTE data.

	ISOTEDATA/Trade/Party
	Meaning/Comment

	Participant (EAN)
	Unique participant identification within IS OTE (EAN) . It means the participant  that is a DM bid owner. Regarding the DM coordination bids the matter is referred to the anonymous participant code, or EIC according to the anonymity settings.


4.6.2 DM results in the area

The request will allow receiving/sending DM results in the area. The meaning of individual items is described below. 

One operation will process the DM results of just one day.

4.6.2.1 Request – 936 (ISOTEDATA) 

The meaning of items is entirely consistent with the meanings specified in section 4.5.1 and in the structure set out in section 5.5. Mandatory fields are marked with hatching. Other items are optional.

Additionally the following rules are valid:

	ISOTEDATA/Trade
	Meaning/Comment

	Message code notification
	Identifying codes for various notification types related to the DM results in the area:

· RC006 - Marginal values determining has not taken place within any matching period. All sell bids were removed  by reason of complex indivisibility conditions.

	ISOTEDATA/Trade/ProfileData
	Meaning/Comment

	Hour
	The hour with the index 25 (winter/summer time shift – 24; summer/winter time shift – 26) identifies a record containing daily statistics of all hours of the day.

	Electricity
	A total volume of matched bids in the CZ and SK within a specified hour (MWh).

	Message code
	Notification or error message description specification at the level of a trading day hour (e.g. about marginal values missing by reason of buy or sell bids absence):

· RC007 – No buy bids within a period. No marginal values were determined for that period.
· RC008 - No sell bids within a period. No marginal values were determined for that period.
· RC009 - All sell bids within a period were removed by reason of complex indivisibility conditions. No marginal values were determined for that period.


4.6.3 DM results related to SS

Request will allow receiving/sending DM results related to particular subjects/participants. The meaning of individual items is described below. 

One operation will process DM results related to particular subjects/participants of just one day. This message (report) will contain a set of results related to particular subjects.

4.6.3.1 Request – 939 (ISOTEDATA) 

The meaning of items is entirely consistent with the meanings specified in section 4.5.1 and in the structure set out in section 5.5. Mandatory fields are marked with hatching. Other items are optional.

Additionally the following rules are valid:

	ISOTEDATA/Trade
	Meaning/Comment

	Message code Notification
	Identifying codes for various notification types related to the DM results in the area:

· RC001 – The bid was removed by reason of complex indivisibility conditions.
· RC002 - The bid was not matched by reason of optimizing the matching result (application of optimization criteria for maximizing the traded volume).

	ISOTEDATA/Trade/ProfileData
	Meaning/Comment

	Matched electricity
	The total volume of matched electricity within a specified hour. If the item "Period matching attribute" = P, then the volume of matched electricity is less than the volume offered / demanded. If the item "Bid matching attribute" = N, then the volume of matched electricity is equal to zero. If the item "Bid matching attribute" = A, then the volume of matched electricity is equal to the volume offered / demanded.

	Message code
	Notification or error message description specification at the level of a trading day hour (e.g. about marginal values missing by reason of buy or sell bids absence):

· RC003 – The bid was not matched within a specified period.  The price does not match defined marginal values.
· RC004 – Matched partially by reason of volume splitting.
· RC005 – The block was removed by reason of volume indivisibility conditions related to the block 1 bid component.


XML files contain extended structure with an option to repeat the ProcReason element

4.6.4 DM trade results determination in the area 

The request will allow the external market initiator to determine DM trade results in the area. One operation will process just one request to determine the DM trade results in the area.
4.6.4.1 Request – 934 (ISOTEREQ)

The meaning of items is entirely consistent with the meanings specified in section 4.5.1 and in the structure set out in section 5.5. Mandatory fields are marked with hatching. Other items are optional.

The query can be considered for a specific day:

	ISOTEREQ/Trade
	Meaning/Comment

	Date
	Mandatory field


4.6.4.2 Response – 935 (RESPONSE) 

The response structure is specified in section 4.14.1 with the general formats. 

4.6.4.3 Data transcript – 936 (ISOTEDATA) 

The data transcript structure is specified in section 5.5. 

4.6.5 DM SS trade results determination 

The request will allow the external market initiator to determine DM trade results related to specific SS. One operation will process just one request to determine the DM trade results related to specific SS.

4.6.5.1 Request – 937 (ISOTEREQ)

The meaning of items is entirely consistent with the meanings specified in section 4.5.1 and in the structure set out in section 5.5. Mandatory fields are marked with hatching. Other items are optional.

The query can be considered for a specific day:

	ISOTEREQ/Trade
	Meaning/Comment

	Date
	Mandatory field


4.6.5.2 Response – 938 (RESPONSE) 

The response structure is specified in section 4.14.1 with the general formats. 

4.6.5.3 Data transcript – 939 (ISOTEDATA) 

The data transcript structure is specified in section 5.5.1. The data transcript may generate several SS trade results for a single request.

4.6.6 Notification about change (shift) of gate closure time – 981 (RESPONSE) 

Notification about change (shift) of gate closure time in DM (time) . Notification about shift of publication of results in DM(time). 

Structure of response is presented in chapter 4.1.1 and Summary of notification structure – RESPONSE in chapter 5.11.1
4.7 Communications scripts for gas DM

Single items of this section are defined in the maximum classification, which means that some items may be accumulated in a common format of the data into one item (e.g., items of a date type), or may not be used at all.
4.7.1 DM bid structure items meaning – ISOTEDATA/ISOTEREQ
The sentence structure will consist of the following items: 

	ISOTEDATA
	Meaning/Comment
	ISOTEREQ

	Message code
	Message code that identifies a message type.
	Yes

	Commodity code
	Commodity is type of energy, which is traded on energy market. System support trading for commodities electricity (E) and gas (P).
	n/a

	ISOTEDATA/Trade
	Meaning/Comment
	

	Gas day
	Gas day for which the bid was generated.  It means a date in the form of  YYYY-MM-DD.
	Yes

	Session
	Time interval pro trading on day market: morning (1), afternoon (2)
	Yes

	Bid type
	Identifies whether it is a buy (N) or a sell (P) bid.
	n/a

	Comment
	DM bid description. Maximum length is 30 characters.
	n/a

	Bid cancellation time
	The time mark of the bid cancellation in the form of YYYY-MM-DDThh:mm:ss.
	n/a

	Bid ID
	Bid ID (identifier) used within EMTAS. This is a seven-digit number. Along with bid version it is a unique bid identifier in the CS OTE system.
	Yes

	Bid version
	Bid version within EMTAS. This is a three-digit number. Along with bid ID it is a unique bid identifier in the CS OTE system.
	Yes

	Replaced
	Attribute that indicates, whether the bid was replaced with a new version (A – replaced, N – not replaced).
	n/a

	Bid entry time
	Time mark of the bid entry into the source system in form of YYYY-MM-DDThh:mm:ss. It is mandatory for bids intended for gas DM coordination.
	n/a

	Error code
	Identification of errors that can occur during processing the request. Individual identifiers will be defined by a dial (section 4.14.3). 
	n/a

	Settlement currency code
	Currency for gas DM settlement (CZK/EUR).
	n/a

	Data source
	Identification of the source system, which received the bid (PXE/OTE).
	n/a

	Bid status
	Attribute that indicates, whether the bid is valid (P) or not (N). 
	n/a

	Bid cancellation attribute
	Attribute that indicates, whether the bid was cancelled (A) or not (N).
	n/a

	ISOTEDATA/Trade/ProfileData
	Meaning/Comment
	

	Interval
	Identification of time interval for which the required action will be performed. The defined interval is always one gas day (1).
	n/a

	Volume
	Volume is entered for a specified trading interval. Volume is specified in tenth of MWh.
	n/a

	Price
	Price for one MWh of gas. Price is defined in whole EUR.
	n/a

	Block 1 volume divisibility
	Volume divisibility attribute will be taken into account only for block 1, but it must be entered for all blocks (A – volume is divisible, N – volume is not divisible).

Buy bids can only have the value A.
	n/a

	Trading block ID
	Trading block identification (BC01-25, BP01-25). For bids for sell, prices in blocks must be sorted in ascending order. For bids for buy, prices in blocks must be sorted in descending order.
	n/a

	ISOTEDATA/Trade/Party
	Meaning/Comment
	ISOTEREQ

	Participant (EIC)
	A unique identification of the participant within IS OTE (EIC). It is the participant that created a Gas DM bid. Regarding the DM bid coordination the matter is referred to the anonymous participant code or EIC according to the anonymity settings. 
	n/a


4.7.2 Gas DM bid entry

The request will allow the entry/replacement of the gas DM bid. The meaning of individual items is shown below and is identical to the entry through EMTAS.

 One operation will process exactly one bid.

4.7.2.1 Request – GD1 (ISOTEREQ) 

The data sentence structure expected in the EMTAS module.

The meaning of items is entirely consistent with the meanings specified in section 4.7.1 and in the structure set out in section 5.8. Mandatory fields are marked with hatching. Other items are optional.

4.7.2.2 Response – GD2 (RESPONSE)

The response structure is specified in section 4.14.1 with the general formats. 

4.7.2.3 Data transcript – GD3 (ISOTEDATA)

The data transcript structure is specified in section 4.7.5 with the general formats. Data transcript is created only if the request comes from the automatic communication and the bid was created. If the request comes from the EMTAS, then data transcript will be not created.
4.7.3 Gas DM bid cancellation

The request will allow the cancellation of the Gas DM bid. The meaning of individual items is shown below and is identical to the cancellation through EMTAS . 

One operation will process exactly one bid cancellation.

4.7.3.1 Request – GD4 (ISOTEREQ) 

The meaning of items is entirely consistent with the meanings specified in 4.7.1 and in the structure set out in section 5.8. Mandatory fields are marked with hatching. Other items are optional.

4.7.3.2 Response – GD5 (RESPONSE) 

The response structure is specified in section  4.14.1. with the general formats 

4.7.3.3 Data transcript – GD6 (ISOTEDATA)

The data transcript structure is specified in section  4.7.5 with the general formats.

Data transcript is created only if the request comes from the automatic communication and the bid was cancelled. If the request comes from the EMTAS, then data transcript will be not created.

4.7.4 Gas DM bid status determination

The request will allow identifying the Gas DM bid status in the EMTAS module. One operation will process just one request to identify the bid status, the resulting response may contain none, one or a set of bids.
4.7.4.1 Request – GD7 (ISOTEREQ) 

The data sentence structure expected in the EMTAS module.

The meaning of items is entirely consistent with the meanings specified in section 4.7.1 and in the structure set out in section 5.8. Mandatory fields are marked with hatching. Other items are optional.

The query can be considered in two variants:

A – request for a specific bid: 

	ISOTEREQ/Trade
	Meaning/Comment

	Bid ID
	Mandatory field

	Bid version
	Mandatory field


B – request for all bids related to a specific trading day:

	ISOTEREQ/Trade
	Meaning/Comment

	Gas day
	Mandatory field

	Session
	Optional field


If the request would contain completed items of both variants, option A is always preferred.
4.7.4.2 Response – GD8 (RESPONSE)

The response structure is specified in section  4.14.1 with the general formats. 

4.7.4.3 Data transcript – GD9 (ISOTEDATA)

The data transcript structure is specified in section  4.7.5 with the general formats.

The data transcript may generate several bids for a single request. This assumption is valid for the variant B.

4.7.5 Gas DM bid transcript general format (ISOTEDATA – GD3, GD6, GD9)

The meaning of items is entirely consistent with the meanings specified in section 4.7.1 and in the structure set out in section 5.8. Mandatory fields are marked with hatching. Other items are optional.

4.7.6 Notification about change (shift) of gate closure time – 981 (RESPONSE) 

Notification about change (shift) of gate closure time in GAS DM (time) . 

Structure of response is presented in chapter 4.1.1 and Summary of notification structure – RESPONSE in chapter 5.11.1
4.8 Gas IM communication scripts

Single items of this section are defined in the maximum classification, which means that some items may be accumulated in a common format of the data into one item (e.g. items of a date type), or may not be used at all. 
4.8.1 Gas IM order structure items meaning – ISOTEDATA/ISOTEREQ
The sentence structure will consist of the following items:

	ISOTEDATA
	Meaning/Comment
	ISOTEREQ

	Message code
	Message code for identification of the message type.
	Yes

	ISOTEDATA/Trade
	Meaning/Comment
	 

	Order type/Trade type
	Identifies whether it is a sell (P) or a buy (N) order / trade.
	n/a

	Instance title
	Maximum item length is 30 characters.
	Yes

	Order cancellation time
	Order cancellation time mark in form of YYYY-MM-DDThh:mm:ss.
	n/a

	Order code
	Order identification code used within EMTAS. This is a ten-digit number.
	Yes

	Automatic cancellation attribute
	The attribute that indicates, whether the order was automatically cancelled or cancelled by the user (A – automatically cancelled, U – cancelled by the user, if not cancelled the item is not indicated).
	n/a

	Order attribute - mode
	The attribute that indicates, whether the order was  entered in the market maker mode (T – market maker mode, not indicated for standard mode).
	n/a

	Order entry time /Trade creation time
	Order/trade entry time mark in form of YYYY-MM-DDThh:mm:ss.
	Yes

	Trading type
	Trading type, for which the order is determined (A – auction, K – continual, AK – auction and continual). Still always K.
	n/a

	Order status
	The attribute that indicates, whether the order is valid (P) or invalid (N).
	n/a

	Trade code 
	Defines the identification code of created trade.
	Yes

	ISOTEDATA/Trade/ProfileData
	Meaning/Comment
	 

	Order index
	Identification of detail records. For the Gas IM trading the following is valid: 1 – trade price and number of contracts, 2 – total price amount and traded volume.
	n/a

	Traded volume and Final price/Bottom price
	Indicates traded volume for specified product of Gas IM..
	n/a

	Limit price, Trading price/Total price and Limit price/Ceiling price
	A limit price for one unit of MWh in orders (price stated in CZK, with precision of 2 decimals). A trade price or a total price for the Gas IM trading.
	n/a

	Number of contracts
	A number of contracts in the order.
	n/a

	Number of traded contracts
	A number of Gas IM traded contracts related to the specific instance (product).
	n/a

	ISOTEDATA/Trade/Party
	Meaning/Comment
	 

	Participant (EIC)
	A unique participant ID within IS OTE (EIC).
	n/a


A Gas IM market order to be successful must meet following requirements:

4) The order must be successfully entered for a specific instance (product).

5) The order must be valid – the item „Order status” must have the value „P“.

6) The order must not be cancelled – the item „Automatic cancellation attribute“ must have no value - the field is blank.

4.8.2 Gas IM order entry
This request will allow entering a new Gas IM order with an option to cancel the order that was entered earlier. The meaning of individual items is shown below and is identical to the entry through EMTAS.

One operation will process exactly one order entry.

4.8.2.1 Request – GV1 (ISOTEREQ)

The meaning of items is entirely consistent with the meanings specified in section 4.8.1 and in the structure set out in section 5.6. Mandatory fields are marked with hatching. Other items are optional.

4.8.2.2 Response – GV2 (RESPONSE)

The response structure is specified in section 4.14.1 with the general formats. 

4.8.2.3 Data transcript – GV3 (ISOTEDATA)

The data transcript structure is specified in section 4.8.13 with the general formats. Data transcript is created only if the request comes from the automatic communication and the order was created. 

4.8.3 Gas IM order cancellation

This request will allow cancelling a Gas IM order. The meaning of individual items is shown below and is identical to the cancellation through EMTAS.
One operation will process exactly one order or a set of orders cancellation for a specific product (instance).

4.8.3.1 Request – GV4 (ISOTEREQ) 

The meaning of items is entirely consistent with the meanings specified in section 4.8.1 and in the structure set out in section 5.6. Mandatory fields are marked with hatching. Other items are optional.

The cancellation can be considered in two variants:

A – cancellation of a specific order: 

	ISOTEREQ/Trade
	Meaning/Comment

	Order code
	Mandatory field


B – cancellation of all orders related to a specific product:

	ISOTEREQ/Trade
	Meaning/Comment

	Product name
	Mandatory field


4.8.3.2 Response – GV5 (RESPONSE)

The response structure is specified in section 4.14.1 with the general formats. 

4.8.3.3 Data transcript – GV6 (ISOTEDATA)

The data transcript structure is specified in section 4.8.13 with the general formats. Data transcript is created only if the request comes from the automatic communication and the order was cancelled. If the request comes from the EMTAS, then data transcript will be not created.
4.8.4 Gas IM order status determination

The request will allow identifying the Gas IM order status in the EMTAS module. One operation will process just one request to identify the order status, the resulting response may contain none, one or a set of orders.

4.8.4.1 Request– GV7 (ISOTEREQ) 

The meaning of items is entirely consistent with the meanings specified in section 4.8.1 and in the structure set out in section 5.6. Mandatory fields are marked with hatching. Other items are optional.

The query can be considered in three variants:

A – request for a specific order: 

	ISOTEREQ/Trade
	Meaning/Comment

	Order code
	Mandatory field


B – request for an order related to a specific product:

	ISOTEREQ/Trade
	Meaning/Comment

	Product name
	Mandatory field


C – request for an order related to a specific order entry day:

	ISOTEREQ/Trade
	Meaning/Comment

	Order entry time
	Mandatory field


If the request items would be filled up with two or all three variants, the request will be treated as an error query.

4.8.4.2 Response – GV8 (RESPONSE)

The response structure is specified in section 4.14.1 with the general formats. 

4.8.4.3 Data transcript – GV9 (ISOTEDATA)

The data transcript structure is specified in section 4.8.13 with the general formats.

The data transcript may generate several orders for a single request. This assumption is valid for the variants B and C.

4.8.5 Gas IM trade status determination
The request will allow identifying the Gas IM trade status in the EMTAS module. One operation will process just one request to identify the trade status; the resulting response may contain none, one or a set of trades.

4.8.5.1 Request– GVC (ISOTEREQ) 

The data sentence structure expected in the EMTAS module.

The meaning of items is entirely consistent with the meanings specified in section 4.8.1 and in the structure set out in section 5.6. Mandatory fields are marked with hatching. Other items are optional.

The query can be considered in three variants:

A – request for a specific trade: 

	ISOTEREQ/Trade
	Meaning/Comment

	Trade code
	Mandatory field


B – request for trades related to a specific product:

	ISOTEREQ/Trade
	Meaning/Comment

	Product name
	Mandatory field


C – request for trades related to a specific trade creation day:

	ISOTEREQ/Trade
	Meaning/Comment

	Trade creation time
	Mandatory field


If the request items would be filled up with two or all three variants, the request will be treated as an error query.

4.8.5.2 Response – GVD (RESPONSE)

The response structure is specified in section 4.14.1 with the general formats. 

4.8.5.3 Data transcript – GVE (ISOTEDATA)

The data transcript structure is specified in section 4.8.13 with the general formats.

The data transcript may generate several trades for a single request. This assumption is valid for the variants B and C.  

4.8.6 Gas IM trading screen status change notification
This is a communication script where the trade system transmits information to the rest of the neighboring systems on the Gas IM trading screen status changes that occur after the transactions listed below:

· Order entry
· Order cancellation by the user/system
Notification will be sent in the form of RESPONSE message along with the transcript trading screen status of the ISOTEDATA trading to all SS, which have the right to trade on Gas IM.

4.8.6.1 Response – GVJ (RESPONSE)

The response structure is specified in section 4.14.1 with the general formats. Additionally the following rules are valid for this part:

	ISOTEDATA/Trade
	Meaning/Comment

	Order code
	The item is not indicated


4.8.6.2 Data transcript – GVK (ISOTEDATA)

The data transcript structure is specified in section  4.8.13. with the general formats. 

The trading screen data transcript may generate several orders.

4.8.7 Gas IM notification of instance opening

This is a communication script where the trade system transmits information to the rest of the neighboring systems on a specific transaction, in this case – on the instance (product) opening. Notification will be sent in the form of RESPONSE message all SS, which have the right to trade on Gas IM. When CDS mails are assigned to a specific message it is possible to take a decision for a separate SS, of whether such information would be transmitted to them or would remain at the CDS level in the unsent messages folder (or messages sent to the default CDS mail).
4.8.7.1 Response – 984 (RESPONSE) 

The response structure is specified in section 4.14.1 with the general formats. 

4.8.8 Gas IM notification of not opening an instance
This is a communication script where the trade system transmits information to the rest of the neighboring systems on a specific transaction, in this case – on the instance (product) not opening. Notification will be sent in the form of RESPONSE message all SS, which have the right to trade on Gas IM. When CDS mails assigning to the specific message it is possible to take a decision for a separate SS, whether such information would be transmitted to them or would remain at the CDS level in the unsent messages folder (or messages sent to the default CDS mail).

4.8.8.1 Response – 988 (RESPONSE) 

The response structure is specified in section 4.14.1 with the general formats. 

4.8.9 Gas IM instance trading opening notification
This is a communication script where the trade system transmits information to the rest of the neighboring systems on a specific transaction, in this case – on the instance (product) trading opening. Notification will be sent in the form of RESPONSE message all SS, which have the right to trade on Gas IM. When CDS mails assigning to the specific message it is possible to take a decision for a separate SS, whether such information would be transmitted to them or would remain at the CDS level in the unsent messages folder (or messages sent to the default CDS mail).

4.8.9.1 Response – 985 (RESPONSE) 

The response structure is specified in section 4.14.1 with the general formats. 

4.8.10 Gas IM instance trading closing notification
This is a communication script where the trade system transmits information to the rest of the neighboring systems on a specific transaction, in this case – on the instance (product) trading closing. Notification will be sent in the form of RESPONSE message all SS, which have the right to trade on Gas IM. When CDS mails assigning to the specific message it is possible to take a decision for a separate SS, whether such information would be transmitted to them or would remain at the CDS level in the unsent messages folder (or messages sent to the default CDS mail).

4.8.10.1 Response – 986 (RESPONSE) 

The response structure is specified in section 4.14.1 with the general formats. 

4.8.11 Gas IM trading aggregation notification
This is a communication script where the trade system transmits information to the rest of the neighboring systems on a specific transaction, in this case – Gas IM aggregation. Notification will be sent in the form of RESPONSE message all SS, which have the right to trade on Gas IM. When CDS mails assigning to the specific message it is possible to take a decision for a separate SS, whether such information would be transmitted to them or would remain at the CDS level in the unsent messages folder (or messages sent to the default CDS mail). Notification will be generated automatically as part of the Gas IM aggregation process in the phase next to the successful completion of aggregation.

4.8.11.1 Response – 983 (RESPONSE) 

The response structure is specified in section 4.14.1 with the general formats. 

4.8.12 Instance trading results publishing notification
This is a communication script where the trade system transmits information to the rest of the neighboring systems on a specific transaction, in this case – instance trading results publishing. Notification will be sent in the form of RESPONSE message all SS, which have the right to trade on Gas IM. When CDS mails assigning to the specific message it is possible to take a decision for a separate SS, whether such information would be transmitted to them or would remain at the CDS level in the unsent messages folder (or messages sent to the default CDS mail). 
4.8.12.1 Response – 987 (RESPONSE) 

The response structure is specified in section 4.14.1 with the general formats. 

4.8.13 Gas IM order transcript general format (ISOTEDATA – GV3, GV6, GV9, GVE, GVK)

The meaning of items is entirely consistent with the meanings specified in section 4.8.1 and in the structure set out in section 5.6. Mandatory fields are marked with hatching. Other items are optional.

4.9 Query communication script upon Gas IM data instances (products)
4.9.1 Gas IM instance (product) items structure determination – ISOTEMASTERDATA

Data structure will consist of the following items:

	ISOTEMASTERDATA
	Meaning/Comment

	Message code
	Message code that identifies a message type.

	ISOTEMASTERDATA/Instance
	Meaning/Comment

	Instance
	Product (instance) short title.

	Commodity code
	Commodity is type of energy, which is traded on energy market. System support trading for commodities electricity (E) and gas (P).

	Long instance title
	Product (instance) description.

	Instance class
	Specifies the instance (product) supply period length of the delivery of the product (a week or a day). Currently only the D (Daily) value may be selected. 

	Block type  
	Specifies the instance (product) supply period  interval (B – Baseload, P – Peakload, O – Offpeakload).

	Instance location
	Physical supply location.

	Instance contract unit
	Contractual unit  (e.g., kWh, MWh).

	Instance currency unit
	Currency unit. This can have values in CZK and EUR (for future use).

	Settlement type
	Method of settlement of a completed trade (default PS – physical supply).

	Contract volume
	Volume of a single contract in terms of defined units. Technological limit is 0,1 – 999.

	Minimum supply volume
	Minimum supply volume is the product of the number of hours of the supply interval, number of days of the supply period and the minimum tradable unit (MWh).

	Initial delivery day
	The supply period initial day in the form of  YYYY-MM-DD.

	Final delivery day
	The supply period final day in the form of  YYYY-MM-DD.

	ISOTEMASTERDATA/Instance/Interval
	Meaning/Comment

	Order index
	The detail record order number.

	Supply interval
	The delivery day in the form of YYYY-MM-DD.

	Supply interval - initial period
	The initial trading hour index of the continuous interval of trading hours on the delivery day. It is a two-digit number, e.g. 01. The defined interval is 01 to 25 taking into account the number of hours of the day (default 24 hours, winter/summer time shift – 23; summer/winter time shift – 25).

	Supply interval – final period
	The final trading hour index of the continuous interval of trading hours on the delivery day. It is a two-digit number, e.g. 24. The defined interval is 01 to 25 taking into account the number of hours of the day (default 24 hours, winter/summer time shift – 23; summer/winter time shift – 25).

	Event title
	The time event title within the instance (product) life cycle:

· N_ISSUE – instance not opening notification,

· ISSUE - instance opening notification,

· TRC_START_MM – continual trading commencement  for the market maker,

· TRC_START_SS - continual trading commencement  for subjects of settlement,

· TRC_CLOSE - continual trading completion,

· AGGREG – data aggregation,

· PUBLICATION – data publishing

	Time of event
	The time mark of the event occurrence  in the form of YYYY-MM-DDThh:mm:ss.


4.9.2 Gas IM instance (product) data
The request will allow identifying the instance (product) data in the EMTAS module. One operation will process just one request to identify the instance (product) data, the resulting response may contain none, one or a set of instances.

4.9.2.1 Request– GVF (ISOTEREQ) 

The meaning of items is entirely consistent with the meanings specified in section 4.9.1 and in the structure set out in section 5.7. Mandatory fields are marked with hatching. Other items are optional.

	ISOTEREQ/Trade
	Meaning/Comment

	Product
	Mandatory field – note: using the asterisk character as a wildcard marker (e.g., DB0801*) it is possible to enquire for more instances, then the request would process all daily baseload instances (products) related to January 2008.


4.9.2.2 Response – GVG (RESPONSE)

The response structure is specified in section 4.14.1 with the general formats. 

4.9.2.3 Data transcript – GVH (ISOTEMASTERDATA)

The meaning of items is entirely consistent with the meanings specified in section 4.9.1 and in the structure set out in section 5.7. Mandatory fields are marked with hatching. Other items are optional.

The data transcript may generate several instances for a single request. This assumption is valid for the variant of the use of the asterisk character as a wildcard marker in the instance title.

4.10 Communication scripts for messages in ETSO format

This section describes the message scripts in ETSO format.

4.10.1 MCC for DM 

This message serves for the implementation of the actual profile length needed for the coordination of the day-ahead market, or as a transcript in the case of enquiry for a larger MCC. 

It is an ETSO ECAN Document (version 4.0). See below for the description of the individual items in the ETSO document.

	CapacityDocument
	Meaning/Comment

	DocumentIdentification
	Unique document identifier generated by the system source of the sender (SEPS/TSO), e.g. 20090501_A13_27XOTE-CZECHREPB

	DocumentVersion
	Document Version

	DocumentType
	Interconnection Capacity

	ProcessType
	Capacity Allocation

	SenderIdentification
.codingScheme
	EIC code of the sender (SEPS/TSO):10XSK-SEPS-GRIDB
ETSO coding scheme

	SenderRole
	System operator

	ReceiverIdentification
.codingScheme
	EIC code of the receiver. (OTE): 27XOTE-CZECHREPB
ETSO coding scheme

	ReceiverRole
	Transmission Capacity Allocator

	CreationDateTime
	Time stamp of the document creation. ISO 8601 UTC format.

	CapacityTimeInterval
	The time is in UTC ISO 8601 format. The period of the 1 day. DD corresponds to the Delivery Day-1. HH is 23 (winter time CET=GMT+1) or 22 (summer time CEST=GMT+2). In the case of transition to/from CEST/CET the period will be 23/25 hours, respectively. 

The time interval is possible solely in a range of 1 day. 

	Domain
	Domain

	CapacityTimeSeries
	Comment

	TimeSeriesIdentification
	Unique time series identifier generated by the system source of the sender (SEPS/TSO)

	BusinesType
	Offered Capacity

	Product
	ActivePower

	InArea
.codingScheme
	EIC code of the importing area. ČEPS/area: 10YCZ-CEPS-----N or SEPS/area: 10YSK-SEPS-----K
ETSO coding scheme

	OutArea
.codingScheme
	EIC code of the exporting area ČEPS/area: 10YCZ-CEPS-----N or SEPS/area: 10YSK-SEPS-----K
ETSO coding scheme

	MeasurementUnit
	Unit Mega Watt

	AuctionIdentification
	Not in use

	Period
	Comment

	TimeInterval
	Always the same value as the CapacityTimeInterval.

	Resolution
	Hourly interval

	Interval
	Comment

	Pos
	Sequence starting with a value of 1. There are as many intervals as many resolutions fit in the Time interval. Usually n=24, when transition to CEST n=23 and transition to CET n=25.

	Qty
	Energy quantity (absolute value) for each interval with accuracy of a whole number.


The listing of all values and the survey of the individual items on an xml document is presented in chapter 5.12.1 Mandatory values are marked by ciphering. All other items are not mandatory.

4.10.2 Request for MCC 

This message serves for status location of MCC size. It is an ETSO Status Request Document – ESR (version 1.1). See below for the description of the individual items in the ETSO document.

	StatusRequest
	Meaning/Comment

	MessageIdentification
	Unique document identifier generated by the system source of the sender, e.g.:

  20080905_A02_8591824010402_1 
  20080905_A13_11XSEBRATISLAVA4_1

	MessageType
	Message type that is the subject of enquiry 

	ProcessType
	Process type that is the subject of enquiry.

	SenderIdentification
.codingScheme
	EIC code of the sender (e.g. 11XSEBRATISLAVA4), or EAN code of the sender (e.g. 8591824010402)

	SenderRole
	Role of the sender

	ReceiverIdentification
.codingScheme
	Identification of OTE as the receiver of the document, either EAN or EIC.

	ReceiverRole
	Role of the Receiver

	MessageDateTime
	Time stamp of document creation. ISO 8601 UTC format.

	RequestedTimeInterval
	The time is in UTC ISO 8601 format. The period of the 1 day. DD corresponds to the Delivery Day-1. HH is 23 (winter time CET=GMT+1) or 22 (summer time CEST=GMT+2). In the case of transition to/from CEST/CET the period will be 23/25 hours, respectively. 

The time interval is possible solely in a range of 1 day.


The listing of all values and the survey of the individual items on an xml document is presented in chapter 5.12.6. Mandatory values are marked by ciphering. All other items are not mandatory.

4.10.3 RD implementation

This message serves for the submission of bilateral contracts through RD. It is an ETSO ESS Schedule Message (version 3.1). See below the description of the individual items in the ETSO document.

	ScheduleMessageHeader
	Meaning/Comment

	MessageIdentification
	Unique document identifier. In the case of automatic communication or submission through file upload it is the generated by the system source of the sender (participant, ČEPS or the energy exchange), when submitting through a form it is generated by the OTE system. Example: 20080905_A01_10XCZ-CEPS-GRIDE_1

	MessageVersion
	Document version

	MessageType
	Balance responsible schedule or Finalised schedule (only for external schedules registered by ČEPS)

	ProcessType
	Day-ahead, IntraDay or LongTerm

	ScheduleClassificationType
	Exchange type

	SenderIdentification
.codingScheme
	Identification of the sender of the diagram (participant, ČEPS or the energy exchange), EAN. ETSO coding scheme or EAN coding scheme

	SenderRole
	Trade responsible party (Participant) or System operator (ČEPS) or Market Operator (energy exchange)

	ReceiverIdentification
.codingScheme
	Identification of OTE as the receiver of the document,EAN.
ETSO coding scheme or EAN coding scheme

	ReceiverRole
	Imbalance settlement responsible

	MessageDateTime
	Time stamp of the document creation. ISO 8601 UTC format.

	ScheduleTimeInterval
	The time is in UTC ISO 8601 format. The period of the 1 day DD corresponds to the Delivery Day-1. HH is 23 (winter time CET=GMT+1) or 22 (summer time CEST=GMT+2). In the case of transition to/from CEST/CET the period will be 23/25 hours, respectively. 

The time interval is possible solely in a range of 1 day.

	Domain
	Domain

ETSO coding scheme

	SubjectParty
.codingScheme
	Identification of the market participant whose diagram is being sent. Usually it is the same as the identification of the sender. The identification might be different in the case of foreign diagrams submitted by ČEPS or domestic diagrams submitted by the energy exchange.
EAN coding scheme

	SubjectRole
	Trade responsible party. The role of the participant whose diagram is being sent.

	MatchingPeriod
	Matching period. Time is in UTC ISO 8601 format DD corresponds to delivery day-1. Final outer value HH is 23 (winter time CET=GMT+1) or 22 (summer time CEST=GMT+2). Matching period is: 

· In the case of day-ahead and long term transmissions (Process Type=A01, A12) equals to the time interval (ScheduleTimeInterval).
· In the case of Intraday transmissions (ProcessType=A02) only within the time interval (ScheduleTimeInterval), while shortening is possible only from the left.

	ScheduleTimeSeries
	Comment

	SendersTimeSeriesIdentification
	Unique time series identifier generated by the source system of the sender.

	SendersTimeSeriesVersion
	Time series Version (same as the version of the document)

	BusinesType
	Internal trade (for RD submitted by participants or the energy exchange) or External trade with non explicit capacity (for RD submitted by ČEPS). 

	Product
	ActivePower

	ObjectAgregation
	Party

	InArea
.codingScheme
	Area into which the product is delivered
ETSO coding scheme

	OutArea
.codingScheme
	Area from which the product is taken 
ETSO coding scheme

	MeteringPointIdentification
	Not in use

	InParty
.codingScheme
	Identification of the buying participant, EAN. 

EAN coding scheme

	OutParty
.codingScheme
	Identification of the selling participant, EAN.
EAN coding scheme

	CapacityContractType
	Not in use

	CapacityAgreementIdentification
	Not in use

	MeasurementUnit
	Unit  Mega Watt

	Period
	Comment

	TimeInterval
	Always the same value as the ScheduleTimeInterval.

	Resolution
	Hourly interval

	Interval
	Comment

	Pos
	Sequence with a starting value of 1. There are as many intervals as many resolutions fit into the Time Interval (TimeInterval). Usually it is n=24, when transition to CEST n=23, when transition to CET n=25. 

	Qty
	Amount of energy for each interval with an accuracy  of 3 decimal places (separation symbol for decimal places is '.').


The listing of all values and the survey of the individual items on an xml document is presented in chapter 5.12.3. Mandatory values are marked by ciphering. All other items are not mandatory.

4.10.4  RD enquiry

This message serves for RD status location. It is an ETSO Status Request Document – ESR (version 1.1). See below the description of the individual items in the ETSO document.

	StatusRequest
	Meaning/Comment

	MessageIdentification
	Unique document identifier generated by the system source of the sender, example: 

20080905_A02_8591824010402_1 

20080905_A13_11XSEBRATISLAVA4_1

	MessageType
	Message Type that is being enquired by the sender. A09 can be used for external schedules registered by ČEPS.

	ProcessType
	Process type that is being enquired by the sender.

	SenderIdentification
.codingScheme
	EAN code of the sender (e.g. 8591824010402)

	SenderRole
	Role of the sender

	ReceiverIdentification
.codingScheme
	Identification of OTE as the receiver of the document, EAN.

	ReceiverRole
	Role of the receiver

	MessageDateTime
	Time stamp of document creation. ISO 8601 UTC format.

	RequestedTimeInterval
	The time is in UTC ISO 8601 format. The period of the 1 day. DD corresponds to the Delivery Day-1. HH is 23 (winter time CET=GMT+1) or 22 (summer time CEST=GMT+2). In the case of transition to/from CEST/CET the period will be 23/25 hours, respectively. 

The time interval is possible solely in a range of 1 day.

	Items over the scope of ETSO standard
	 

	ReqSenderIdentification
	Identification of the sender of the requested RD. Usually the same as the ReqSubjectParty. They might be different in the case of domestic RDs submitted by the energy exchange. 
ETSO coding scheme or EAN coding scheme.
Mandatory in the case of the participant’s request for a domestic RD submitted by the energy exchange. 

	ReqSenderRole
	Role of the sender of the requested document. 

Obligation see ReqSender

	ReqSubjectParty
.codingScheme
	Identification of the market participant for which the requested document was submitted. Usually it is the same as the  identification of the sender. It might be different for requests submitted by ČEPS or the energy exchange for foreign diagrams submitted by ČEPS or for domestic diagrams submitted by the energy exchange. 

ETSO coding scheme or EAN coding scheme.
Mandatory for requests for RD data (Message Type=A01)when in the document  the time stamp of the Sender and SubjectParty (diagrams submitted by ČEPS and the energy exchange) and or the ReqMessageIdentification and ReqMessageVersionis not used. Otherwise it is not mandatory. 

	ReqSubjectRole
	Balance responsible party. Role of the participant for which the diagram is being sent. Obligations see ReqSubjectParty.

	ReqMatchingPeriod
	Matching period

Mandatory in the case of enquiries for a concrete document with the foreign party, intraday RD. If it is not stated then the lastly registered document with the foreign parties, intraday RD, is returned.

	ReqBusinesType
	Trade type (domestic/foreign), for which the requested time stamps (RD) were submitted. 

Mandatory for enquiry for RD data (MessageType=A01)

	ReqCounterparty
	Market participant identification, when he is already the counterparty of the owner of the diagram (in the required dokument he is specified as IN or OUT party). ETSO coding scheme or EAN coding schneme. Mandatory in the case of RD data enquiery requests (MessageType=A01), not submitted by ČEPS or the Energy Exchange or when the ReqMessageIdentification and ReqMessageVersion is not used. Otherwise not mandatory. 

	ReqMessageIdentification
	Unique document identifier of the requested RD.


Mandatory for RD data requests (MessageType=A01), if the ReqSubject, BusinessType or ReqSender is not used (ReqSender solely for participant’s enquiry for domestic RDs that were submitted by the energy exchange).

	ReqMessageVersion
	Document version of the requested RD. 

Obligations see ReqMessageIdentification


The listing of all values and the survey of the individual items on an xml document is presented in chapter 5.7.6 Mandatory values are marked by ciphering. All other items are not mandatory.

	Enquiry
	Sender/MessageType / ProcessType/ReqSender/ReqSubjectParty/BusinessType

	Enquiry of the participant for domestic RD submitted by this participant:
	ID-MP/A01/A01/n-a/n-a/A02
or
ID-MP/A01/A01/ID-MP/ID-MP/A02

	Enquiry of SS (ID-SS) for the domestic RD of the participant (ID-MP) who is taking the responsibility (default SS)
	ID-SS/A01/A01/n-a/ID-MP/A02
or 
ID-SS/A01/A01/ID-MP/ID-MP/A02

	Enquiry of the energy exchange (ID-EXCH) for internal RD of the participant submitted by the energy exchange:
	ID-EXCH/A01/A01/n-a/ID-MP/A02
or
ID-EXCH/A01/A01/ID-EXCH/ID-MP/A02

	Enquiry of the participant (ID-MP) for internal RD submitted by the energy exchange (ID-EXCH):
	ID-MP/A01/A01/ID-EXCH/ID-MP/A02

	Enquiry of ČEPS (ID-ČEPS ) for day-ahead foreign RD of the participant (ID-MP)


	ID-ČEPS/A01/A01/n-a/ID-MP/A06
or
ID-ČEPS/A01/A01/ID-ČEPS/ID-MP/A06

	Enquiry ČEPS (ID-ČEPS) for intraday foreign RD of the participant (ID-MP)


	ID-ČEPS/A01/A02/n-a/ID-MP/A06
or
ID-ČEPS/A01/A02/ID-ČEPS/ID-MP/A06

	Enquiry of the participant  (ID-MP) for day-ahead foreign RD submitted by ČEPS (ID-ČEPS):
	ID-MP /A01/A01/n-a/ID-MP/A06/n-a
or 
ID-MP /A01/A01/ID-ČEPS/ID-MP/A06/n-a

	Enquiry of the participant  (ID-MP) for intraday foreign RD submitted by ČEPS (ID-ČEPS):
	ID-MP /A01/A02/n-a/ID-MP/A06/<period>
or

ID-MP/A01/A02/ID-ČEPS/ID-MP/A06/<period>


Results of the implicit auction on the DM

This message serves for sending the results of the implicit auction to both of the TSOs (SEPS/TSO, ČEPS/TSO). It is an ETSO ECAN Implicit Auction Result Document (version 4.0). See below the description of the individual items in the ETSO document:

	ImplicitAuctionResultDocument
	Meaning/Comment

	DocumentIdentification
	Unique document identifier generated by the system source of the sender (ČEPS or SEPS), example: 20080905_A25_10XSK-SEPS-GRIDB

	DocumentVersion
	Document version

	DocumentType
	Allocation result document

	SenderIdentification
.codingScheme
	EIC code of the market operator in the position of a primary coordinator on the common DM. 

OTE/OT: 27XOTE-CZECHREPB; SEPS/OT: 24X-OT-SK------V
ETSO coding scheme

	SenderRole
	Transmission capacity allocator

	ReceiverIdentification
.codingScheme
	EIC code TSO. ČEPS/TSO: 10XCZ-CEPS-GRIDE; SEPS/TSO: 10XSK-SEPS-GRIDB
ETSO coding scheme

	ReceiverRole
	System operator

	CreationDateTime
	Time stamp of document creation ISO 8601 UTC format.

	PublicationTimeInterval
	The time is in UTC ISO 8601 format. The period of the 1 day DD corresponds to the Delivery Day-1. HH is 23 (winter time CET=GMT+1) or 22 (summer time CEST=GMT+2). In the case of transition to/from CEST/CET the period will be 23/25 hours, respectively. 

The time interval is possible solely in a range of 1 day.

	Domain
	Domain

	ResultTimeSeries
	Comment

	TimeSeriesIdentification
	Unique time series identifier generated by the system source of the sender (ČEPS or SEPS)

	AllocationIdentification
	Not in use

	AllocationType
	Implicit

	BusinesType
	Market capacity price

	InArea
.codingScheme
	EIC code of the import area ČEPS/Area: 10YCZ-CEPS-----N or SEPS/Area: 10YSK-SEPS-----K
ETSO coding scheme

	OutArea
.codingScheme
	EIC code of the export area. ČEPS/Area: 10YCZ-CEPS-----N or SEPS/Area: 10YSK-SEPS-----K
ETSO coding scheme

	ContractType
	Daily

	MeasureUnitQuantity
	Unit Mega Watt

	Currency
	Currency

	MeasureUnitPrice
	Unit €/Mega Watt 

	Period
	Comment

	TimeInterval
	Always the same value as the PublicationTimeInterval.

	Resolution
	Hourly Interval

	Interval
	Comment

	Pos
	Sequence starting with a value 1. As many Intervals exist as many resolutions fit in the Time Interval (TimeInterval). Usually it is n=24, if transition to CEST n=23, if transition to CET n=25.

	Qty
	Amount of energy for each interval with an accuracy of 1 decimal place (decimal place separator is '.') 

	Price
	The price in the importing area in EUR with an accuracy of 2 decimal places (decimal place separator is '.')


The listing of all values and the survey of the individual items on an xml document is presented in chapter 5.12.2. Mandatory values are marked by ciphering. All other items are not mandatory.

4.10.5 Cross-border exchanges

This message serves for sending a report on day-ahead diagrams of cross-border exchanges that arose on the DM  ČEPS/TSO and SEPS/TSO. It is an ETSO ESS Schedule Message (version 3.1). See below the description of the individual items in the ETSO document. 

	
	ScheduleMessageHeader
	Meaning/Comment

	
	MessageIdentification
	Unique document identifier generated by the system source of the sender (ČEPS or SEPS), example: 20080905_A02_10XSK-SEPS-GRIDB

	
	MessageVersion
	Document version

	
	MessageType
	Allocated capacity schedule

	
	ProcessType
	Day ahead

	
	ScheduleClassificationType
	Exchange type

	
	SenderIdentification
.codingScheme
	EIC code of the market operator in the position of a primary coordinator of the comment DM.  OTE/OT: 27XOTE-CZECHREPB; SEPS/OT: 24X-OT-SK------V
ETSO coding scheme

	
	SenderRole
	Transmission capacity allocator

	
	ReceiverIdentification
.codingScheme
	EIC code TSO. ČEPS/TSO: 10XCZ-CEPS-GRIDE; SEPS/TSO: 10XSK-SEPS-GRIDB 
ETSO coding scheme

	
	ReceiverRole
	System operator

	
	MessageDateTime
	Time stamp of document creation ISO 8601 UTC format.

	
	ScheduleTimeInterval
	The time is in UTC ISO 8601 format. The period of the 1 day. DD corresponds to the Delivery Day-1. HH is 23 (winter time CET=GMT+1) or 22 (summer time CEST=GMT+2). In the case of transition to/from CEST/CET the period will be 23/25 hours, respectively. 

The time interval is possible solely in a range of 1 day.

	
	Domain
	Domain

	
	SubjectParty
.codingScheme
	EIC code of the market operator of the common DM for whom the diagram is being sent. OTE/OT: 27XOTE-CZECHREPB; SEPS/OT: 24X-OT-SK------V 
ETSO coding scheme

	
	SubjectRole
	This element is important so that it would be distinguishable that the primary coordinator is sending the foreign scheduling in the place of the secondary coordinator. The primary coordinator is in a role A07 (Transmission capacity allocator) the secondary coordinator in a role A11 (Market Operator), since he does not perform self allocation. 

	
	MatchingPeriod
	Not in use

	
	ScheduleTimeSeries
	Comment

	
	SendersTimeSeriesIdentification
	Unique time series identifier generated by the system source of the sender (ČEPS or SEPS)

	
	SendersTimeSeriesVersion
	Version of the time series (same as the document version)

	
	BusinesType
	External trade with non explicit capacity

	
	Product
	ActivePower

	
	ObjectAgregation
	Party

	
	InArea
.codingScheme
	EIC code of the importing area ČEPS/Area: 10YCZ-CEPS-----N or SEPS/Area: 10YSK-SEPS-----K
ETSO coding scheme

	
	OutArea
.codingScheme
	EIC code of the export area ČEPS/Area: 10YCZ-CEPS-----N or SEPS/Area: 10YSK-SEPS-----K
ETSO coding scheme

	
	MeteringPointIdentification
	Not in use

	
	InParty
.codingScheme
	EIC code of the market operator of the importing area: OTE/OT: 27XOTE-CZECHREPB or SEPS/OT: 24X-OT-SK------V
ETSO coding scheme

	
	OutParty
.codingScheme
	EIC code of the market operator of the export area. OTE/OT: 27XOTE-CZECHREPB or SEPS/OT: 24X-OT-SK------V
ETSO coding scheme

	
	CapacityContractType
	Daily

	
	CapacityAgreementIdentification
	Contract Identification – Constant value

	
	MeasurementUnit
	Unit Mega Watt

	
	Period
	Comment

	
	TimeInterval
	Always the same value as at the ScheduleTimeInterval.

	
	Resolution
	Hourly Interval

	
	Interval
	Comment

	
	Pos
	Sequence starting with a value 1. As many Intervals exist as many resolutions fit in the Time Interval (TimeInterval). Usually it is n=24, if transition to CEST n=23, if transition to CET n=25. 

	
	Qty
	Amount of energy for each interval with an accuracy of 1 decimal place (decimal place separator is '.') At least for one direction there must be a zero value for a respective hour.


The listing of all values and the survey of the individual items on an xml document is presented in chapter 5.12.3. Mandatory values are marked by ciphering. All other items are not mandatory.

4.10.6 Message on the results of RD processing

This message serves for informing the sender about the result of processing of the given ETSO document. It is an ETSO Acknowledgement Document - EAD (version 5.0). See below the description of the individual items in the ETSO document. 

	AcknowledgementDocument
	Meaning/Comment

	Documentdentification
	Unique document identifier generated by the system source of the receiver, example: 

20090501_A13_27XOTE-CZECHREPB_1

	DocumentDateTime
	Time stamp of document creation. ISO 8601 UTC format.

	SenderIdentification
.codingScheme
	Identification of OTE as the sender of the document, either EAN or EIC. ETSO coding scheme or EAN coding scheme

	SenderRole
	Imbalance settlement responsible

	ReceiverIdentification
.codingScheme
	Identification of the receiver of the document (ČEPS or energy exchange), either EAN or EIC.
ETSO coding scheme or EAN coding scheme

	ReceiverRole
	Transmission capacity allocator (ČEPS) or Balance responsible party (Participant) or Market Operator (energy exchange)

	ReceivingDocumentIdentification
	Unique document identifier, which was received. Not filled in if the document was not received successfully. .  

	ReceivingDocumentVersion
	Document version that was received.

	ReceivingDocumentType
	Document type that was received (acc. to ETSO standards)

	ReceivingPayloadName
	Not in use

	DateTimeReceivingDocument
	Time stamp of the receipt of the document ISO 8601 UTC format.

	  Reason
	Comment 

	ReasonCode
	Reason codes (acc. to ETSO standards) identify the errors on the level of the header of the document. 

	ReasonText
	Specifies the  error description.

	TimeSeriesRejection
	Comment

	SendersTimeSeriesIdentification
	Unique time series identifier in the document that has been received from the sender (only in that case if the error is in the time series, otherwise it is not sent).  

	SendersTimeSeriesVersion
	Version of the time series in the document, which was received (only if it was stated in the received document). 

	  Reason
	Comment

	ReasonCode
	Reason codes (acc. to ETSO standards) indentifying the errors on the level of the header of the time series. 

	ReasonText
	Specifies the error description.

	TimeIntervalError
	Comment

	QuantityTimeInterval
	Time interval in which the error was found. 

The time is in UTC ISO 8601 format. The period of the 1 day. DD corresponds to the Delivery Day-1. HH is 23 (winter time CET=GMT+1) or 22 (summer time CEST=GMT+2). In the case of transition to/from CEST/CET the period will be 23/25 hours, respectively. 

The time interval is possible solely in a range of 1 day.

	  Reason
	Comment

	ReasonCode
	Reason codes (acc. to ETSO standards) identifying the error on the interval level.

	ReasonText
	Specifies the  error description.


The listing of all values and the survey of the individual items on an xml document is presented in chapter 5.12.7. Mandatory values are marked by ciphering. All other items are not mandatory.

Reason codes and their specifying description for each type of message generated by the CS OTE system in the EAD document:

	Message type
	ReasonCode (element)
	ReasonText (element)


	Comment

	MCC for DM
	A01 

(AcknowledgementDocument)
	
	Document received

	
	A69 

(AcknowledgementDocument)
	Name of the mandatory item
	Any mandatory item missing

	
	A51

(AcknowledgementDocument)
	
	- DocumentIdentification not in a format <BusinessDay in format YYYYMMDD>_<DocumentType>_<ReceiverEIC>,

- there is a document already registered with the same ID and the same or lower document version

- there is a document already registered with a same ID and at least with one different item: delivery day (CapacityTimeInterval), processing type (ProcessType)

	
	A52

(AcknowledgementDocument)
	
	New document does not contain any time series

	
	A94

(AcknowledgementDocument)
	DocumentType invalid
	DocumentType is not the required constant

	
	
	CreationDateTime invalid
	CreationDateTime not in a valid format

	
	A79

(AcknowledgementDocument)
	
	ProcessType is not the required constant

	
	A78

(AcknowledgementDocument)
	
	- SenderIdentification.codingScheme is not the required constant - ReceiverIdentification.codingScheme is not the required constant 

- SenderRole is not the required constant

- ReceiverRole is not the required constant,

- Invalid SenderIdentification,

- Invalid ReceiverIdentification

	
	A80

(AcknowledgementDocument)
	
	Domain, or Domain.codingScheme is not the required constant

	
	A02

(AcknowledgementDocument)

A62

(TimeSeriesRejection)
	
	BusinesType is not the required constant

	
	A02

(AcknowledgementDocument)

A94

(TimeSeriesRejection)
	Product invalid

(TimeSeriesRejection)
	BusinesType is not the required constant

	
	A03

(AcknowledgementDocument)

A94

(TimeSeriesRejection)
	MeasurementUnit invalid (TimeSeriesRejection)
	MeasurementUnit is not the required constant

	
	A02

(AcknowledgementDocument)

A41

(TimeSeriesRejection)
	
	Resolution is not the required constant

	
	A02

(AcknowledgementDocument)

A09

(TimeSeriesRejection)
	
	There is an already registered document with the same ID and a different time series identification 

	
	A02

(AcknowledgementDocument)

A55

(TimeSeriesRejection)
	
	The new document contains the same time series ID 

	
	A02

(AcknowledgementDocument)

A20

(TimeSeriesRejection)
	More then 2 TimeSeries in a document (TimeSeriesRejection)
	The new document contains more than 2 time series

	
	A04

(AcknowledgementDocument)
	More then 2 TimeSeries in a document (TimeSeriesRejection)
	Time interval of the time series (TimeInterval) is not the same as the time interval in the header of the document (CapacityTimeInterval)

	
	A03

(AcknowledgementDocument)

A21

(TimeSeriesRejection)

A49

(TimeIntervalError)
	Too many positions, positions out of interval have been ignored. (TimeIntervalError)
	The time series contains more hours than the calendar day, the hours outside of the interval were ignored. The document was received.

	
	A03

(AcknowledgementDocument)

A21

(TimeSeriesRejection)

A49

(TimeIntervalError)
	Missing positions, quantities have been zeroed out in missed positions (TimeIntervalError)
	The time series contains fewer hours than the calendar day, the remaining hours were degenerated with a zero amount. The document was received.

	
	A02

(AcknowledgementDocument)

A21

(TimeSeriesRejection)

A42

(TimeIntervalError)
	Quantity must be a whole number. (TimeIntervalError)
	The amount is not a whole positive number, incl. zero.

	
	A02

(AcknowledgementDocument)

A57

(TimeSeriesRejection)
	
	MCC submitted for an already closed DM session.

	
	A59

(AcknowledgementDocument)
	
	The submitter of the message is not SEPS/TSO.

	
	999

(AcknowledgementDocument)
	Description of ORA error.


	System error in CS OTE.

	Enquiry for MCC
	A04

(AcknowledgementDocument)
	
	The requested time interval must be((RequestedTimeInterval)) always for one trading day. 

	
	A69 

(AcknowledgementDocument)
	Name of the mandatory item
	Any mandatory item is missing

	
	A51

(AcknowledgementDocument)
	
	- MessageIdentification is not in a format <BusinessDay in format YYYYMMDD>_<A13>_<SenderEIC>,

- there is a document already registered with the same ID and the same or lower document version

- there is a document already registered with a same ID and at least with one different item: delivery day (CapacityTimeInterval), processing type (ProcessType)

	
	A94

(AcknowledgementDocument)
	MessageType invalid (AcknowledgementDocument)
	MessageType is not of a value ‚A13‘

	
	A94

(AcknowledgementDocument)
	ReceiverIdentification.codingScheme invalid 

(AcknowledgementDocument)
	ReceiverIdentification.codingScheme is not the required constant

	
	A94

(AcknowledgementDocument)
	MessageDateTime invalid 

(AcknowledgementDocument)
	MessageDateTime is not in a valid format

	
	A94

(AcknowledgementDocument)
	
	

	
	A79

(AcknowledgementDocument)
	
	ProcessType is not the value ‚A07‘

	
	A78

(AcknowledgementDocument)
	
	- SenderIdentification.codingScheme is not the required constant 

- SenderRole is not the required constant, (A07,A08,A11)

- Invalid SenderIdentification,

- Invalid ReceiverIdentification

	
	A94

(AcknowledgementDocument)
	No ATC, delivery day not yet  open for trading 

(AcknowledgementDocument)
	Enquiry for  MCC value of an unopened session on DM.

	
	999

(AcknowledgementDocument)
	Description of ORA error.


	System error in CS OTE.


4.10.7 Message on RD discrepancies

This message informs the sender about discrepancies while processing the given ETSO document. It is an ETSO ESS Anomaly Report (version 3.1). See below the description of the individual items in the ETSO document. 

	AnomalyReport
	Meaning/Comment

	MessageIdentification
	Unique document identifier generated by the system source of OTE. Example: 20090501_8591824010402_1

	MessageDateTime
	Time stamp of document creation. ISO 8601 UTC format.

	SenderIdentification
.codingScheme
	OTE identification as the sender of the document either EAN or EIC (EIC is preferred).
ETSO coding scheme or EAN coding scheme

	SenderRole
	Imbalance settlement responsible

	ReceiverIdentification
.codingScheme
	Identification of the receiver of the document (participant, ČEPS, or energy exchange) , either  EAN or EIC
ETSO coding scheme or EAN coding scheme

	ReceiverRole
	Trade responsible party (Participant) or System operator (ČEPS) or Market Operator (energy exchange)

	ScheduleTimeInterval
	The time is in UTC ISO 8601 format. The period of the 1 day DD corresponds to the Delivery Day-1. HH is 23 (winter time CET=GMT+1) or 22 (summer time CEST=GMT+2). In the case of transition to/from CEST/CET the period will be 23/25 hours, respectively. 

The time interval is possible solely in a range of 1 day.

	  Reason
	Comment

	ReasonCode
	Reason Code (acc. to ETSO standard).

	ReasonText
	Anomaly description, does not have to be stated.

	TimeSeriesAnomaly
	Comment

	MessageSenderIdentification
.codingScheme
	Identification of the producer/consumer in the document, where the discrepancy was found (participant, ČEPS, or energy exchange), EAN.

EAN coding scheme

	SendersMessageIdentification
	Unique identifier of the received document in which a discrepancy was found.

	SendersMessageVersion
	Version of the received document in which a discrepancy was found.. 

	SendersTimeSeriesIdentification
	Unique time series identifier in which a discrepancy was found. 

	SendersTimeSeriesVersion
	Time series version (same as the document version)

	BusinesType
	Internal trade (for RD submitted by participants or the energy exchange) or External trade with non explicit capacity (for RD submitted by ČEPS). 

	Product
	ActivePower

	ObjectAgregation
	Party

	InArea
.codingScheme
	Area into which the product is delivered.
ETSO coding scheme

	OutArea
.codingScheme
	Area from which the product is withdrawn.
ETSO coding scheme

	MeteringPointIdentification
	Not in use

	InParty
.codingScheme
	Identification of the buying participant, EAN.
EAN coding scheme

	OutParty
.codingScheme
	Identification of the Keller participant, EAN.
EAN coding scheme

	CapacityContractType
	Not in use

	CapacityAgreementIdentification
	Not in use

	MeasurementUnit
	Unit Mega Watt

	Period
	Comment

	TimeInterval
	Always the same value as the Schedule TimeInterval.

	Resolution
	Hourly Interval

	Interval
	Comment

	Pos
	Sequence starting with a value 1. As many Intervals exist as many resolutions fit in the Time Interval (TimeInterval). Usually it is n=24, if transition to CEST n=23, if transition to CET n=25.

	Qty
	Amount of energy for each interval with an accuracy of 1 decimal place (decimal place separator is '.') At least for one direction there must be a zero value for a respective hour.


The listing of all values and the survey of the individual items on an xml document is presented in chapter 5.12.4. Mandatory values are marked by ciphering. All other items are not mandatory.

4.10.8 Message confirming the received RD values 

This message informs the sender about the confirmed values while processing the given ETSO document. It is and ETSO ESS Confirmation Report (version 3.1) See below the description of the individual items in the ETSO document. 

	ConfirmationReport
	Meaning/Comment

	MessageIdentification
	Unique document identifier generated by the system source of the receiver, example: 

20090501_A03_27XOTE-CZECHREPB_1

	MessageType
	Message type document that was received from the sender (acc. to ETSO standard). 

	MessageDateTime
	Time stamp of the document creation ISO 8601 UTC format.

	SenderIdentification
.codingScheme
	Identification of OTE as the sender of the document, EAN. 

EAN coding scheme

	SenderRole
	Imbalance settlement responsible

	ReceiverIdentification
.codingScheme
	Identification of the receiver of the document (participant, ČEPS, or Energy Exchange) , EAN.

EAN coding scheme

	ReceiverRole
	Trade responsible party (Participant) or System operator (ČEPS) or Market Operator (Energy Exchange)

	ScheduleTimeInterval
	The time is in UTC ISO 8601 format. The period of the 1 day. DD corresponds to the Delivery Day-1. HH is 23 (winter time CET=GMT+1) or 22 (summer time CEST=GMT+2). In the case of transition to/from CEST/CET the period will be 23/25 hours, respectively. 

The time interval is possible solely in a range of 1 day.

	ConfirmedMessageIdentification
	Unique document identifier that has been received from the sender.

	ConfirmedMessageVersion
	Document version, received from the sender.

	Domain
.codingScheme
	Domain
ETSO coding scheme 

	SubjectParty
.codingScheme
	Identification of the receiver of the document (participant, ČEPS, or Energy Exchange) , EAN.

EAN coding scheme

	SubjectRole
	Trade responsible party (Participant) or System operator (ČEPS) or Market Operator (Energy Exchange)

	ProcessType
	Process type of the document that was received from the sender. (acc. to ETSO standards)

	  Reason
	Comment

	ReasonCode
	

	ReasonText
	

	TimeSeriesConfirmation
	Comment 

	SendersTimeSeriesIdentification
	Unique time series identifier generated by the system source of the sender (ČEPS or SEPS) 

	SendersTimeSeriesVersion
	Time series version (same as the document version)

	BusinesType
	Internal trade (for RD submitted by participants or the energy exchange) or External trade with non explicit capacity (for RD submitted by ČEPS). 

	Product
	ActivePower

	ObjectAgregation
	Party

	InArea
.codingScheme
	Area into which the product is delivered. 

ETSO coding scheme

	OutArea
.codingScheme
	Area from which the product is withdrawn.
ETSO coding scheme

	MeteringPointIdentification
	Not in use

	InParty
.codingScheme
	Identification of the selling participant, EAN. 
EAN coding scheme

	OutParty
.codingScheme
	Identification of the buying participant, EAN. 
EAN coding scheme

	CapacityContractType
	Not in use

	CapacityAgreementIdentification
	Not in use

	MeasurementUnit
	Unit Mega Watt

	Period
	Comment

	TimeInterval
	Always the same as the value in the ScheduleTimeInterval.

	Resolution
	Hourly interval

	Interval
	Comment

	Pos
	Sequence starting with a value 1. As many Intervals exist as many resolutions fit in the Time Interval (TimeInterval). Usually it is n=24, if transition to CEST n=23, if transition to CET n=25.

	Qty
	Amount of energy for each interval with an accuracy of 3 decimal place (decimal place separator is '.') 


The listing of all values and the survey of the individual items on an xml document is presented in chapter 5.12.5. Mandatory values are marked by ciphering. All other items are not mandatory.

4.10.9 Notification about change (shift) of gate closure time – 981 (RESPONSE) 

Notification about change of gate closure time in RRD session (time) – type of digram, session start time, sesión deadline, sesión report)
Type of  diagrams : 

· DDD –day-ahead domestic diagram

· DDDo - day-ahead domestic diagram corrective, 

· ZDD –day-ahead foreign diagram

· ZDV – intraday diagram

Structure of response is presented in chapter 4.1.1 and Summary of notification structure – RESPONSE in chapter 5.11.1
4.11 Settlement and aggregation communication scripts

Single items of this section are defined in the maximum classification, which means that some items may be accumulated in a common format of the data into one item (e.g., items of a date type), or may not be used at all.
4.11.1 Settlement result items structure determination – ISOTEDATA

The sentence structure will consist of the following items:

	ISTOTEDATA
	Meaning/Comment

	Message code
	Message code identifying the message type.

	Participant (EAN)/anonymous participant/EIC code
	Unique participant identification within IS OTE (EAN). Anonymous participant code, or EIC according to anonymity settings.

	ISOTEDATA/Trade
	Meaning/Comment

	Date/Delivery day
	Delivery day or starting validity date in the form of YYYY-MM-DD.

	Bid type
	Identifies whether it is a sell (P) or a buy (N) bid. It is used only for messages (reports) 939 and 973.

	Matching ID
	A unique matching identifier within a specific day.

	LP change date
	LP period change date; it is determining the values of energy splitting for specific periods of clearing prices validity in the form of YYYY-MM-DD. This item is used only for the Settlement version 6 (Clearing LP), otherwise the field is empty.

	Bid matching attribute
	The attribute that indicates whether a bid was matched (A) or not (N).

	Message code
	Notification or error message description specification at the level of a trading day  (RC001 - the bid was removed by reason of complex indivisibility conditions; RC002 - the bid was not matched by reason of optimizing the matching result (application of optimization criteria for maximizing the volume traded); RC006 - Marginal values determining has not taken place within any matching period. All sell bids were removed  by reason of complex indivisibility conditions).

	Message text
	Reason code specification. The item (field) is optional.

	Bid ID
	Bid Identification code (ID) used within EMTAS. Along with the bid version it is a unique bid identifier in the CS OTE system.

	Settlement version/Bid version
	Settlement version identification (1 - Daily DM Settlement, 2 - Daily Imbalance Settlement, 3 - Interim Monthly Settlement, 4 - Final Monthly Settlement, 5 – State of Emergency, 6 – Clearing LP) / Bid version within EMTAS. Along with the Bid ID it is a unique bid identifier in the CS OTE system.

	Market type/Area
	Market identification (OKO – Day-ahead market, DVS – Registration of RD, VDT – Intraday market, BT – Block market) / Area identification, where the bid was entered (CZ, SK).

	ISOTEDATA/Trade/ProfileData
	Meaning/Comment

	Hour
	Identification of the trading hour within which the required action will be performed. The defined interval is 1 to 25, depending on the number of hours of a trading day. (winter/summer time shift – 23; summer/winter time shift – 25). Detailed records for each item must be clear and must be sorted in ascending order.
For daily settlement the item has always the value „0“.

	Volume /Matched volume
	Volume /Matched volume is determined for a specified trading hour. Volume is specified in tenth of MWh. 

	Price
	Total price. Price is defined in CZK or EUR with accuracy to 2 decimal positions.

	Currency code
	Currency specification (CZK, EUR).

	Message code
	Notification or error message description specification at the level of a trading day hour (e.g. about marginal values missing by reason of buy or sell bids absence).

	Message text
	Notification or error message description specification at the level of a trading day hour. The field would be filled up in the case that it would be necessary to specify a notification or an error message, defined by the code.

	System price
	Marginal price resulted from a matching of bids in both areas within a specified hour. If during that hour the demand did not exceed the capacity profile (demand excess), items of "Price CZ", "Price SK" and "System price" will have equal value. In case there occurred such a demand excess, values of those items may be different from each other.

	System volume 
	Marginal volume resulted from a matching of both areas within a specified hour. If during that hour the demand did not exceed the capacity profile (demand excess), the items "Total volume " and "System volume" will have equal value. In case there occurred such a demand excess, values of those items may be different from each other.

	Price CZ
	The marginal price of matched bids in the CZ within a specified hour (EUR). 

	Volume CZ - sell
	Total volume of matched sell bids in the CZ within a specified hour (MWh).

	Volume CZ - buy
	Total volume of matched buy bids in the CZ within a specified hour (MWh).

	Flow CZ => SK
	Energy flow from the CZ area to the SK area (export from the CZ). Settled as a difference between the CZ sell volume and the CZ buy volume within a specified hour. The item is specified only if the resulting value is positive or zero. Energy flow is 
specified as its absolute value.

	Period matching attribute
	The attribute of a total/all (A) or a partial (P) matching of the offered / demanded volume or of a not matched bid (N) within a specified hour.

	Requested flow CZ => SK
	Requested energy flow from the CZ area to the SK area (export from the CZ). In case that  the demand did not exceed the capacity profile (demand excess) in the appropriate direction, the item value is equal to the value of the resulting flow field (the value „Flow CZ => SK“). In case that  the demand exceeded the available capacity profile in the appropriate direction, the item value would exceed the value of the resulting flow and also higher than the available capacity profile in the appropriate direction.

	Requested flow SK => CZ
	Energy flow from the SK area to the CZ area (export from the SK). In case that  the demand did not exceed the capacity profile (demand excess) in the appropriate direction, the item value is equal to the value of the resulting flow field (the item „Flow SK => CZ“).In case that  the demand exceeded the available capacity profile in the appropriate direction, , the item value would exceed the value of the resulting flow and also higher than the available capacity profile in the appropriate direction.

	Price SK
	Marginal price of matched bids in the SK within a specified hour (EUR).

	Volume SK - sell
	Total volume of matched sell bids in the SK within a specified hour (MWh).

	Volume SK - buy
	Total volume of matched buy bids in the SK within a specified hour (MWh).

	Flow SK => CZ
	Energy flow from the SK area to the CZ area (import into the CZ). Settled as a difference between the CZ sell volume and the CZ buy volume within a specified hour. The item is specified  only if the resulting value is negative or zero. Energy flow is 
specified as its absolute value.

	Profile identification
	Detailed information on the identification of profiles is specified in section 5.13 Allocation of profiles to IS OTE data.


4.11.2 Data request - Final plan

The request will allow determining the traded volume plan for a specific trading day divided up according to individual markets. One operation will contain just one request to identify the final plan, which results may contain more than one record.

As a result, we receive final plan data (summary) divided up according to the target markets (ERD, OKO, BT, VDT), which mean the ERD data as a result of the RD aggregation procedure, OKO data as a result of Day-ahead market bids matching, BT data as a result of the block market aggregation procedure and VDT market data, which were generated as a result of intraday market closed trades including those related to open trading hours.

4.11.2.1 Request – 941 (ISOTEREQ) 

The data sentence structure expected in the EMTAS module. 

The meaning of items is entirely consistent with the meanings specified in section 4.11.1 and in the structure set out in section 5.5. Mandatory fields are marked with hatching. Other items are optional. 

The query may request a final data plan for a specific day:

	ISOTEREQ/Trade
	Meaning/Comment

	Date
	Mandatory field

	Market type
	Optional field – If the item is specified, only data related to a specific market will be selected (DVS, OKO, VDT, BT); if not specified, all markets will be taken into consideration.


4.11.2.2 Response – 942 (RESPONSE) 

The response structure is specified in section 4.14.1 with the general formats. 

4.11.2.3 Data transcript – 943 (ISOTEDATA) 

The data transcript structure is specified in section 4.11.11 with the general formats. Data transcript is created only if the request comes from the CDS. If the request comes from the EMTAS, then data transcript will be not created
The data transcript may generate several records for a single request.
If there is no value specified for any trading hour and profile (see more information in section 5.13 Allocation of profiles to IS OTE data, clause “Final plan”), that means that that hour will be not an element of data transcript.
Note. In the response to the query (request) the specified volume is always with a positive sign. Price is sign inclusive: positive price = SS claim to OTE, negative price = SS commitment to OTE. Price means a total price for that volume. See more information in section 5.13 Allocation of profiles to IS OTE data, clause “Final plan”.
4.11.3 Data request – DM Marginal prices 

The request will allow determining marginal prices achieved on a specific trading day market. One operation will contain just one request to determine the marginal prices related to a specific trading day, with a response containing one record or none.
4.11.3.1 Request – 944 (ISOTEREQ) 

The data sentence structure expected in the EMTAS module. 

The meaning of items is entirely consistent with the meanings specified in section 4.11.1 and in the structure set out in section 5.5. Mandatory fields are marked with hatching. Other items are optional. 

The query may request DM marginal prices for a specific day:

	ISOTEDATA/Trade
	Meaning/Comment

	Date
	Mandatory field


4.11.3.2 Response – 945 (RESPONSE) 

The response structure is specified in section 4.14.1 with the general formats.  

4.11.3.3 Data transcript – 946 (ISOTEDATA) 

The data transcript structure is specified in section 4.11.11 with the general formats. Data transcript is created only if the request comes from the CDS. If the request comes from the EMTAS, then data transcript will be not created.

Only one data transcript may be generated for one request.  

In the case that there exist no value for any trading hour or a profile (see more information in section 5.13 Allocation of profiles to IS OTE data, clause „DM marginal prices“), it means that this hour is not a part of the data transcript.

Note: In the response to the request there is always a positive price (see more information in section 5.13 Allocation of profiles to IS OTE data, clause „DM marginal prices“).

4.11.4 Data request – Hourly settlement

The request will allow determining an hourly settlement results specification achieved within a specific trading day and a settlement version divided up according to separate clearing concepts. One operation will contain just one request to determine settlement data, which result may contain more than one record.
4.11.4.1 Request – 951 (ISOTEREQ) 

The data sentence structure expected in the EMTAS module. 

The meaning of items is entirely consistent with the meanings specified in section 4.11.1 and in the structure set out in section 5.5. Mandatory fields are marked with hatching. Other items are optional. 

The query may request DM marginal prices for a settlement result, specific trading and a settlement version:

	ISOTEDATA/Trade
	Meaning/Comment

	Date
	Mandatory field


4.11.4.2 Response – 952 (RESPONSE) 

The response structure is specified in section 4.14.1 with the general formats. 

4.11.4.3 Data transcript – 953 (ISOTEDATA) 

The data transcript structure is specified in section 4.11.11 with the general formats. Data transcript is created only if the request comes from the CDS. If the request comes from the EMTAS, then data transcript will be not created.

More than one data transcript records may be generated for one request.  

In the case that there exist no value for any trading hour or a profile (see more information in section 5.13 Allocation of profiles to IS OTE data, clause „Settlement – Hourly data“), it means that this hour is not a part of the data transcript.

Note. In the response to the query (request) price in all clearing concepts is specified including the sign: positive price = SS claim to OTE, negative price = SS commitment to OTE. Price means a total price for that volume.
Volume is always defined as a positive value. Please, find identification of a buy or sell in „Profile ID“ see section 5.13 Allocation of profiles to IS OTE data, clause „Settlement – Hourly data“.

In clearing concepts like EC, FMD, IMF volume is specified as its absolute value for buy and sell.

In clearing concepts AF, EI, IFF, OF volume value is zero.

4.11.5 Data request – Daily settlement

The request will allow determining settlement daily results specification within a specific trading day and a settlement version divided up according to separate clearing concepts. One operation will contain just one request to determine settlement data, which result may contain more than one record.
4.11.5.1 Request – 961 (ISOTEREQ) 

The data sentence structure expected in the EMTAS module. 

The meaning of items is entirely consistent with the meanings specified in section 4.11.1 and in the structure set out in section 5.5. Mandatory fields are marked with hatching. Other items are optional. 

The query may request settlement results of a specific trading day and a settlement version:

	ISOTEREQ/Trade
	Meaning/Comment

	Date
	Mandatory field


4.11.5.2 Response – 962 (RESPONSE) 

The response structure is specified in section 4.14.1 with the general formats. 

4.11.5.3 Data transcript – 963 (ISOTEDATA) 

The data transcript structure is specified in section 4.11.11 with the general formats. Data transcript is created only if the request comes from the CDS. If the request comes from the EMTAS, then data transcript will be not created.

More than one data transcript records may be generated for one request.  

In the case that there exist no value for any trading hour or a profile (see more information in section 5.13 Allocation of profiles to IS OTE data, clause „Settlement – Daily data“), it means that this hour is not a part of the data transcript.

	ISOTEDATA/Trade/ProfileData
	Meaning/Comment

	Hour
	Mandatory field – always has the value „0“.


Note. In the response to the query requesting daily settlement the sign convention for volume and price will be similar to that in the results of the hourly settlement request. See more information in section 5.13 Allocation of profiles to IS OTE data, clause „Settlement – Daily data“.
4.11.6 Data request – OTE settlement rate

This communication script will allow determining OTE settlement rate used for the Day-ahead market settlement in CZK.
Automatic transmission of the settlement rate after entering to the system:

When entering the final OTE settlement rate it will be distributed by the system to all participants, which on that day (rate date) have applicable activity permissions to conduct trading operations on the DM market. 

The rate is distributed by automatic communication as an XML document in the ISOTEDATA system structure.

Settlement rate transmission as the response to a request:

Participant in the request specifies the period (from – to), for which the participant requires to obtain the rate. 

A report in the ISOTEDATA format will be transmitted in response to an inquiry. The report will  contain a settlement rate for each day of the period, in which the rate is available.

4.11.6.1 Request (ISOTEREQ) – 425

The attributes will be used as follows:

Location date-time-from   commencement of the period, for which the settlement rate was required

Location date-time-to           expiry of the period, for which the settlement rate was required 

Other attributes are not used in the Location element.

4.11.6.2 Response (RESPONSE) – 426

The response structure is specified in section 4.14.1 with the general formats
4.11.6.3 Data – OTE settlement rate (ISOTEDATA) – 427

ISOTEDATA attributes will be used as follows:

Trade  trade-day                    
the date of a trading day, for which the rate is transmitted

Trade / Profile-data / Data /value      
the rate value in CZK/EUR with an accuracy to 3 decimal positions

Trade / Profile-data /Data  unit        
„-„ – without a unit (the matter is referred to a mandatory field)

Trade / Profile-data profile-role

„R01“OTE settlement rate 

4.11.7 Notification of the final plan aggregation of traded volume

The matter is referred to a communication script, when trading system transmits information to the rest of the systems in order to perform particular actions; in this particular case - the aggregation of  traded volume final plan. The plan is being dynamically altered over time depending on trading hours closure on the DM. Notification will be generated automatically 1x per day after aggregation of the last trading hours on the IM market (after 20:00). Notification will be distributed via a RESPONSE message among all SS. When assigning of a mail to CDS it is possible to make a decision related to a dedicated SS, whether such information would be transmitted or would remain in the CDS system in the unsent messages folder (or messages sent to a default CDS mail).
4.11.7.1 Response – 972 (RESPONSE) 

The response structure is specified in section 4.14.1 with the general formats. 

4.11.8 Settlement performance notification 

The matter is referred to a communication script, when trading system transmits information to the rest of the systems in order to perform particular actions; settlement in this particular case. Notification will be distributed via a RESPONSE message among all SS, which at least one day were SS within a defined period. When assigning of a mail to CDS it is possible to make a decision related to a dedicated SS, whether such information would be transmitted or would remain in the CDS system in the unsent messages folder (or messages sent to a default CDS mail). There will be always just one notification for the operator-defined range of days for one run. Notification will be generated automatically as the last step in the clearing processing by the EMTAS, i.e. before the data sending to the SFVOT application (regarding the monthly and final monthly settlement the data will be transmitted to the SFVOT application just after the warranty period expiry). When assigning of a mail to CDS it is possible to make a decision related to a dedicated SS, whether such information would be transmitted to or would remain in the CDS system in the unsent messages folder (or messages sent to a default CDS mail).
4.11.8.1 Response – 982 (RESPONSE)

The response structure is specified in section 4.14.1 with the general formats. 

4.11.9 RD aggregation notification

The matter is referred to a communication script, when trading system transmits information to the rest of the systems in order to perform particular actions; RD aggregation in this case. Notification will be distributed via a RESPONSE message among all SS, which have an applicable activity permission to conduct trading operations on the DM market. When assigning of a mail to CDS it is possible to make a decision related to a dedicated SS, whether such information would be transmitted or would remain in the CDS system in the unsent messages folder (or messages sent to a default CDS mail). Notification will be generated automatically as a part of the RD aggregation procedure, i.e. after the end of the successful aggregation procedure.  

4.11.9.1 Response – 992 (RESPONSE) 

The response structure is specified in section 4.14.1 with the general formats. 

4.11.10 DM and Gas DM bids matching notification

The matter is referred to a communication script, when trading system transmits information to the rest of the systems in order to perform particular actions; DM and Gas DM bids matching in this case. Notification will be distributed via a RESPONSE message among all SS, which have an applicable activity permission to conduct trading operations on the DM and Gas DM market. When assigning of a mail to CDS it is possible to make a decision related to a dedicated SS, whether such information would be transmitted or would remain in the CDS system in the unsent messages folder (or messages sent to a default CDS mail). Notification will be generated automatically after the end of the successful DM and Gas DM bids matching procedure.  

4.11.10.1 Response – 997 (RESPONSE) 

The response structure is specified in section 4.14.1 with the general formats. 

4.11.11 Result transcripts general format (ISOTEDATA - 943, 946, 953, 963)

The meaning of items is entirely consistent with the meanings specified in section 4.11.1 and in the structure set out in section 5.5. Mandatory fields are marked with hatching. Other items are optional. 

4.11.12 Data request – Statistical data of imbalance settlement

The request will allow determining the statistical data of imbalance settlement for a specific trading day and settlement version. One operation will contain just one request to identify settlement data, which results may contain more than one record. 
4.11.12.1 Request – 964 (ISOTEREQ) 

The data sentence structure expected in the EMTAS module. 

The meaning of items is entirely consistent with the meanings specified in section 4.11.1 and in the structure set out in section 5.5. Mandatory fields are marked with hatching. Other items are optional. 

The query may request a statistical data for a specific day and settlement version:

	ISOTEREQ/Trade
	Meaning/Comment

	Trade day
	Mandatory field

	Settlement version
	Mandatory field – only versions: 2 – Daily imbalance settlement, 3 - Interim monthly settlement, 4 – Final monthly settlement


4.11.12.2 Response – 965 (RESPONSE) 

The response structure is specified in section 4.14.1 with the general formats. 

4.11.12.3 Data transcript – 966 (ISOTEDATA) 

The data transcript structure is specified in section 4.11.11 with the general formats. Data transcript is created only if the request comes from the CDS. 
The data transcript may generate several records for a single request.
If some profile is filled in data transcript, then all hours of trade day are filled.

Both price and volume are noted with sign in all settlement concepts of data transcript (see section 5.13- Allocation of profiles to IS OTE data - „Statistical data of imbalance settlement “ part).

Price of contrary imbalance is valid from 2010/01/01. Requests on delivery day before this date will not return data of this profile.

4.12 Settlement and aggregation communication scripts for gas trading

Single items of this section are defined in the maximum classification, which means that some items may be accumulated in a common format of the data into one item (e.g., items of a date type), or may not be used at all.
4.12.1 Settlement result items structure determination – ISOTEDATA

The sentence structure will consist of the following items:

	ISOTEDATA
	Meaning/Comment

	Message code
	Message code identifying the message type.

	ISOTEDATA/Trade
	Meaning/Comment

	Date/Gas day
	Gas day or initial date in YYYY-MM-DD format.

	Matching ID
	A unique matching identifier within one day.

	Settlement version
	Settlement version identification (9 – Gas DM morning session, 10 – Gas DM afternoon session, 11 – Monthly settlement with gas, 12 – Final monthly settlement with gas, 13 – Gas IM daily settlement)

	Market type
	Market identification (DTP – Gas DM, VDP – Gas IM)

	ISOTEDATA/Trade/ProfileData
	Meaning/Comment

	Hour
	Identification of the trading hour within which the required action will be performed. The defined interval is 1 to 25, depending on the number of hours of a trading day. (winter/summer time shift – 23; summer/winter time shift – 25). Detailed records for each item must be clear and must be sorted in ascending order.
For daily settlement the item has always the value „0“.

	Volume
	Volume is determined for a specified trading hour. Volume is specified in tenth of MWh.

	Price
	Total price. Price is defined in CZK or EUR with accuracy to 2 decimal positions. 

	Currency code
	Currency specification (CZK, EUR).

	Profile identification
	Detailed information on the identification of profiles is specified in section 5.13 - Allocation of profiles to IS OTE data

	ISOTEDATA/Trade/Party
	Meaning/Comment

	Participant (EIC)/Anonymus participant/EIC
	Unique participant identification within IS OTE (EIC). Anonymous participant code, or EIC according to anonymity settings.


4.12.2 Data request – marginal prices for Gas DM

The request will allow determining marginal prices achieved on Gas DM market. One operation will contain just one request to determine the marginal prices related to a specific gas day, with a response containing one record or none.
4.12.2.1 Request – GDD (ISOTEREQ) 

The data sentence structure expected in the EMTAS module. 

The meaning of items is entirely consistent with the meanings specified in section 4.12.1 1 and in the structure set out in section 5.9. Mandatory fields are marked with hatching. Other items are optional. 

The query may request Gas DM marginal prices for a specific day:

	ISOTEDATA/Trade
	Meaning/Comment

	Date
	Mandatory item


4.12.2.2 Response – GDE (RESPONSE) 

The response structure is specified in section 4.14.1 with the general formats. 

4.12.2.3 Data transcript – GDF (ISOTEDATA) 

The data transcript structure is specified in section  4.12.4 with the general formats. Data transcript is created only if the request comes from the CDS. If the request comes from the EMTAS, then data transcript will be not created.

Only one data transcript may be generated for one request.  

Note: In the response to the request there is always a positive price (see more information in section 5.13 Allocation of profiles to IS OTE data, clause „DM marginal prices“).

4.12.3 Data request - Daily settlement
The request will allow determining settlement daily results specification for specified gas day and settlement version divided by according clearing concepts. One operation will contain just one request to determine settlement data, which result may contain more than one record.
4.12.3.1 Request – GSD (ISOTEREQ) 

The data sentence structure expected in the EMTAS module. 

The meaning of items is entirely consistent with the meanings specified in section 4.12.1 1 and in the structure set out in section 5.9. Mandatory fields are marked with hatching. Other items are optional. 

The query may request settlement results of a specific gas day and a settlement version:

	ISOTEDATA/Trade
	Meaning/Comment

	Date
	Mandatory field


4.12.3.2 Response – GSE (RESPONSE) 

The response structure is specified in section 4.14.1 with the general formats. 

4.12.3.3 Data transcript – GSF (ISOTEDATA) 

The data transcript structure is specified in section  4.12.4 with the general formats. Data transcript is created only if the request comes from the CDS. If the request comes from the EMTAS, then data transcript will be not created.

More than one data transcript records may be generated for one request.  

	ISOTEDATA/Trade/ProfileData
	Meaning/Comment

	Hour
	Mandatory field – always has the value „0“.


Note. In the response to the query requesting daily settlement the sign convention for volume and price will be similar to that in the results of the hourly settlement request. See more information in section 5.13 Allocation of profiles to IS OTE data, clause „Settlement – Daily data“.
4.12.4 Result transcripts general format (ISOTEDATA - GDF, GSF)

The meaning of items is entirely consistent with the meanings specified in section 4.12.1 and in the structure set out in section 5.9. Mandatory fields are marked with hatching. Other items are optional. 

Communication scripts of enquiries for financial settlement data SFVOT

The financial reports have the same businness logic for communication scripts. Data are automatically distributed, when the settlement would be done. Anyway client should request it by SFVOTREQ message.

Reporty a jejich kódy:

	Report name
	Structure
	The request code
	The data code
	The response code

	Billing Report
	SFVOTBILLING
	400
	401
	402

	Billing Report OTE
	SFVOTBILLING
	403
	404
	405

	Report of Claims
	SFVOTCLAIM
	406
	407
	408

	Report of Claims OTE
	SFVOTCLAIM
	409
	410
	411

	Clearing of Load Profiles (TDD) Differences
	SFVOTTDD
	412
	413
	414

	Clearing of Load Profiles (TDD) Differences OTE
	SFVOTTDD
	415
	416
	417

	Billing Report PXE - OTE
	SFVOTBILLINGEMO
	418
	419
	420

	Billing Report OTE - PXE
	SFVOTBILLINGEMO
	421
	422
	423

	List of included receivables and payables
	SFVOTDTEXPIMP
	428
	429
	430

	Daily report for bank (credit-debit/confirmation)
	SFVOTCONFDATA
	431
	432
	433

	Billing Report  – summary
	SFVOTBILLINGSUM
	434
	435
	436

	Billing Report OTE – summary
	SFVOTBILLINGSUM
	437
	438
	439

	Report of Claims – summary
	SFVOTCLAIMSUM
	440
	441
	442

	Report of Claims OTE – summary
	SFVOTCLAIMSUM
	443
	444
	445


4.12.4.1 Request for financial report – (SFVOTREQ) 

The meaning of items:

	Item
	Meaning

	SFVOTREQ@message-code
	The report code

	SFVOTREQ/SenderIdentification@id
	Subject identifier (EAN or EIC), it must match the ID resolved from signature certificate.

	SFVOTREQ/ReceiverIdentification @id
	OTE identifier (EAN or EIC).

	SFVOTREQ/Interval@date-from
	start of period for report

	SFVOTREQ/Interval@date-to
	end of period for report


4.12.4.2 Response for report request – (RESPONSE) 

If client requested some report, then response message is returned.

Response codes (RESPONSE/Reason@code) for financial reports:
	ID
	Description
	Returns Data
	Notes

	9000
	In order
	Yes
	Reason does not contain any text. XML with data cannot be empty. 

	9001
	No data found 
	No
	Reason does not contain any text.

	9002
	Enquiry for data is not a valid XML. 
	No
	Error description is in Reason

	9003
	Error in the reporting module.
	No
	Reason does not contain any text.

	9004
	Other error of the financial module.
	No
	Reason does not contain any text.

	9005
	Warning: In the selected period an Emergency Status was announced. The values of daily settlement are not valid for invoicing.
	Yes
	Reason does not contain any text.


The reports description are in the appropriates XML schemas.

4.13 IS OTE general scripts

4.13.1 Mail structure items meaning – RESPONSE
E-mail message structure for the area, which means that the processing evaluation will contain following fields.

1 – Message code: message type identification. It is a 3-digit alphanumeric chain. 

2 – Bid code: identification code of the bid/order used within EMTAS. It is a ten-digit number. Together with the bid version (item 3) they make up the unique bid identifier. If the bid/offer was not created/found  then the item will be left empty. 

3 – Bid version: The bid version within EMTAS. It is a 5-digit number. Together with the bid code they make up the unique bid identifier. If the bid/offer was not created/found  then the item will be left empty. 

4 – Description message of the receiver/Message body: own text of notification, warning or error. 

5 – Error code: number of notification/warning/error. 

6 – Error type: error type identification. It is a 3-digit alphanumeric chain. 

7 – Sender Identification: identification of the sender. For electricity trading usually EAN OTE, for gas trading usually EIC OTE. 

8 – Receiver Identification: identification of the receiver of the message. For electricity trading usually EAN, for gas trading usually EIC. 

9 - Message identifier: consequently, in the case of client-server communication, it is used for enquiring the process results. 

4.13.2 IS OTE data transfer application (request) 

The matter is referred to a particular request type, which is relevant only for certain architecture type like client-server asynchronous communication through http(s) channels. This Request is used to obtain a response (output data) for asynchronous processing of another (previous) data request. 

Data transfer request will acquire following results:

· Bid status determination
· Resultant BalM prices 
· Notice board data
· Market results
· Trading hours data
· DM bid status determination
· BM order status determination
· BM trade status determination
· BM instance (product) data
· DM trade results determination in the area
· DM SS trade results determination 
· RD status determination
· MCC volume determination

Data request is processed with the WAS/CDS tools. 

4.13.2.1 Request – 921 (ISOTEREQ) 

As a unique identifier of the requested data (reference data exchange in asynchronous processing via HTTPs client-server) there will be used a RESPONSE message number, which the WAS system returns synchronously (within a single session) at entering a previous appropriate request into the external data system

If this number is not included into the report, the WAS system returns the first identified data file found in the table of unsent messages. 

Processing procedure:

· One of the requests is transferred to the system via a HTTPs channel:

· Request MSG_CODE 881 – Bid status determination
· Request MSG_CODE 884 – Resultant BalM prices 
· Request MSG_CODE 891 – Notice board data
· Request MSG_CODE 901 – Market results
· Request MSG_CODE 911 – Trading hours data
· Request MSG_CODE 831 – DM bid status determination
· Request MSG_CODE 864 – BM order status determination
· Request MSG_CODE 874 – BM trade status determination
· Request MSG_CODE 877 – BM instance (product) data
· The system receives data in a single session, sends back RESPONSE with information on receiving a data request. The identifier of this message (report) will be used by the external system to identify a processing result with subsequent sending of the request to ISOTEREQ with the MSG_CODE 921 IS OTE data transfer request. For a repeated query with the same request an initial identifier is used for the subsequent processing of the application. After sending RESPONSE synchronous connection closes.

· After that the external system sends a request containing the MSG_CODE 921 IS OTE data transfer request with the above mentioned data exchange reference number.

· The WAS system will check resulting data in the unsent messages table and synchronously send the data back to the external system
4.13.2.2 Request – 922 (RESPONSE) 

In the event that in the communication server WAS at a current time the data related to the reference number assigned to the data exchange requirement 921 of data exchange are not available or if the reference number is not specified (in the case that the system is not able to find any data for a specific RMP in the unsent messages table) the WAS system returns as an output the RESPONSE with an appropriate error code and error message.

4.13.3 Code list of logical errors incurred during instructions/request processing 

The contractor reserves the right to update the list of errors.

Errors on the IM&BalM:

	Notification
	Used in:
	 

	ID
	Description
	Type
	Submission / 

Replacement
	Cancellation
	Acceptation
	Enquiry
	Notes

	2200
	The guarantee limits are not fulfilled.
	E
	*
	*
	*
	 
	 

	2261
	Meets guarantee: Guarantee limits are almost used up.
	W
	*
	*
	*
	 
	 

	2536
	Your user rights are insufficient for completing this operation.
	E
	*
	*
	*
	
	

	2923
	Action has been completed successfully.
	I
	*
	*
	*
	
	

	3029
	Participant %s is not registered as a market participant. 
	E
	*
	*
	*
	 
	 

	3122
	Participant %s does not exist. 
	E
	*
	*
	*
	*
	 

	3143
	Error in hour %d: invalid electricity volume. 
	E
	*
	 
	*
	 
	 

	3422
	Aggregation of hour %d3 of IM for trading day %d1 was conducted.
	I
	
	
	
	
	After closing the last hour of IM for trading day.

	4003
	No date found in table CALENDER.
	E
	*
	 
	 
	 
	 

	4004
	Participant %s does not have a right to access the IM market.
	E
	*
	*
	*
	 
	 

	4005
	Participant %s does not have access rights to the BalM market.
	E
	*
	*
	*
	 
	 

	4008
	Error in hour %d: amount of electricity may not be 0. 
	E
	*
	 
	 
	 
	 

	4009
	Error in hour %d: price may not be 0. 
	E
	*
	 
	 
	 
	 

	4010
	Error in hour %d: invalid price. 
	E
	*
	 
	 
	 
	 

	4011
	Error in hour %d: the Volume in the block may not be divisible. 
	E
	*
	 
	 
	 
	 

	4014
	Time validity of the bid must be smaller then the Closing time of the last hour of the bid.
	E
	*
	 
	 
	 
	 

	4015
	Time validity of the bid must be higher then the current time. 
	E
	*
	 
	 
	 
	 

	4016
	For the given trading day there are no trading hours generated. 
	E
	*
	 
	 
	 
	 

	4019
	Error in bid header: participant is a mandatory field. 
	E
	*
	 
	 
	 
	 

	4023
	Error in bid header: invalid date. 
	E
	*
	 
	 
	 
	 

	4024
	Error in bid header: bid type is a mandatory field. 
	E
	*
	 
	 
	 
	 

	4025
	Error in bid header: invalid bid type. 
	E
	*
	 
	*
	 
	 

	4026
	Error in bid header: invalid bid order. 
	E
	*
	 
	 
	 
	 

	4027
	Error in bid header: invalid time validity of bid.
	E
	*
	 
	 
	 
	 

	4028
	Error in bid header: Total Acceptance of bid is a mandatory field. 
	E
	*
	 
	 
	 
	 

	4029
	Error in bid detail: hour is a mandatory field. 
	E
	*
	 
	*
	 
	 

	4030
	Error in bid detail: invalid hour. 
	E
	*
	 
	*
	 
	 

	4031
	Error in the hour %d: electricity is a mandatory field. 
	E
	*
	 
	*
	 
	 

	4032
	Error in the hour %d: invalid electricity.
	E
	*
	 
	*
	 
	 

	4033
	Error in the hour %d: price is a mandatory field. 
	E
	*
	 
	 
	 
	 

	4034
	Error in the hour %d: invalid price.
	E
	*
	 
	 
	 
	 

	4035
	Error in the hour %d: Volume divisibility is a mandatory field.
	E
	*
	 
	 
	 
	 

	4036
	Error in the hour %d: invalid Volume divisibility. 
	E
	*
	 
	 
	 
	 

	4038
	Error in bid detail: hours must be in an ascending order.
	E
	*
	 
	*
	 
	 

	4039
	Error in bid detail
	E
	*
	 
	*
	 
	 

	4043
	No data found in the processing table.
	E
	*
	*
	*
	*
	 

	4044
	Error in bid header: bid code is a mandatory field. 
	E
	 
	*
	*
	 
	 

	4045
	Error in bid header: invalid bid code. 
	E
	 
	*
	*
	 
	 

	4046
	Error in bid header: bid version is a mandatory field 
	E
	 
	*
	*
	 
	 

	4047
	Error in bid header: invalid bid version 
	E
	 
	*
	*
	 
	 

	4048
	Error in bid header: market type is a mandatory field. 
	E
	 
	 
	*
	 
	 

	4049
	Error in bid header: invalid market type.. 
	E
	 
	 
	*
	 
	 

	4051
	Invalid operation type.
	E
	*
	*
	*
	 
	Only for access from the WEB

	4054
	Acceptation of bid %d1 after the trading hour %d2 on the market %d3. 
	E
	 
	 
	*
	 
	 

	4057
	Error in hour%d: open trading hour not found. 
	E
	*
	 
	 
	 
	 

	4058
	Error in hour %d: hour > max. amount of hours 
	E
	*
	 
	 
	 
	 

	4059
	No data found in table  IM_PARAMETERS. 
	E
	*
	 
	*
	 
	 

	4060
	Error in hour %d: open trading hour not found.
	E
	*
	 
	*
	 
	 

	4061
	Error in hour %d: electricity amount is a mandatory field. 
	E
	*
	 
	*
	 
	 

	4062
	There is no open trading hour for the bid.
	E
	*
	*
	*
	 
	 

	4063
	Bid not found. 
	E
	*
	*
	*
	 
	 

	4064
	Bid was cancelled. 
	E
	*
	 
	 
	 
	 

	4065
	Bid was fully or partially accepted.
	E
	*
	 
	 
	 
	 

	4066
	Another participant is working with the bid at the moment. Please try again later. 
	E
	*
	*
	*
	 
	 

	4067
	Error in hour%d: invalid electricity, max. decimal places: %s. 
	E
	*
	 
	*
	 
	 

	4068
	Participant %s has no rights to submit bids on IM.
	E
	*
	*
	*
	 
	 

	4069
	Participant %s has no rights to accept bids on IM.
	E
	*
	*
	*
	 
	 

	4070
	Participant %s does not have right to submit BalM bids.
	E
	*
	*
	*
	 
	 

	4071
	Participant %s does not have right to conduct BalM acceptation.
	E
	*
	*
	*
	 
	 

	4074
	Participant %s has no entry rights (modification).
	E
	*
	*
	*
	 
	 

	4075
	Error during trade type assessment. 
	E
	 
	*
	 
	 
	 

	4077
	Bid does not fulfill the conditions for cancellation. 
	E
	 
	*
	 
	 
	 

	4078
	Bid was already withdrawn. 
	E
	 
	*
	*
	 
	 

	4079
	Bid may be cancelled only by the owner of the bid. 
	E
	 
	*
	 
	 
	 

	4080
	Error in bid header: invalid Total Acceptance. 
	E
	*
	 
	 
	 
	 

	4081
	Bid may be replaced only by the owner of the bid. 
	E
	*
	 
	 
	 
	 

	4082
	Error in bid header: process type is a mandatory field.
	E
	 
	*
	 
	 
	 

	4083
	Error in bid header: invalid process type. 
	E
	 
	*
	 
	 
	 

	4085
	Bid was not processed due to the rejection of the whole amount.
	E
	 
	*
	 
	 
	 

	4086
	May not be cancelled, the bid was fully accepted. 
	E
	 
	*
	 
	 
	 

	4091
	For the bid%d no trading hours were found. 
	E
	 
	 
	*
	 
	 

	4092
	When accepting the whole bid all trading hours must be accepted. 
	E
	 
	 
	*
	 
	 

	4093
	Error in hour %d: trading on the market %t is closed. 
	E
	 
	 
	*
	 
	 

	4094
	Error in hour %d: electricity for this hour must be accepted as a whole. 
	E
	 
	 
	*
	 
	 

	4095
	Error in hour %d: for successful acceptation only %c unit of electricity is left. 
	E
	 
	 
	*
	 
	 

	4096
	Accepted bid is not active. 
	E
	 
	 
	*
	 
	 

	4097
	Accepted bid was already replaced. 
	E
	 
	 
	*
	 
	 

	4098
	Accepted bid was already cancelled. 
	E
	 
	 
	*
	 
	 

	4101
	Error occurred when processing SFVOT.
	E
	*
	*
	*
	
	

	4102
	Error in hour%d: bid must be accepted as a whole. 
	E
	 
	 
	*
	 
	 

	4114
	Error in hour %d: Hour in bid%n not found. 
	E
	 
	 
	*
	 
	 

	4115
	Unexpected parameter for block processing. 
	E
	
	*
	
	
	

	4116
	Error occurred when processing SFVOT. Error code = %s.
	E
	*
	*
	*
	
	

	4117
	Unexpected processing code ( %s ) of SFVOT record.
	E
	*
	*
	*
	
	

	4119
	For the participant %s no bid unit was found. 
	E
	*
	 
	*
	 
	 

	4120
	User rights check – invalid operation type %s. 
	E
	*
	*
	*
	 
	 

	4121
	Only the remaining amount of electricity was accepted. 
	E
	 
	 
	*
	 
	 

	4122
	In the bid %s no electricity was accepted. 
	E
	 
	 
	*
	 
	 

	4123
	In the bid the total amount of electricity is 0.
	E
	*
	 
	 
	 
	 

	4124
	Bid/version/hour: required-confirmed
	E
	 
	 
	*
	 
	 

	4127
	Bid may not be created, participant is not the bid owner. 
	E
	*
	 
	 
	 
	 

	4128
	Bid was already accepted by another user. 
	E
	 
	 
	*
	 
	 

	4129
	Error in hour %d: the electricity was already accepted by another user.
	E
	 
	 
	*
	 
	 

	4130
	Error in bid detail: invalid bid hour.(%d) 
	E
	*
	 
	*
	 
	 

	4131
	Error in bid header: invalid %d. header item. %c 
	E
	*
	*
	*
	 
	 

	4134
	Bid may not be accepted, bid is submitted for IM.
	E
	 
	 
	*
	 
	 

	4138
	Error when generating bid sequence order. 
	E
	 
	 
	 
	 
	 

	4146
	Total acceptance of bid must be N. 
	E
	*
	
	
	
	

	4161
	Max. number of submitted orders by a participant within a trading day was reached. 
	E
	*
	
	
	
	

	4162
	Index “%s” of accepted bid was not found during profile table survey. 
	E
	
	
	*
	
	

	4163
	Max. number of submitted orders within a trading day could not be detected. 
	E
	*
	
	
	
	

	4165
	Participant %s1 doesn’t have conveyed imbalance responsibility for %s2.
	E
	*
	*
	*
	
	

	4171
	Own bid may not be accepted.
	E
	
	
	*
	
	

	4172
	Only TSO’s bids may be accepted. 
	E
	
	
	*
	
	

	4175
	Max. number of acceptations for participant within day and hour %s was exceeded.
	E
	
	
	*
	
	

	5011
	Error when calling the API function. Error code =%s. 
	E
	*
	*
	*
	*
	 

	5022
	Error in header: bid code is missing. 
	E
	 
	 
	 
	*
	 

	5023
	Error in header: bid version is missing. 
	E
	 
	 
	 
	*
	 

	5024
	Error in header: bid code and version or date is missing. 
	E
	 
	 
	 
	*
	 

	5500
	Bid was created with a code %d1and version %d2. 
	I
	*
	 
	 
	 
	 

	5501
	Bid was accepted with a code %d1and version%d2. 
	I
	 
	 
	*
	 
	 

	5502
	Acceptation bid was created with a code %d1 and version %d2. 
	I
	 
	 
	*
	 
	 

	5503
	Bid was cancelled with a code %d1 and version %d2. 
	I
	 
	*
	 
	 
	 

	5504
	Enquiry executed. Data found 
	I
	 
	 
	 
	*
	 

	5505
	Enquiry executed. No data found
	I
	 
	 
	 
	*
	 

	5521
	The IM notice board for the trading day %s was changed.
	I
	
	
	
	
	Distribution of data on the notice board

	5522
	The BM notice board for the trading day %s was changed.
	I
	
	
	
	
	Distribution of data on the notice board

	5538
	Inquiry conducted. Data not available yet.
	I
	
	
	
	*
	


Errors on DM:

	Notification
	 

	ID
	Description
	Type
	Submission / 

Renewal
	Cancellation
	Enquiry
	Notes

	2000
	Session is closed.
	E
	*
	
	
	

	2007
	Only one indivisible block per hour is allowed, unless it is an overfilling.
	E
	*
	
	
	

	2009
	Price of a bid is smaller than the minimal allowed price in the system. 
	E
	*
	
	
	

	2010
	Price of the bid is higher than the maximal allowed price in the system.
	E
	*
	
	
	

	2011
	Offered hourly amount is lower than the allowed minimum in the system. 
	E
	*
	
	
	

	2012
	Offered hourly amount is higher than the allowed minimum in the system.
	E
	*
	
	
	

	2014
	In the offer for buy prices must be strictly descending. 
	E
	*
	
	
	

	2015
	Prices on the side of production must be at each consequent block strictly ascending.
	E
	*
	
	
	

	2019
	Trading day must be higher than the date of the actual day.
	E
	*
	
	
	

	2020
	In the table of parameters there is no record.
	E
	*
	
	
	

	2024
	Indivisible blocks must always have the lowest price of all blocks.
	E
	*
	
	
	

	2027
	Offering participant has no rights for this type of bid.
	E
	*
	
	
	

	2038
	Amount is 0 for each hour of the bid. 
	E
	*
	
	
	

	2200
	Guarantee limits are not fulfilled.
	E
	*
	*
	
	

	2201
	The product of amount and price in every hour of the bid is 0.
	E
	*
	
	
	

	2261
	Guarantees fulfilled: Guarantee limits are almost exhausted.
	W
	*
	*
	
	

	2262
	SFVOT - error %d occurred when verifying guarantee.
	E
	*
	*
	
	

	2264
	SFVOT – guarantee limits are locked. Please repeat the action later. 
	E
	*
	*
	
	

	2501
	The clocks will change on Sunday.
	I
	*
	
	
	

	2502
	Today, the time change takes place. 
	I
	*
	
	
	

	2531
	The cancellation date cannot be lower than the date of the actual session.
	E
	
	*
	
	

	2532
	The bid was cancelled for this date %d.
	E
	
	*
	
	

	2538
	Bid for participant %s cannot be entered
	E
	*
	
	
	

	2604
	Unauthorized value of electricity amount.
	E
	*
	
	
	

	2605
	Unauthorized value of price.
	E
	*
	
	
	

	2627
	Divisibility attribute must be Y in bid offers.
	E
	*
	
	
	

	2632
	In bid offers, the attribute for total acceptance of first block must be N.
	E
	*
	
	
	

	2638
	The bid does not fulfill the necessary conditions for cancellation.
	E
	
	*
	 
	

	2641
	The participant is not a valid  settlement subject (from %d1 to %d2).
	E
	*
	*
	 
	

	2642
	The participant may not participate on the day-ahead market (from %d1 to %d2).
	E
	*
	*
	 
	

	2643
	Error in the bid header: Total Acceptance of the 1st Block is a mandatory field.
	E
	*
	
	
	

	2644
	Error in the bid header: invalid Total Acceptance of Block 1.
	E
	*
	
	
	

	2645
	Error in the bid header: identification of the bid block is a mandatory field.
	E
	*
	
	
	

	2646
	Error in the bid header: invalid identification of the bid block.
	E
	*
	
	
	

	2648
	Participant is not 
uthorized to participate in the day-ahead-market.
	E
	*
	*
	
	

	2929
	Default settlement currency code not found.
	E
	*
	
	
	

	2649
	Error in bid header: settlement currency code is required data.
	E
	*
	
	
	

	2650
	Error in bid header: invalid settlement currency code.
	E
	*
	
	
	

	2923
	Action has been completed successfully.
	I
	*
	*
	
	

	2924
	Request %s is waiting for the financial security check. Check the request queue.
	I
	*
	*
	
	

	3015
	The participant does not have the necessary permission to realize this operation.
	E
	*
	*
	
	

	3029
	The participant %s is not registered as a market participant. 
	E
	*
	*
	
	

	3122
	The participant %s does not exist. 
	E
	*
	*
	*
	 

	3165
	Unexpected cancellation type.
	E
	
	*
	
	

	3423
	The bid matching process for trading day %d1 was conducted.
	I
	
	
	
	After finishing DM matching.

	3424
	The new MCC for delivery day %d1 was defined.
	I
	
	
	
	After receiving MCC for delivery day.

	3570
	Error in syntax in verifying bid blocks.
	E
	*
	
	
	

	3700
	There was no detail entered for this bid.
	E
	*
	
	
	

	4019
	Error in the bid header: the participant is a mandatory field.
	E
	*
	 
	 
	 

	4023
	Error in the bid header: invalid date.
	E
	*
	 
	 
	 

	4024
	Error in the bid header: bid type is a mandatory field.
	E
	*
	 
	 
	 

	4025
	Error in the bid header: invalid bid type. 
	E
	*
	 
	 
	 

	4029
	Error in the bid header: bid hour is a mandatory field.
	E
	*
	 
	 
	 

	4030
	Error in the bid header: invalid bid hour.  
	E
	*
	 
	 
	 

	4031
	Error in the hour %d: electricity is a mandatory  field. 
	E
	*
	 
	 
	 

	4033
	Error in the hour %d: price is a mandatory field. 
	E
	*
	 
	 
	 

	4035
	Error in the hour %d: Volume Divisibility is a mandatory field.
	E
	*
	 
	 
	 

	4036
	Error in the hour %d: Invalid Volume Divisibility.
	E
	*
	 
	 
	 

	4039
	Invalid bid detail. 
	E
	*
	 
	 
	 

	4043
	Data not found in the processing table. 
	E
	*
	*
	*
	 

	4044
	Error in the bid header: bid code is a mandatory field. 
	E
	 
	*
	 
	 

	4046
	Error in the bid header: bid version is a mandatory field. 
	E
	 
	*
	 
	 

	4051
	Invalid operation type. 
	E
	*
	*
	 
	

	4063
	Bid was not found. 
	E
	*
	*
	 
	 

	4077
	The bid does not fulfill the conditions for cancellation.
	E
	 
	*
	 
	 

	4079
	The bid may be cancelled only by the owner of the bid. 
	E
	 
	*
	 
	 

	4118
	Invalid bid header.
	E
	*
	
	
	

	4131
	Error in the bid header: invalid %d. header item %c 
	E
	*
	*
	 
	 

	5011
	Error when calling the API function. Error code = %s. 
	E
	*
	*
	*
	 

	5500
	Bid was created with a code %dl and version %d2. 
	I
	*
	 
	 
	 

	5503
	Bid was cancelled with a code %d1 and version %d2.
	I
	 
	*
	 
	 

	5504
	Enquiry was accomplished. Data was found.
	I
	 
	 
	*
	 

	5505
	Enquiry was accomplished. No data was  found.
	I
	 
	 
	*
	 

	5528
	Bid was cancelled by the market operator. 
	I
	
	*
	
	In the case of cancellation of all valid trades on the back of changes in rights validity of SS. 

	5537
	Bid has been cancelled by system (SFVOT).
	I
	
	*
	
	


Errors on the BM :

	Notification
	

	ID
	Description
	Type
	Order Submission
	Order Cancellation
	Enquiry
	Notes

	2641
	The participant is not a valid  settlement subject (from %d1 to %d2).
	E
	*
	*
	 
	

	6000
	The Participant %s placing an order for sell does not have selling rights.
	E
	*
	
	
	

	6001
	The Participant %s placing an order for buy does not have  buying rights.
	E
	*
	
	
	

	6002
	The participant %s has no rights to participate on the BM (from %d1 to %d2).
	E
	*
	*
	
	

	6003
	The participant %s has no rights to submit/cancel orders.
	E
	*
	*
	
	

	6004
	The order was not entered. The product is not a valid product on the block market.
	E
	*
	
	
	

	6005
	The order was entered as invalid. The product %s2 is not published.
	E
	*
	
	
	

	6006
	The order %s1 was entered as invalid. The product %s2 is not in a period, when it is possible to trade with it.
	E
	*
	
	
	

	6007
	The order %s1 was entered as invalid. The product %s2 is in the period for submitting orders for market makers and the participant %s3 does not have delegated rights of a Market Maker.
	E
	*
	
	
	

	6008
	The order %s1 was entered as invalid. Product %s2 is not in the period designated for submitting orders. 
	E
	*
	
	
	

	6009
	The order %s1 was entered as invalid. The number of contracts %s2 of the order exceeds the set limit %s3.
	E
	*
	
	
	

	6010
	The order %s1 was entered as invalid. The financial volume %s2 of all active orders surpasses the set limit %s3 of the participant.
	E
	*
	
	
	

	6011
	The order %s1 was entered as invalid. The actual financial security of the participant %s2 is insufficient.
	E
	*
	
	
	

	6012
	The order %s1 was entered as invalid. The order submitted by the market maker %s2 there must be a defined limit price.
	E
	*
	
	
	

	6013
	The order %s1 was entered as invalid. The limit price %s2 exceeds the allowed price interval of the product (%s3 - %s4).
	E
	*
	
	
	

	6014
	The order %s1 was entered as invalid. The number of contracts %s2 does not comply with the integer of the multiplied product parameters. The minimum tradable unit is =%s3.
	E
	*
	
	
	

	6015
	The order %s1 cannot be cancelled. The participant %s does not have rights to cancel orders.
	E
	
	*
	
	

	6016
	The order %s1 cannot be cancelled. The order may be cancelled only by its owner.
	E
	
	*
	
	

	6017
	The order %s1 cannot be cancelled. The product %s2 is outside of the trading period , when the instruction for cancellation cannot be processed. 
	E
	
	*
	
	

	6018
	The order %s1 cannot be cancelled. The number of orders of a market maker of the same type %s2 would be 0. 
	E
	
	*
	
	

	6019
	Cancellation of all orders according to product %s1 was completed with an error. Cancellation was not executed.
	E
	
	*
	
	

	6021
	Order was created with a code %s.
	I
	*
	
	
	

	6022
	Order was cancelled with a code %s.
	I
	
	*
	
	

	6023
	The order %s1 was already cancelled.
	E
	
	*
	
	

	6024
	By matching of the order with the number %s1 of the product %s2  the trade %s3 was created.
	I
	*
	
	
	

	6026
	Item %s is filled in incorrectly. 
	E
	*
	*
	*
	

	6037
	Error in the header of the order: invalid %d. item in the order.
	E
	*
	
	
	

	6038
	Invalid order header. 
	E
	*
	
	
	

	6039
	Error in the header of the order: invalid order type %s.
	E
	*
	
	
	

	6040
	Error in the header of the order: product name is a mandatory field.
	E
	*
	
	
	

	6041
	Error in the header of the order: trade type is a mandatory field.
	E
	*
	
	
	

	6042
	Invalid order detail.
	E
	*
	
	
	

	6043
	Error in the order detail: number of contracts is a mandatory field.
	E
	*
	
	
	

	6044
	Error in the order detail: invalid number of contracts %s.
	E
	*
	
	
	

	6045
	Error in the header of the order: invalid product name %s.
	E
	*
	
	
	

	6046
	No data was found in the table of FS status.
	E
	*
	
	
	

	6047
	It was found, when submitting the order %s1 on the BM that the actual status of the FS of the participant %s2 is insufficient.
	E
	*
	
	
	

	6048
	No data was found in the table of defined financial limits of orders for the given RMP. 
	E
	*
	
	
	

	6049
	It was found, when submitting the order %s1 on the BM that the FS limit of the participant %s2 was exceeded. 
	E
	*
	
	
	

	6050
	It was found, when submitting the order %s1 on the BM by the participant %s2 that the contracts in the order are outside of the set limit. 
	E
	*
	
	
	

	6051
	Message code %s1 not found in global structure.
	E
	*
	*
	
	

	6052
	The order was entered as invalid. Submitting an order without a limit price is not allowed. 
	E
	*
	
	
	

	6053
	Error in the header of the order: invalid trade type %s.
	E
	*
	
	
	

	6054
	Error in the order detail: order code is a mandatory field. 
	E
	*
	
	
	

	6055
	Error in the order detail: invalid order code %s. 
	E
	*
	
	
	

	6056
	The order %s was not found. 
	E
	
	*
	*
	

	6057
	The order %s1 cannot be cancelled, does not fulfill the conditions for cancelling.
	E
	
	*
	
	

	6058
	The order %s1 cannot be cancelled, as it was already traded as a whole.
	E
	
	*
	
	

	6059
	The order %s1 cannot be cancelled, as it is being processed.
	E
	
	*
	
	

	6060
	Too many parameters; Submit either the order ID or Product or Data of entry of the order. 
	E
	
	
	*
	

	6061
	Missing parameter: Submit order ID.
	E
	
	*
	*
	

	6062
	Missing parameter: submit trade ID.
	E
	
	
	*
	

	6063
	Too many parameters; Submit either the order ID or Product or Data of origin of trade.
	E
	
	
	*
	

	6064
	Missing parameter: Submit at least one parameter.
	E
	
	*
	*
	

	6065
	For the order %s1 the trade %s2 was created.
	I
	*
	
	
	

	6066
	The order was cancelled by the system.
	I
	
	*
	
	

	6067
	BM aggregation of the product %s1 was conducted.
	I
	
	
	
	After product aggregation on BM.

	6068
	The product %s1 has been issued on block market.
	I
	
	
	
	After product issue on BM.

	6069
	Trading of the product %s1 has been opened on block market.
	I
	
	
	
	After opening product trading on BM.

	6070
	Trading of the product %s1 has been closed on block market.
	I
	
	
	
	After closing product trading on BM.

	6071
	Data of the product %s1 traded on BM has been finalized.
	I
	
	
	
	After finalizanig product trading data on BM.

	6072
	The cancellation of set of orders was completed with an error. Details are stated in the audit log.
	E
	
	*
	
	

	6073
	The order %s1 cannot be matched. Some of the orders of the counterparty are being processed (probably with a request for cancellation).
	E
	*
	
	
	

	6074
	Missing parameter: Submit a product.
	E
	*
	*
	*
	

	6075
	Market depth for product %s has been changed.
	I
	
	
	
	When the product detail has been changed.

	6076
	The cancellation of a set of orders was completed successfully.
	I
	
	*
	
	

	6078
	The cancellation of all orders according to the product %s was completed successfully.
	I
	
	*
	
	

	6079
	While processing the incident on the BM with a code %s1 type %s2 and error was found. 
	E
	*
	*
	*
	

	6080
	The product %s1 has NOT been issued on BM.
	I
	
	
	
	

	6086
	The product %s is outside of the trading period, when no instruction for cancellation may be processed.
	
	
	
	
	

	6087
	There were no active orders found for the given product.
	E
	
	*
	*
	

	6089
	The cancellation of all orders may not be executed during the period of submitting orders by the market maker. 
	E
	
	*
	
	

	6090
	The cancellation of set of orders may not be executed during the period of submitting orders by the market maker.
	E
	
	*
	
	

	6091
	The order %s1 was entered as invalid. The limit price %s2 is not in accordance with the defined price step of the product %s3. 


	E
	*
	
	
	

	6092
	Error in the order detail: the number of decimal places of the limit price of the order exceeded the technological limit.
	E
	*
	
	
	

	6094
	Order %s1 can't be cancelled. The order is not active yet.
	E
	
	*
	
	

	6095
	The modification of the order was finished with an error: %s.
	E
	*
	*
	
	

	6096
	The modification of the order was finished successfully.
	I
	*
	*
	
	

	6097
	The modification of the order %s1 was not executed due to trading. 
	E
	*
	*
	
	


Errors on the RRD:

	 
	 
	
	 
	Control level
	ACK report
	 
	 

	ID
	Description
	Type
	Code acc. to  ETSO
	Error  LEVEL
	Rejection of the whole message
	Rejection of the time series
	Anomaly report
	Confirmation report

	2200
	Guarantee limits have not been met.
	E
	Z20
	TS
	 
	x
	 x
	 

	2261
	Meets guarantee: Guarantee limits are almost used up.
	W
	Z21
	TS
	 
	
	 
	 x

	3015
	The user does not have the required permission to realize this operation.
	E
	Z04
	 
	x
	 
	 
	 

	3034
	In or Out party %s1 without valid contract to access RRD (from %s2 to %s3).
	E
	Z03
	 
	x
	 
	 
	 

	3800
	In or Out party %s1 is not a subject of settlement and there is no relation to any party responsible for its imbalances.
	E
	Z01
	DOC
	x
	 
	 
	 

	3801
	RRD not allowed by balance responsible party for In or Out party %s1.
	E
	Z02
	DOC
	x
	 
	 
	 

	3802
	Only TSO is accepted as a sender of the external schedule.
	E
	A78 
	DOC
	x
	 
	 
	 

	3808
	A subject party is to be either In party or Out party.
	E
	Z08
	TS
	x
	 
	 
	 

	3809
	A sender of zeroing schedule is to be the same in the being zeroed schedule.
	E
	Z09
	TS
	 
	x
	 
	 

	3810
	There is no schedule to be cancelled. Zeroing schedule has been rejected.
	E
	Z10
	TS
	 
	x
	 
	 

	3811
	Mandatory attributes missing.
	E
	A69
	ALL
	x
	 
	 
	 

	3812
	GCT for receiving schedule messages is not open yet or has

passed. Message rejected.
	E
	A57
	DOC
	x
	 
	 
	 

	3813
	The time interval is to be within one delivery day only.
	E
	A04
	DOC
	x
	 
	 
	 

	3814
	A period time interval is not the same as schedule interval.
	E
	A04
	DOC
	x
	 
	 
	 

	3815
	At least one time series version is to be equal to document version.
	E


	A50
	TS
	x
	 
	 
	 

	3816
	Superior TS version to document version is not allowed. 
	E
	A50
	TS
	x
	 
	 
	 

	3817
	The end of matching period interval is to be the same as of schedule interval.
	E
	A81
	DOC
	x
	 
	 
	 

	3818
	The matching period interval is out of the range of the schedule interval.
	E
	A81
	DOC
	x
	 
	 
	 

	3819
	The matching period interval is to be shorted with each sequent intraday schedule.
	E
	A81
	DOC
	x
	 
	 
	 

	3820
	A schedule receiver is to be Czech imbalance settlement responsible party. (OTE, a.s.)
	E
	A53
	DOC
	x
	 
	 
	 

	3821
	Message identification is already in the system.
	E
	A51
	DOC
	x
	 
	 
	 

	3822
	Schedule accepted.
	I
	A06
	DOC
	
	
	
	x

	3823
	Schedule partially accepted.
	I
	A07
	DOC
	
	
	
	x

	3825
	Time series not matching.
	E
	A09
	TS
	 
	 
	x
	 

	3826
	The area is unknown or not allowed.
	E
	A23
	TS
	 
	x
	 
	 

	3827
	Counterpart time series missing
	E
	A28
	TS
	 
	 
	x
	x

	3828
	Quantity difference between TSs with the same version number is not allowed.
	E
	A42
	INT
	 
	x
	 
	 

	3829
	Signed values are not allowed.
	E
	A46
	INT
	 
	x
	 
	 

	3830
	A position is missing or too many.
	E
	A49
	INT
	 
	x
	 
	 

	3831
	The schedule message is already in the system but with different identification.
	E
	A51
	DOC
	x
	 
	 
	 

	3832
	A time series is not contained in a new version of the message. Message rejected.
	E
	A52
	DOC
	x
	 
	 
	 

	3833
	The identification of the time series is duplicated or incorrect. Time series will be rejected.
	E
	A55
	TS
	x
	x
	 
	 

	3834
	The time series has been successfully matched.
	I
	A88
	TS
	 
	 
	 
	x

	3835
	Message partially rejected.
	W
	A03
	DOC
	 
	 
	 
	 

	3836
	Message fully rejected.
	E
	A02
	DOC
	x
	 
	 
	 

	3837
	Message fully accepted.
	I
	A01
	DOC
	 
	 
	 
	 

	3838
	Not permitted number of digits before/after the decimal point.
	E
	A42
	TS
	 
	x
	 
	 

	3839
	Process type invalid.
	E
	A79
	DOC
	x
	 
	 
	 

	3840
	Classification type invalid.
	E
	Z14
	DOC
	x
	 
	 
	 

	3841
	Sender role invalid.
	E
	A78 
	DOC
	x
	 
	 
	 

	3842
	Receiver role is invalid.
	E
	Z13
	DOC
	x
	 
	 
	 

	3843
	Domain invalid.
	E
	A80
	DOC
	x
	 
	 
	 

	3844
	Subject role invalid.
	E
	Z15
	DOC
	x
	 
	 
	 

	3845
	Invalid business type.
	E
	A62
	TS
	x
	 
	 
	 

	3846
	Invalid product.
	E
	Z16
	TS
	x
	 
	 
	 

	3847
	Invalid object aggregation.
	E
	Z17
	TS
	x
	 
	 
	 

	3848
	Unexpected measurement unit.
	E
	Z18
	TS
	x
	 
	 
	 

	3849
	Not supported resolution.
	E
	A41
	PER
	 
	x
	 
	 

	3850
	Invalid/not supported coding scheme.
	E
	Z19
	DOC
	x
	x
	 
	 

	3851
	Time series fully rejected.
	E
	A20
	TS
	 
	x
	 
	 

	3852
	Time series accepted with specific time interval errors.
	W
	A21
	TS
	 
	 
	 
	 

	3853
	Counterpart time series quantity differences.
	E
	A29
	TS
	 
	 
	x
	 

	3854
	Other anomaly.
	E
	Z22
	TS
	 
	 
	x
	 

	3855
	The zeroed time series has been ignored and not matched since it does not figure in a counterparty transmission. All are correctly equal to zero.
	E
	A94
	DOC
	x
	 
	 
	 

	3856
	Document cannot be processed by receiving system.
	E
	A89
	DOC
	x
	 
	 
	 

	3861
	Invalid In Area.
	E
	A23
	TS
	
	x
	
	

	3862
	Invalid Out Area.
	E
	A23
	TS
	
	x
	
	

	3863
	RD volume is out of specified minimum and maximum value.
	E
	A42
	TS
	
	x
	
	

	3864
	In/Out party cannot be the Exchange or TSO in case of internal daily RD not sent by Exchange.
	E
	A22
	TS
	x
	
	
	

	3865
	In and Out party have to be different in one RD
	E
	A22
	TS
	x
	
	
	

	3866
	An invalid request (ESR ) data -  duplicity or no document found
	E
	Z05
	ESR
	x
	
	
	

	3867
	Within one schedule document only position with one counterparty is allowed.
	E
	Z06
	DOC
	x
	
	
	

	3899
	The same pair of in/out party is not allowed in more than one time series within one schedule document.
	E
	A22
	TS
	x
	
	
	

	3902
	A counterparty of schedules sent by PXE is to be dedicated PXE's subject of settlement.
	E
	A22
	TS
	x
	
	
	

	3903
	A sender of daily internal schedule is to be equal to subject party.
	E
	A78
	TS
	x
	
	
	

	3904
	A sender of schedule doesn't correspond to the participant providing data.
	E
	A78
	TS
	x
	
	
	

	3909
	Schedule has been accepted and is waiting for FS calculation.
	E
	Z23
	TS
	
	
	x
	

	3932
	Same identification of the time series for another In/Out party. Use another one.
	E
	A55
	TS
	x
	x
	
	


Errors in the field of settlement:

	Notification
	Used in:
	Notes

	ID
	Description
	Type
	Definition Implementation
	Confirmation/Rejection of definition 
	Submitting/Replacing of realizations 
	Confirmation/Rejection of realization 
	Cancellation of realization
	Removal of definition
	Enquiries
	

	4043
	No data was found in the processing table.
	E
	*
	*
	*
	*
	*
	*
	*
	

	4051
	Invalid operation type.
	E
	*
	*
	*
	*
	*
	*
	*
	

	5011
	Error while calling the API function. Error code = %s. 
	E
	*
	*
	*
	*
	*
	*
	*
	

	5504
	Enquiry completed. Data was found. 
	I
	
	
	
	
	
	
	*
	

	5505
	Enquiry completed. No data was found.
	I
	
	
	
	
	
	
	*
	

	5529
	Error in header: invalid market type.
	E
	
	
	
	
	
	
	*
	

	999
	Enquiry with ID %id is not completed or does not exit..
	I
	
	
	
	
	
	
	
	Only for msg_code 922

	998
	The sender does not match the certificate.
	E
	
	
	
	
	
	
	
	Only for msg_code 922

	997
	The enquiry was received for processing.
	I
	
	
	
	
	
	
	
	

	 
	Successful completion of the requested action by one of the participants.
	
	
	
	
	
	
	
	
	

	 
	Invitation (informative character)
	
	
	
	
	
	
	
	
	

	 
	Successful completion of the requested action by the energy exchange.
	
	
	
	
	
	
	
	
	


5 COMMAND STRUCTURE overview 

XML format interpretation:

	
	Item
	XML location
	Size
	Values/Type

	
	1
	<ISOTEDATA message-code="851">
	3
	Integer

	
	2
	<ISOTEDATA/SenderIdentification id="8591824019999">

<ISOTEDATA/Trade/Party id="8591824019999" role="TO"> - u výstupních zpráv CDS
	13
	<1;9999999999999>; Integer

	
	3
	<ISOTEDATA/Trade trade-day="2004-03-19">
	10
	Varchar

	
	4
	<ISOTEDATA/Trade trade-type="P">
	1
	Char

	
	5
	<ISOTEDATA/Trade trade-order="1">
	10
	<1;9999999999>; Integer

	
	6
	<ISOTEDATA/Trade/TimeData datetime="2004-03-19T15:24" datetime-type="DTR">
	16
	Varchar

	
	7
	<ISOTEDATA/Trade/TimeData timeattribute="L" datetime-type="DTR">
	1
	Char

	
	8
	<ISOTEDATA/Trade acceptance="N">
	1
	Char

	
	9
	<ISOTEDATA/Trade/Comment>Comment<Comment>
	100
	Varchar

	
	10
	<ISOTEDATA/Trade/TimeData datetime="2004-03-19T15:24:37" datetime-type="DTA">
	19
	Varchar

	
	11
	<ISOTEDATA/Trade id="555">
	10
	<1;9999999999>; Integer

	
	12
	<ISOTEDATA/Trade version="0">
	5
	<0;99999>; Integer

	
	13
	<ISOTEDATA/Trade replacement="N">
	1
	Char

	
	14
	<ISOTEDATA/Trade trade-state="A">
	1
	Char 

	
	15
	<ISOTEDATA/Trade/TimeData datetime="2004-03-19T15:24:18" datetime-type="DTC">
	19
	Varchar

	
	16
	<ISOTEDATA/Trade error-code="5000">
	4
	0;<1000;9999>; Integer

	
	17
	<ISOTEDATA err-reaction ="A">
	1
	Char

	
	18
	<ISOTEDATA/Trade market="VDT">
	3
	Varchar

	
	19
	<ISOTEDATA/Trade short-description="Descr.">
	8
	Varchar

	
	20
	<ISOTEDATA/Trade/Party id="8591824000007" role="TOS">
	13
	<1;9999999999999>; Integer

	
	21
	<ISOTEDATA/Trade/Party id="8591824000007" role="TOB">
	13
	<1;9999999999999>; Integer

	
	22
	<ISOTEDATA/Trade/Party id="8591824000007" role="TOR">
	13
	<1;9999999999999>; Integer

	
	23
	<ISOTEDATA trade-stage ="P">
	1
	Char

	
	24
	<ISOTEDATA trade-flag ="N">
	1
	Char

	
	25
	<ISOTEDATA anulation-proposer ="N">
	1
	Char

	
	26
	<ISOTEDATA id-definition ="N">
	10
	<1;9999999999>; Integer

	
	27
	<ISOTEDATA trade-day-to ="2004-03-25">
	10
	Varchar

	
	28
	<ISOTEDATA anulation-type ="0">
	2
	<0;99>; Integer

	
	1
	<ISOTEDATA/Trade/ProfileData profile-role="C71(2)"/Data period="17">
	2
	<1;25>; Integer

	
	2
	<ISOTEDATA/Trade/ProfileData profile-role="C71(2)"/Data value="10,5">
	16,4
	<-9999999999999999.9999; 9999999999999999.9999>; Float

	
	3
	<ISOTEDATA/Trade/ProfileData profile-role="P71(2)"/Data value="899">
	16,4
	<-9999999999999999.9999; 9999999999999999.9999>; Float

	
	4
	<ISOTEDATA/Trade/ProfileData profile-role="C71(2)"/Data splitting="A">
	1
	Char

	
	5
	<ISOTEDATA/Trade/ProfileData profile-role="C73(4)"/Data value="899">
	5,1
	<0;99999.9>; Float

	
	6
	<ISOTEDATA/Trade/ProfileData profile-role="C75(76)"/Data value="899">
	5,1
	<0;99999.9>; Float

	
	7
	<ISOTEDATA/Trade/ProfileData profile-role="T11"/Data value="2004-03-18T16:00:00">
	19
	Varchar

	
	8
	<ISOTEDATA/Trade/ProfileData profile-role="T11"/Data timeattribute="Z">
	1
	Char

	
	9
	<ISOTEDATA/Trade/ProfileData profile-role="T12"/Data value="2004-03-18T16:00:00">
	19
	Varchar

	
	10
	<ISOTEDATA/Trade/ProfileData profile-role="T12"/Data timeattribute="Z">
	1
	Char

	
	11
	<ISOTEDATA/Trade/ProfileData profile-role="T11(2)"/Data perflag-cancel="N">
	1
	Char

	
	12
	<ISOTEDATA/Trade/ProfileData profile-role="T11(2)"/Data perflag-aggregation="N">
	1
	Char

	
	13
	<ISOTEDATA/Trade/ProfileData profile-role="ST13"/Data anulation-proposer ="N">
	1
	Char

	
	14
	<ISOTEDATA/Trade/ProfileData profile-role="ST13">
	4
	Char


Note: for support of compatibility with CDS OTE system it is necessary to indicate the attribute unit for the element ISOTEDATA/Trade/ProfileData/Data with the denotation „Volume relative unit”. There are following restrictions applied to the attribute unit: MWH (for energy values), CZK or EUR (for prices and payment amounts).

5.1 IM&BalM Commands

5.1.1 Command structure overview – ISOTEDATA

	L.I.
	IM&BalM description 
	XML location (ISOTEDATA)
	Size
	Values/Type
	Bid Entry / Replacement 
	Bid cancellation
	Bid acceptance 
	Bid data transcript (entry, cancellation, acceptance, own bid data)
	Notice board data - bid data transcript
	Trade hour status - Trade hour data transcript
	Market result - Market result data transcript
	Notice board data - bid data transcript at distribution of changes

	1
	Message code
	<ISOTEDATA/@message_code>
	3
	Integer
	851
	861
	871
	853, 863, 873, 883, 886
	893
	913
	903
	933

	2
	Participant (EAN)
	ISOTEDATA/Trade/Party/@id
ISOTEDATA/Trade/Party/@role="TO"

eg: <Party id="1291824000077" role="TO"/>
	13
	<1;9999999999999>; Integer
	 
	 
	 
	 
	 
	 
	 
	 

	3
	Delivery day (YYYY-MM-DD)
	<ISOTEDATA/Trade/@trade-day>
	10
	Varchar
	 
	 
	 
	 
	 
	 
	 
	 

	4
	Bid type (N - buy, P - sell)
	ISOTEDATA/Trade/@trade-type
	1
	Char
	 
	 
	 
	 
	 
	 
	 
	 

	5
	Bid order
	ISOTEDATA/Trade/@trade-order
	10
	<1;9999999999>; Integer
	 
	 
	 
	 
	 
	 
	 
	 

	6
	Bid withdrawal time (YYYY-MM-DDThh:mm)
	<ISOTEDATA/Trade/TimeData datetime="2004-03-19T15:24" datetime-type="DTR">
	16
	Varchar
	 
	 
	 
	 
	 
	 
	 
	 

	7
	Bid withdrawal time -attribute (Z-winter, L-summer)
	ISOTEDATA/Trade/TimeData/@timeattribute
	1
	Char
	 
	 
	 
	 
	 
	 
	 
	 

	8
	Total bid aceptance (A - yes, N - no)
	ISOTEDATA/Trade/@acceptance
	1
	Char
	 
	 
	 
	 
	 
	 
	 
	 

	9
	Comment
	ISOTEDATA/Trade/Comment
	100
	Varchar
	 
	 
	 
	 
	 
	 
	 
	 

	10
	Bid cancellation time (YYYY-MM-DDThh:mm:ss)
	<ISOTEDATA/Trade/TimeData datetime="2004-03-19T15:24:37" datetime-type="DTA">
	19
	Varchar
	 
	 
	 
	 
	 
	 
	 
	 

	11
	Bid ID 
	<ISOTEDATA/Trade id="555">
	10
	<1;9999999999>; Integer
	 
	 
	 
	 
	 
	 
	 
	 

	12
	Bid version
	ISOTEDATA/Trade/@version
	5
	<0;99999>; Integer
	 
	 
	 
	 
	 
	 
	 
	 

	13
	Bid replacement attribute (A - replaced, N – not replaced)
	<ISOTEDATA/Trade replacement="A">
	1
	Char
	 
	 
	 
	 
	 
	 
	 
	 

	14
	Bid origin (A - acceptance, N - bid)
	<ISOTEDATA/Trade trade-state="A">
	1
	Char 
	 
	 
	 
	 
	 
	 
	 
	 

	15
	Bid entry time (YYYY-MM-DDThh:mm:ss)
	<ISOTEDATA/Trade/TimeData datetime="2004-03-19T15:24:32" datetime-type="DTC">
	19
	Varchar
	 
	 
	 
	 
	 
	 
	 
	 

	16
	Error code
	ISOTEDATA/Trade/@error-code
	4
	0;<1000;9999>; Integer
	 
	 
	 
	 
	 
	 
	 
	 

	17
	Error reaction (A – apply changes only error-free bids, N – cancel all changes if error occurred)
	ISOTEDATA/@err-reaction
	1
	Char
	 
	 
	 
	 
	 
	 
	 
	 

	18
	Market type (VDT – Intraday Market, VT – Balancing Market)
	ISOTEDATA/Trade/@market
	3
	Varchar
	 
	 
	 
	 
	 
	 
	 
	 

	19
	Participant (EAN) – counterparty
	ISOTEDATA/Trade/Party/@id
	13
	<1;9999999999999>; Integer
	 
	 
	 
	 
	 
	 
	 
	 

	20
	Settlement version (2 - Daily Imbalance Settlement, 3 - Interim Monthly Settlement, 4 - Final Monthly Settlement)
	ISOTEDATA/Trade/@version
	1
	<2;4>; Integer
	 
	 
	 
	 
	 
	 
	 
	 

	1
	Hour (period)
	ISOTEDATA/Trade/ProfileData/Data/@period
	2
	<1;25>; Integer
	 
	 
	 
	 
	 
	 
	 
	 

	2
	Volume
	ISOTEDATA/Trade/ProfileData/Data/@value
	16,4
	<-9999999999999999.9999; 9999999999999999.9999>; Float
	 
	 
	 
	 
	 
	 
	 
	 

	3
	Price
	ISOTEDATA/Trade/ProfileData/Data/@value
	16,4
	<-9999999999999999.9999; 9999999999999999.9999>; Float
	 
	 
	 
	 
	 
	 
	 
	 

	4
	Volume divisibility (A-yes, N-no)
	ISOTEDATA/Trade/ProfileData/Data/@splitting
	1
	Char
	 
	 
	 
	 
	 
	 
	 
	 

	5
	IM accepted 
	ISOTEDATA/Trade/ProfileData/@profile-role=C73 || C74
	5,1
	<0;99999.9>; Float
	 
	 
	 
	 
	 
	 
	 
	 

	6
	BalM accepted
	ISOTEDATA/Trade/ProfileData/@profile-role=C75 || C76
	5,1
	<0;99999.9>; Float
	 
	 
	 
	 
	 
	 
	 
	 

	7
	Open from (YYYY-MM-DDThh:mm:ss)
	ISOTEDATA/Trade/ProfileData/@profile-role=T11 … ProfileData/Data/@value='2009-01-01' @unit='date'
	19
	Varchar
	 
	 
	 
	 
	 
	 
	 
	 

	8
	Open from – attribute (Z - winter, L - summer)
	ISOTEDATA/Trade/ProfileData/Data/@timeattribute
	1
	Char
	 
	 
	 
	 
	 
	 
	 
	 

	9
	Closed from (YYYY-MM-DDThh:mm:ss)
	ISOTEDATA/Trade/ProfileData/@profile-role=T12 … ProfileData/Data/@value='2009-01-01' @unit='date'
	19
	Varchar
	 
	 
	 
	 
	 
	 
	 
	 

	10
	Closed from – attribute (Z - winter, L - summer)
	ISOTEDATA/Trade/ProfileData/Data/@timeattribute
	1
	Char
	 
	 
	 
	 
	 
	 
	 
	 

	11
	Cancelled (A-yes, N-no)
	ISOTEDATA/Trade/ProfileData/Data/@perflag-cancel
	1
	Char
	 
	 
	 
	 
	 
	 
	 
	 

	12
	Aggregated (A-yes, N-no)
	ISOTEDATA/Trade/ProfileData/Data/@perflag-aggregation
	1
	Char
	 
	 
	 
	 
	 
	 
	 
	 

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	Mandatory field
	
	
	
	
	
	
	
	
	
	
	


5.1.2 Requirement structure overview – ISOTEREQ

	 
	Description
	XML location
	Size
	Value/Type
	Own bid data (status determination) 
	Resultant prices BalM
	Notice board data
	Trade hour status
	Market result

	1
	Message code
	ISOTEREQ/@message-code
	3
	Integer
	881
	884
	891
	911
	901

	2
	Delivery day
	ISOTEREQ/Trade/@trade-day
	10
	Varchar
	 
	 
	 
	 
	 

	3
	Bid type
	ISOTEREQ/Trade/@trade-type
	1
	N, P (N - buy, P - sell); Char
	 
	 
	 
	 
	 

	4
	Bid ID 
	ISOTEREQ/Trade@id
	10
	<1;9999999999>; Integer
	 
	 
	 
	 
	 

	5
	Bid version
	ISOTEREQ/Trade/@version
	5
	<0;99999>; Integer
	 
	 
	 
	 
	 

	6
	Bid origin
	ISOTEREQ/Trade/@trade-state
	1
	A, N (A - acceptance, N - bid); Char
	 
	 
	 
	 
	 

	7
	Market type
	ISOTEREQ/Document/@market
	3
	VDT, VT (VDT - Intraday Market, VT – Balancing Market); Varchar
	 
	 
	 
	 
	 

	8
	Settlement version
	ISOTEREQ/Trade/@version-a
	1
	<2;4>; Integer
	 
	 
	 
	 
	 

	9
	Hour (period)
	ISOTEREQ/Trade/@period
	2
	<1;25>; Integer
	 
	 
	 
	 
	 

	
	
	
	
	
	
	
	
	
	

	 
	Mandatory field
	
	
	
	
	
	
	
	


5.2 DM Commands

5.2.1 Command structure overview  – ISOTEDATA

	L.I.
	DM description
	XML location (ISOTEDATA)
	Size
	Value/Type
	Bid Entry / Replacement
	Bid cancellation 
	Bid data transcript (entry, cancellation, own bid data)

	1
	Message code
	<ISOTEDATA/@message_code>
	3
	Integer
	811
	821
	813, 823, 833

	2
	Participant (EAN) – bid creator ID, EIC – SK bid
	ISOTEDATA/Trade/Party/@id
ISOTEDATA/Trade/Party/@role="TO"

eg: <Party id="1291824000077" role="TO"/>
	16
	Varchar
	 
	 
	 

	3
	Delivery day (YYYY-MM-DD)
	<ISOTEDATA/Trade/@trade-day>
	10
	Varchar
	 
	 
	 

	4
	Bid type (N - buy, P -sell)
	ISOTEDATA/Trade/@trade-type
	1
	Char
	 
	 
	 

	5
	Block 1 total acceptance (A-yes, N-no)
	ISOTEDATA/Trade/@acceptance
	1
	Char
	 
	 
	 

	6
	Comment
	ISOTEDATA/Trade/Comment
	30
	Varchar
	 
	 
	 

	7
	Bid cancellation time  (YYYY-MM-DDThh:mm:ss)
	<ISOTEDATA/Trade/TimeData datetime="2004-03-19T15:24:35" datetime-type="DTA">
	19
	Varchar
	 
	 
	 

	8
	Bid ID 
	<ISOTEDATA/Trade id="555">
	10
	<1;9999999999>; Integer
	 
	 
	 

	9
	Bid version
	ISOTEDATA/Trade/@version
	5
	<0;99999>; Integer
	 
	 
	 

	
	
	
	
	
	
	
	

	10
	Bid replacement attribute (A - replaced, N - not replaced)
	<ISOTEDATA/Trade replacement="A">
	1
	Char
	 
	 
	 

	11
	Default bid attribute (A - default, N – non-default)
	<ISOTEDATA/Trade trade-state="A">
	1
	Char 
	 
	 
	 

	12
	Bid entry time (YYYY-MM-DDThh:mm:ss)
	<ISOTEDATA/Trade/TimeData datetime="2004-03-19T15:24:35" datetime-type="DTC">
	19
	Varchar
	 
	 
	 

	13
	Error code
	ISOTEDATA/Trade/@error-code
	4
	0;<1000;9999>; Integer
	 
	 
	 

	14
	Settlment currency code  (CZK, EUR)
	ISOTEDATA/Trade/@sett-curr
	3
	Char
	 
	 
	 

	15
	Data source (PXE, OTE)
	ISOTEDATA/Trade/@source-sys
	3
	Char
	 
	 
	 

	16
	Bid status (P – valid,  N – invalid)
	<ISOTEDATA trade-stage ="P">
	1
	Char
	 
	 
	 

	17
	Bid cancellation  attribute (N – not cancelled, A - cancelled)
	ISOTEDATA/Trade/@trade-flag
	1
	Char
	 
	 
	 

	18
	Trade Market Profile (SPT - spot, DER - derivative)
	ISOTEDATA/Trade/@trade-market-flag
	10
	Varchar
	 
	 
	 

	1
	Hour (period)
	ISOTEDATA/Trade/ProfileData/Data/@period
	2
	<1;25>; Integer
	 
	 
	 

	2
	Volume
	ISOTEDATA/Trade/ProfileData/Data/@value
	16,4
	<-9999999999999999.9999; 9999999999999999.9999>; Float
	 
	 
	 

	
	
	(if <ProfileData profile-role="BC##">)
	
	
	
	
	

	3
	Price ( in case of DER bids the price may not be set) 
	ISOTEDATA/Trade/ProfileData/Data/@value
	16,4
	<-9999999999999999.9999; 9999999999999999.9999>; Float
	 
	 
	 

	
	
	(if <ProfileData profile-role="BP##">)
	
	
	 
	
	

	4
	Block 1 volume divisibility (A-yes, N-no)
	ISOTEDATA/Trade/ProfileData/Data/@splitting
	1
	Char
	 
	 
	 

	5
	Bid block  ID
	ISOTEDATA/Trade/ProfileData/@profile-role
	4
	Char
	 
	 
	 

	
	
	(Value: BC01-25, BP01-25)
	
	
	
	
	

	
	
	
	
	
	
	
	

	 
	Mandatory field
	
	
	
	
	
	


5.2.2 Requirement structure overview – ISOTEREQ

	L.I.
	DM description
	XML location
	Size
	Value/Type
	Own bid data (status determining) 

	1
	Message code
	ISOTEREQ/@message-code
	3
	Integer
	831

	2
	Delivery day (YYYY-MM-DD)
	ISOTEREQ/Trade/@trade-day
	10
	Varchar
	 

	3
	Bid ID
	ISOTEREQ/Trade/@id
	10
	<1;9999999999>; Integer
	 

	4
	Bid version
	ISOTEREQ/Trade/@version
	5
	<0;99999>; Integer
	 

	5
	Trade Market Profile (SPT - spot, DER - derivative)
	ISOTEDATA/Trade/@trade-market-flag
	10
	Varchar
	 

	
	
	
	
	
	

	
	Mandatory field
	
	
	
	


5.3 BM Commands

5.3.1 Command structure overview  – ISOTEDATA

	L.I.
	BM description - order
	BM description - trade
	BM description – trading screen
	XML location (ISOTEDATA)
	Size
	Value/Type
	Order entry
	Order cancellation
	Order data
transcript (entry, cancellation,
own order data)
	Trading screen data  - order data transcript
	Own trade data transcript

	1
	Message code
	Message code
	Message code
	<ISOTEDATA/@message-code>
	3
	Integer
	854
	857
	856, 859, 866
	869
	876

	2
	Participant (EAN) – order creator ID
	 
	 
	ISOTEDATA/Trade/Party/@id
ISOTEDATA/Trade/Party/@role="TO"

eg: <Party id="1291824000077" role="TO"/>
	13
	<1;9999999999999>; Integer
	 
	 
	 
	 
	 

	3
	Order type (N - buy, P -sell)
	Trade type (N - buy, P -sell)
	 
	<ISOTEDATA/Trade trade-type="P">
	1
	Char
	 
	 
	 
	 
	 

	4
	Product (instance) title
	Product (instance) title
	Product (instance) title
	<ISOTEDATA/Trade/Comment>DB080120<Comment>
	30
	Varchar
	 
	 
	 
	 
	 

	5
	Order cancellation time (YYYY-MM-DDThh:mm:ss)
	 
	 
	<ISOTEDATA/Trade/TimeData datetime="2004-03-19T15:24:35" datetime-type="DTA">
	19
	Varchar
	 
	 
	 
	 
	 

	6
	Order code
	Order code
	 
	<ISOTEDATA/Trade id="555">
	10
	<1;9999999999>; Integer
	 
	 
	 
	 
	 

	7
	Automatic cancellation attribute (A- automatically cancelled, U- cancelled by user, not indicated, if not cancelled)
	 
	 
	<ISOTEDATA/Trade replacement="A">
	1
	Char
	 
	 
	 
	 
	 

	8
	Order attribute – mode (T – market maker mode, not indicated for standard mode)
	 
	 
	<ISOTEDATA/Trade trade-state="T">
	1
	Char 
	 
	 
	 
	 
	 

	9
	Order entry time (YYYY-MM-DDThh:mm:ss)
	Trade creation time (YYYY-MM-DDThh:mm:ss)
	 
	<ISOTEDATA/Trade/TimeData datetime="2004-03-19T15:24:35" datetime-type="DTC">
	19
	Varchar
	 
	 
	 
	 
	 

	10
	Trading type related to the order (A - auction, K - continual, AK - auction and continual)
	 
	 
	<ISOTEDATA/Trade market="K">
	3
	Varchar
	 
	 
	 
	 
	 

	11
	Order status/stage (P - valid, N - invalid)
	 
	 
	<ISOTEDATA trade-stage ="P">
	1
	Char
	 
	 
	 
	 
	 

	12
	 
	Trade code
	 
	<ISOTEDATA id-definition ="1234">
	10
	<1;9999999999>; Integer
	 
	 
	 
	 
	 

	1
	 
	Order index (1 – trade price and number of contracts, 2 – total price amount and traded volume)
	Order index (1 to 5 – top 5 orders to buy, 6 to 10 – top 5 orders to sell, 11 – day statistics, 12 – product (instance) statistics)
	<ISOTEDATA/Trade/ProfileData profile-role="SC48"/Data period="1">
	2
	<1;25>; Integer
	 
	 
	 
	 
	 

	2
	 
	Traded volume [MWh]
	Final price (for 1-10), Bottom price (for11 and 12)
	<ISOTEDATA/Trade/ProfileData profile-role="SC48"/Data value="10">
	16,4
	<-9999999999999999.9999; 9999999999999999.9999>; Float
	 
	 
	 
	 
	 

	3
	Limit price
	Trade price/Total price amount
	Limit price (for 1-10), Ceiling price (for 11 and 12)
	<ISOTEDATA/Trade/ProfileData profile-role="SP46"/Data value="899">
	16,4
	<-9999999999999999.9999; 9999999999999999.9999>; Float
	 
	 
	 
	 
	 

	4
	Number of contracts
	 
	Number of contracts
	<ISOTEDATA/Trade/ProfileData profile-role="SC46"/Data value="10">
	5,1
	<0;999999>; Float
	 
	 
	 
	 
	 

	5
	Number of traded contracts
	Number of traded contracts
	 
	<ISOTEDATA/Trade/ProfileData profile-role="SC42"/Data value="10">
	5,1
	<0;999999>; Float
	 
	 
	 
	 
	 

	
	
	
	
	
	
	
	
	
	
	
	

	
	Mandatory field
	
	
	
	
	
	
	
	
	
	


5.3.2 Requirement structure overview – ISOTEREQ

	L.I.
	Description BM
	XML location
	Size
	Value/Type
	Own order data
	Trading screen data request - market depth (not settled, reserved for future use)
	Trade request (own)

	1
	Message code
	/ISOTEREQ/@message-code
	3
	Integer
	864
	867
	874

	2
	Product (instance) title
	/ISOTEREQ/Trade/@product
	30
	Varchar
	 
	 
	 

	3
	Order code
	/ISOTEREQ/Trade/@id
	10
	<1;9999999999>; Integer
	 
	 
	 

	4
	Order entry time/trade creation time (in format: YYYY-MM-DDThh:mm:ss)
	/ISOTEREQ/Trade/@trade-day
	19
	Varchar
	 
	 
	 

	5
	Trade code
	/ISOTEREQ/Trade/@id
	10
	<1;9999999999>; Integer
	 
	 
	 

	
	
	
	
	
	
	
	

	
	Mandatory field
	
	
	
	
	
	


5.4 BM Instances

5.4.1 Command structure overview  – ISOTEMASTERDATA

	 
	Block market automatic communication interface
	Instance description

	
	Data message  ISOTEMASTERDATA 
	

	
	L.I.
	BM description - trade
	XML location (ISOTEDATA)
	Size
	Value/Type
	

	One record only
	Instance
	1
	Message code
	<ISOTEDATA/@message_code>
	3
	Integer
	879

	
	
	2
	Instance
	<ISOTEMASTERDATA / Instance instance-id = "DB081010">
	30
	Varchar
	 

	
	
	3
	Long instance title
	<ISOTEMASTERDATA / Instance instance-description = "CZ Daily baseload 2008-10-10">
	255
	Varchar
	 

	
	
	4
	Instance class (D - Daily)
	<ISOTEMASTERDATA / Instance instance-class="BMD">
	3
	Varchar
	 

	
	
	5
	Block type  (P - Peak, O-Offpeak, B-Base)
	<ISOTEMASTERDATA / Instance instance-type="PDB">
	10
	Varchar
	 

	
	
	6
	Instance location
	<ISOTEMASTERDATA / Instance location="CZ-ETS">
	30
	Varchar
	 

	
	
	7
	Instance contract unit
	<ISOTEMASTERDATA / Instance unit = "MWH">
	5
	Varchar
	 

	
	
	8
	Instance currency unit
	<ISOTEMASTERDATA / Instance currency = "CZK">
	3
	Varchar
	 

	
	
	9
	Settlement type (PS - actual delivery)
	<ISOTEMASTERDATA / Instance processing-type="PS">
	3
	Varchar
	 

	
	General characteristic
	10
	Contract volume [contract unit]
	<ISOTEMASTERDATA / Instance / Characteristic  charact-role = "Q_BM001" value-qty="1" unit="MWH">
	3,1
	<0,1;999> Float
	 

	
	
	11
	Minimum supply volume [MWh]
	<ISOTEMASTERDATA / Instance / Characteristic  charact-role = "Q_BM002" value-qty="24" unit="MWH">
	3,1
	<0,1;999> Float
	 

	
	
	12
	Initial delivery day (YYYY-MM-DD)
	<ISOTEMASTERDATA / Instance / Characteristic  charact-role = "D_BM001" value-date="2008-10-10">
	10
	Varchar
	 

	
	
	13
	Final delivery day (YYYY-MM-DD)
	<ISOTEMASTERDATA / Instance / Characteristic  charact-role = "D_BM002" value-date="2008-10-10">
	10
	Varchar
	 

	1 up to n records
	Delivery interval
	1
	Order index 
	<ISOTEMASTERDATA / Instance / Interval interval-role="CDI" order-index="1" interval-date="2008-10-10" period-from="1" period-to="8"/>
	2
	<1;25>; Integer
	 

	
	
	2
	Supply interval (YYYY-MM-DD)
	<ISOTEMASTERDATA / Instance / Interval interval-role="CDI" order-index="1" interval-date="2008-10-10" period-from="1" period-to="8"/>
	10
	Varchar
	 

	
	
	3
	Supply interval – initial period
	<ISOTEMASTERDATA / Instance / Interval interval-role="CDI" order-index="1" interval-date="2008-10-10" period-from="1" period-to="8"/>
	2
	<1;25>; Integer
	 

	
	
	4
	Supply interval – final period
	<ISOTEMASTERDATA / Instance / Interval interval-role="CDI" order-index="1" interval-date="2008-10-10" period-from="1" period-to="8"/>
	2
	<1;25>; Integer
	 

	1 up to n records
	Life cycle events
	1
	Event title (N_ISSUE – notification: instance not released, ISSUE - notification: instance released, TRC_START_MM – continual trade open for market maker, TRC_START_SS - continual trade open  for subjects of settlement, TRC_CLOSE - continual trade close, AGGREG – data aggregation, PUBLICATION – data publishing)
	<ISOTEMASTERDATA / Instance / Interval interval-role="ISSUE" order-index="1" date-time-from="2008-10-05T10:00:00"/>
	20
	Varchar
	 

	
	
	2
	Time of event (YYYY-MM-DDThh:mm:ss)
	<ISOTEMASTERDATA / Instance / Interval interval-role="ISSUE" order-index="1" date-time-from="2008-10-05T10:00:00"/>
	19
	Varchar
	 


5.4.2 Requirement structure overview – ISOTEREQ

	Instance data request ISOTEREQ
	Instance data request

	
	

	Pol.
	BM description - trade
	XML location (ISOTEREQ)
	Size
	Value/Type
	

	1
	Message code
	/ISOTEREQ/@message-code
	3
	Integer
	877

	2
	Product
	/ISOTEREQ/Trade/@product
	30
	Varchar
	 


5.5 Settlement commands

5.5.1 Command structure overview  – ISOTEDATA

	L.I.
	Result description
	Message result description 939
	Size
	Value/Type
	XML location
	Data transcripts

	
	
	
	
	
	
	Data request - traded volume overall plan – Data transcript
	Data request - DM Marginal prices - Data transcript
	Data request - Hourly settlement - Data transcript
	Data request – Daily settlement - Data transcript
	Data request - Accepted bids on BalM - Data transcript
	Area DM results - Data transcript
	DM coordination results for SS - Data transcript
	Statistical data of imbalance settlement

	1
	Message code
	Message code
	3
	Integer
	<ISOTEDATA/@message-code>
	943
	946
	953
	963
	973
	936
	939
	966

	2
	Participant (EAN)
	Participant anonymous code / EIC
	16
	<1;9999999999999>; Integer
	ISOTEDATA/Trade/Party/@id
ISOTEDATA/Trade/Party/@role="TO"

Příklad: <Party id="1291824000077" role="TO"/>
	 
	 
	 
	 
	 
	 
	 
	 

	3
	Date (YYYY-MM-DD)
	Delivery day  (YYYY-MM-DD)
	10
	Varchar
	<ISOTEDATA/Trade trade-day="2004-03-19">
	 
	 
	 
	 
	 
	 
	 
	 

	4
	Bid type (N - buy, P -sell)
	Bid type (N - buy, P -sell)
	1
	Char
	<ISOTEDATA/Trade trade-type="P">
	 
	 
	 
	 
	 
	 
	 
	 

	5
	Matching ID
	 
	10
	<1;9999999999>; Integer
	<ISOTEDATA/Trade version-a="123">
	 
	 
	 
	 
	 
	 
	 
	 

	6
	LP change date (YYYY-MM-DD)
	 
	10
	Varchar
	<ISOTEDATA/Trade/TimeData datetime="2004-03-19T15:24:00" datetime-type="DTR">
	 
	 
	 
	 
	 
	 
	 
	 

	7
	 
	Bid matching attribute 
(A - matched, N – not matched)
	1
	Char
	<ISOTEDATA/Trade trade-stage="A">
	 
	 
	 
	 
	 
	 
	 
	 

	8
	Message code:
RC006
	Message code:
RC001, RC002
	5
	 
	<ISOTEDATA/Trade/ProcReason code="RC001">
	 
	 
	 
	 
	 
	 
	 
	 

	9
	Message text (only for message code  specification)
	Message text (only for message code  specification)
	512
	Varchar
	<ISOTEDATA/Trade/ProcReason code="RC001"> text </ProcReason>
	 
	 
	 
	 
	 
	 
	 
	 

	10
	 
	Bid ID
	10
	<1;9999999999>; Integer
	<ISOTEDATA/Trade id="555">
	 
	 
	 
	 
	 
	 
	 
	 

	11
	Settlement version: 1 - Daily DM Settlement, 2 - Daily Imbalance Settlement, 3 - Interim Monthly Settlement, 4 - Final Monthly Settlement, 5 – State of Emergency, 6 – Clearing LP
	Bid version
	5
	<0;99999>; Integer
	<ISOTEDATA/Trade version="0">
	 
	 
	 
	 
	 
	 
	 
	 

	12
	Market type (OKO - Day-ahead market, DVS - Registration of RD, VDT - Intraday market, BT - Block market)
	Area - market area, for which the bid was created (CZ, SK)
	3
	Varchar
	<ISOTEDATA/Trade market-area=“SK“>

/ISOTEDATA/Trade/@market
	 
	 
	 
	 
	 
	 
	 
	 

	1
	Hour (period)
	Hour (period)
	2
	<1;25>; Integer
	<ISOTEDATA/Trade/ProfileData/Data period="17">
	 
	 
	 
	 
	 
	 
	 
	 

	2
	Volume
	Matched volume
	16,4
	<-9999999999999999.9999; 9999999999999999.9999>; Float
	<ISOTEDATA/Trade/ProfileData profile-role="SC02"/Data value="10,5">
	 
	 
	 
	 
	 
	 
	 
	 

	3
	Price
	 
	16,4
	<-9999999999999999.9999; 9999999999999999.9999>; Float
	<ISOTEDATA/Trade/ProfileData profile-role=" SP02"/Data value="899">
	 
	 
	 
	 
	 
	 
	 
	 

	4
	Currency code (CZK, EUR)
	 
	3
	Char
	<ISOTEDATA/Trade/ProfileData Data unit="EUR">
	 
	 
	 
	 
	 
	 
	 
	 

	5
	Message code:
RC007, RC008, RC009
	Message code:
RC003, RC004, RC005
	32
	Varchar
	<ISOTEDATA / Trade / ProfileData / Data / ProcReason code="RC006">
	 
	 
	 
	 
	 
	 
	 
	 

	6
	Message text (only for message code  specification)
	Message text (only for message code  specification)
	512
	Varchar
	<ISOTEDATA / Trade / ProfileData / Data / ProcReason code="RC006"> text </ProcReason>
	 
	 
	 
	 
	 
	 
	 
	 

	7
	System price
	 
	16,4
	<-9999999999999999.9999; 9999999999999999.9999>; Float
	 
	 
	 
	 
	 
	 
	 
	 
	 

	8
	System volume
	 
	16,4
	<-9999999999999999.9999; 9999999999999999.9999>; Float
	 
	 
	 
	 
	 
	 
	 
	 
	 

	9
	Price CZ
	 
	16,4
	<-9999999999999999.9999; 9999999999999999.9999>; Float
	<ISOTEDATA/Trade/ProfileData profile-role=" SP50"/Data value="899">
	 
	 
	 
	 
	 
	 
	 
	 

	10
	Volume CZ - sell
	 
	16,4
	<-9999999999999999.9999; 9999999999999999.9999>; Float
	<ISOTEDATA/Trade/ProfileData profile-role=" SC50"/Data value="899">
	 
	 
	 
	 
	 
	 
	 
	 

	11
	Volume CZ - buy
	 
	16,4
	<-9999999999999999.9999; 9999999999999999.9999>; Float
	<ISOTEDATA/Trade/ProfileData profile-role=" SC51"/Data value="899">
	 
	 
	 
	 
	 
	 
	 
	 

	12
	Flow CZ => SK
	 
	16,4
	<-9999999999999999.9999; 9999999999999999.9999>; Float
	<ISOTEDATA/Trade/ProfileData profile-role=" SC52"/Data value="899">
	 
	 
	 
	 
	 
	 
	 
	 

	13
	 
	Period matching attribute 
(A – total matching, P – partial matching, N – not matched)
	1
	Char
	<ISOTEDATA / Trade / ProfileData /Data period-stage="A">
	 
	 
	 
	 
	 
	 
	 
	 

	14
	Requested flow CZ => SK
	 
	16,4
	<-9999999999999999.9999; 9999999999999999.9999>; Float
	 
	 
	 
	 
	 
	 
	 
	 
	 

	15
	Requested flow SK => CZ
	 
	16,4
	<-9999999999999999.9999; 9999999999999999.9999>; Float
	 
	 
	 
	 
	 
	 
	 
	 
	 

	16
	Price SK 
	 
	16,4
	<-9999999999999999.9999; 9999999999999999.9999>; Float
	<ISOTEDATA/Trade/ProfileData profile-role=" SP53"/Data value="899">
	 
	 
	 
	 
	 
	 
	 
	 

	17
	Volume SK - sell
	 
	16,4
	<-9999999999999999.9999; 9999999999999999.9999>; Float
	<ISOTEDATA/Trade/ProfileData profile-role=" SC53"/Data value="899">
	 
	 
	 
	 
	 
	 
	 
	 

	18
	Volume SK - buy
	 
	16,4
	<-9999999999999999.9999; 9999999999999999.9999>; Float
	<ISOTEDATA/Trade/ProfileData profile-role=" SC54"/Data value="899">
	 
	 
	 
	 
	 
	 
	 
	 

	19
	Flow SK => CZ
	 
	16,4
	<-9999999999999999.9999; 9999999999999999.9999>; Float
	<ISOTEDATA/Trade/ProfileData profile-role=" SC55"/Data value="899">
	 
	 
	 
	 
	 
	 
	 
	 

	20
	Profile ID (Sx01;Sx02;Sx03;Sx04; Sx05;Sx06;Sx07;Sx08; Sx09;Sx10;Sx11;Sx12; Sx14;Sx15;Sx16;Sx17; Sx18;Sx19;Sx20;Sx21; Sx22;Sx23;Sx24;Sx27; Sx28;Sx29;Sx30;Sx31; Sx32;Sx33;Sx34;Sx35; Sx54;Sx56;Sx57;Sx58;
	 
	4
	Char
	<ISOTEDATA/Trade/ProfileData profile-role="SP50">
	 
	 
	 
	 
	 
	 
	 
	 

	
	
	
	
	
	
	
	
	
	
	
	
	
	

	
	Mandatory field
	
	
	
	
	
	
	
	
	
	
	
	


5.5.2 Requirement  structure overview  – ISOTEREQ

	L.I.
	Result description
	Size
	Value/Type
	XML location
	Data requests

	
	
	
	
	
	Traded volume overall plan 
	DM Marginal prices
	Hourly settlement
	Daily settlement
	Accepted bids on BalM 
	Area DM results
	DM coordination results for SS
	Statistical data of imbalance settlement

	1
	Message code
	3
	Integer
	/ISOTEREQ/@message-code
	941
	944
	951
	961
	971
	934
	937
	964

	2
	Date (format: YYYY-MM-DD)
	10
	Varchar
	/ISOTEREQ/Trade/@trade-day
	 
	 
	 
	 
	 
	 
	 
	 

	3
	Settlement version: 1 - Daily DM Settlement, 2 - Daily Imbalance Settlement, 3 - Interim Monthly Settlement, 4 - Final Monthly Settlement, 5 – State of Emergency, 6 – Clearing LP
	5
	<0;99999>; Integer
	/ISOTEREQ/Trade/@version
	 
	 
	 
	 
	 
	 
	 
	 

	4
	Market type (OKO, DVS, VDT, BT)
	3
	Varchar
	/ISOTEREQ/Document/@market
	 
	 
	 
	 
	 
	 
	 
	 

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	Mandatory field
	
	
	
	
	
	
	
	
	
	
	


5.6 Gas IM commands

5.6.1 Command structure overview  – ISOTEDATA

	Gas IM description - order
	Gas IM description - trade
	Gas IM description  - trading screen
	XML location - order (ISOTEDATA)
	XML location - trade (ISOTEDATA)
	XML location - trading screen (ISOTEDATA)
	Size
	Value/Type
	Order entry
	Order cancellation
	Order data
transcript (entry, cancellation,
own order data)
	Own trade data transcript
	Trading screen data  - order data transcript

	Message code
	 
	 
	<ISOTEDATA/@message_code>
	3
	Char
	GV1
	GV4
	GV3, GV6, GV9
	GVE
	GVK

	Participant (EIC) – order creator ID
	 
	 
	<ISOTEDATA/Trade/Party/@id>
	3
	Varchar
	 
	 
	 
	 
	 

	Order type (N - buy, P -sell)
	Trade type (N - buy, P -sell)
	 
	<ISOTEDATA/Trade/@trade-type>
	1
	Char
	 
	 
	 
	 
	 

	Product (instance) title
	Product (instance) title
	Product (instance) title
	<ISOTEDATA/Trade/Comment>G-DD100401<Comment>
	30
	Varchar
	 
	 
	 
	 
	 

	Order cancellation time (YYYY-MM-DDThh:mm:ss)
	 
	 
	<ISOTEDATA/Trade/TimeData datetime="2004-03-19T15:24:00" datetime-type="DTA">
	19
	Varchar
	 
	 
	 
	 
	 

	Order code
	Order code
	 
	<ISOTEDATA/Trade/@id>
	10
	<1;9999999999>; Integer
	 
	 
	 
	 
	 

	Automatic cancellation attribute (A- automatically cancelled, U- cancelled by user, not indicated, if not cancelled)
	 
	 
	<ISOTEDATA/Trade/@replacement>
	1
	Char
	 
	 
	 
	 
	 

	Order attribute – mode (T – market maker mode, S – system order, not indicated for standard mode)
	 
	 
	<ISOTEDATA/Trade/@trade-state>
	1
	Char
	 
	 
	 
	 
	 

	Order entry time (YYYY-MM-DDThh:mm:ss)
	Trade creation time (YYYY-MM-DDThh:mm:ss)
	 
	<ISOTEDATA/Trade/TimeData datetime="2004-03-19T15:24:00" datetime-type="DTC">
	19
	Varchar
	 
	 
	 
	 
	 

	Order status/stage (P - valid, N - invalid)
	 
	 
	<ISOTEDATA/Trade/@trade-stage>
	1
	Char
	 
	 
	 
	 
	 

	 
	Trade code
	 
	<ISOTEDATA/Trade/@id-definition>
	10
	<1;9999999999>; Integer
	 
	 
	 
	 
	 

	 
	Order index (1 – trade price and number of contracts, 2 – total price amount and traded volume)
	Order index (1 to 5 – top 5 orders to buy, 6 to 10 – top 5 orders to sell, 11 – day statistics, 12 – product (instance) statistics)
	 
	<ISOTEDATA/Trade/ProfileData/
Data/@period>
	<ISOTEDATA/Trade/ProfileData/
Data/@period>
	2
	<1;25>; Integer
	 
	 
	 
	 
	 

	 
	Traded volume [MWh]
	Final price (for 1-10), Bottom price (for11 and 12)
	 
	profile-role: 
SC49: buy, SC99: sell

<ISOTEDATA/Trade/ProfileData profile-role="SCx9"/Data value="100">
	profile-role: 
Final price (N, P): 
SC40,SC41
Bottom price (Den,Prod): SP42,SP44

<ISOTEDATA/Trade/ProfileData profile-role="Sx4x"/Data value="100">
	16,4
	<-9999999999999999.9999; 9999999999999999.9999>; Float
	 
	 
	 
	 
	 

	Limit price
	Trade price/Total price amount
	Limit price (for 1-10), Ceiling price (for 11 and 12)
	profile-role: 
SP46: buy, SP96: sell

<ISOTEDATA/Trade/ProfileData profile-role="SPx6"/Data value="100">
	Trade price (period=1): 
profile-role: 
SP48: buy, SP98: sell
Total price (period=2): 
profile-role: 
SP49: buy, SP99: sell

<ISOTEDATA/Trade/ProfileData profile-role="SPxx"/Data value="899">
	profile-role: 
Limit price (N, P): 
SP40,SP41
Ceiling price (Den,Prod): SP43,SP45

<ISOTEDATA/Trade/ProfileData profile-role="SP4X"/Data value="100">
	16,4
	<-9999999999999999.9999; 9999999999999999.9999>; Float
	 
	 
	 
	 
	 

	Number of contracts
	 
	Number of contracts
	profile-role: 
SC46: buy, SC96: sell

<ISOTEDATA/Trade/ProfileData profile-role="SCx6"/Data value="100">
	 
	<ISOTEDATA/Trade/ProfileData profile-role="SC42"/Data value="100">
	5
	<0;999999>; Integer
	 
	 
	 
	 
	 

	Number of traded contracts
	Number of traded contracts
	 
	profile-role: 
SC47: buy, SC97: sell

<ISOTEDATA/Trade/ProfileData profile-role="SCx7"/Data value="100">
	profile-role: 
SC48: buy, SC98: sell

<ISOTEDATA/Trade/ProfileData profile-role="SCx8"/Data value="100">
	 
	5
	<0;999999>; Integer
	 
	 
	 
	 
	 

	
	
	
	
	
	
	
	
	
	
	
	
	

	
	Mandatory field
	
	
	
	
	
	
	
	
	
	
	


5.6.2 Requirement structure overview  – ISOTEREQ

	Description Gas IM - 
order / trade
	XML location (ISOTEREQ)
	Size
	Value/Type
	Own order data
	Trade request (own)

	Message code
	ISOTEREQ/@message_code
	3
	Varchar
	GV7
	GVC

	Product (instance) name
	ISOTEREQ/Trade/@product
	30
	Varchar
	 
	 

	Order code
	ISOTEREQ/Trade/@id
	10
	<1;9999999999>; Integer
	 
	 

	Order entry time  / 
Trade creation time
	ISOTEREQ/Trade/@trade-day
	19
	<10;19> Varchar ("2009-01-03", "2009-03-13T11:48:57")
	 
	 

	Trade code
	ISOTEREQ/Trade/@id
	10
	<1;9999999999>; Integer
	 
	 

	
	
	
	
	
	

	
	Mandatory field
	
	
	
	


5.7 Gas IM instances

5.7.1 Command structure overview  – ISOTEMASTERDATA

	 
	 
	Product description
ISOTEMASTERDATA

	Message code
	ISOTEMASTERDATA/@message_code
	GVH

	Instance
	<ISOTEMASTERDATA / Instance instance-id = "G-DD100401">
	 

	Commodity code (P - gas, E - electricity)
	ISOTEMASTERDATA/@commodity_code
	 

	Long instance title
	<ISOTEMASTERDATA / Instance instance-description = "CZ Daily 2010-04-01">
	 

	Instance class (D - Daily)
	<ISOTEMASTERDATA / Instance instance-class="BMD">
	 

	Block type  (P - Peak, O-Offpeak, B-Base)
	<ISOTEMASTERDATA / Instance instance-type="PDD">
	 

	Instance location
	<ISOTEMASTERDATA / Instance location="CZ">
	 

	Instance contract unit
	<ISOTEMASTERDATA / Instance unit = "MWH">
	 

	Instance currency unit
	<ISOTEMASTERDATA / Instance currency = "EUR">
	 

	Settlement type (PS - actual delivery)
	<ISOTEMASTERDATA / Instance processing-type="PS">
	 

	Contract volume [contract unit]
	<ISOTEMASTERDATA / Instance / Characteristic  charact-role = "Q_BM001" value-qty="1" unit="MWH">
	 

	Minimum supply volume [MWh]
	<ISOTEMASTERDATA / Instance / Characteristic  charact-role = "Q_BM002" value-qty="1" unit="MWH">
	 

	Initial delivery day (YYYY-MM-DD)
	<ISOTEMASTERDATA / Instance / Characteristic  charact-role = "D_BM001" value-date="2010-04-01">
	 

	Final delivery day (YYYY-MM-DD)
	<ISOTEMASTERDATA / Instance / Characteristic  charact-role = "D_BM002" value-date="2010-04-01">
	 

	Order index 
	<ISOTEMASTERDATA / Instance / Interval interval-role="CDI" order-index="1" interval-date="2010-04-01" period-from="1" period-to="1"/>
	 

	Supply interval (YYYY-MM-DD)
	<ISOTEMASTERDATA / Instance / Interval interval-role="CDI" order-index="1" interval-date="2010-04-01" period-from="1" period-to="1"/>
	 

	Supply interval – initial period
	<ISOTEMASTERDATA / Instance / Interval interval-role="CDI" order-index="1" interval-date="2010-04-01" period-from="1" period-to="1"/>
	 

	Supply interval – final period
	<ISOTEMASTERDATA / Instance / Interval interval-role="CDI" order-index="1" interval-date="2010-04-01" period-from="1" period-to="1"/>
	 

	Event title (N_ISSUE – notification: instance not released, ISSUE - notification: instance released, TRC_START_MM – continual trade open for market maker, TRC_START_SS - continual trade open  for subjects of settlement, TRC_CLOSE - continual trade close, AGGREG – data aggregation, PUBLICATION – data publishing)
	<ISOTEMASTERDATA / Instance / Interval interval-role="ISSUE" order-index="1" date-time-from="2010-03-31T17:00:00"/>
	 

	Time of event (YYYY-MM-DDThh:mm:ss)
	<ISOTEMASTERDATA / Instance / Interval interval-role="ISSUE" order-index="1" date-time-from="2010-03-31T17:00:00"/>
	 


5.7.2 Requirement structure overview  – ISOTEREQ

	Description
	XML location (ISOTEREQ)
	Size
	Value/Type
	Instance data request

	Message code
	ISOTEREQ/@message_code
	3
	Varchar
	GVF

	Instance
	ISOTEREQ/Trade/@product
	30
	Varchar
	 

	
	
	
	
	

	
	Mandatory field
	
	
	


5.8 Gas DM commands

5.8.1 Command structure overview  – ISOTEDATA

	Gas DM description
	XML location (ISOTEDATA)
	Size
	Value/Type
	Bid Entry / Replacement
	Bid cancellation 
	Bid data transcript (entry, cancellation, own bid data)

	Message code
	<ISOTEDATA/@message_code>
	3
	Char
	GD1
	GD4
	GD3, GD6, GD9

	Commodity code (P - gas, E - electricity)
	<ISOTEDATA/@commodity_code>
	1
	Char
	 
	 
	 

	Participant (EIC) - owner id
	<ISOTEDATA/Trade/Party/@id>
	16
	Varchar
	 
	 
	 

	Gas day (format: YYYY-MM-DD)
	<ISOTEDATA/Trade/@trade-day>
	10
	Varchar
	 
	 
	 

	Session (1 - morning, 2 - afternoon)
	<ISOTEDATA/Trade/@trade-session
	5
	Integer
	 
	 
	 

	Bid type (N - buy, P -sell)
	<ISOTEDATA/Trade/@trade-type>
	1
	Char
	 
	 
	 

	Comment
	<ISOTEDATA/Trade/Comment>
	30
	Varchar
	 
	 
	 

	Bid cancellation time  (YYYY-MM-DDThh:mm:ss)
	<ISOTEDATA/Trade/TimeData datetime="2004-03-19T15:24:35" datetime-type="DTA">
	19
	Varchar
	 
	 
	 

	Bid ID 
	<ISOTEDATA/Trade id="555">
	10
	<1;9999999999>; Integer
	 
	 
	 

	Bid version
	<ISOTEDATA/Trade/@version>
	5
	<0;99999>; Integer
	 
	 
	 

	Bid replacement attribute (A - replaced, N - not replaced)
	<ISOTEDATA/Trade replacement="A">
	1
	Char
	 
	 
	 

	Bid entry time (YYYY-MM-DDThh:mm:ss)
	<ISOTEDATA/Trade/TimeData datetime="2004-03-19T15:24:35" datetime-type="DTC">
	19
	Varchar
	 
	 
	 

	Error code
	<ISOTEDATA/Trade/@error-code>
	4
	0;<1000;9999>; Integer
	 
	 
	 

	Settlment currency code  (CZK, EUR)
	<ISOTEDATA/Trade/@sett-curr>
	3
	Char
	 
	 
	 

	Data source (PXE, OTE)
	<ISOTEDATA/Trade/@source-sys>
	3
	Char
	 
	 
	 

	Bid status (P – valid,  N – invalid)
	<ISOTEDATA trade-stage ="P">
	1
	Char
	 
	 
	 

	Bid cancellation  attribute (N – not cancelled, A - cancelled)
	<ISOTEDATA/Trade/@trade-flag>
	1
	Char
	 
	 
	 

	Period (for Gas DM always 1)
	<ISOTEDATA/Trade/ProfileData/Data/@period>
	1
	<1>; Integer
	 
	 
	 

	Volume
	<ISOTEDATA/Trade/ProfileData/Data/@value>
(pokud <ProfileData profile-role="BC##">)
	16,4
	<-9999999999999999.9999; 9999999999999999.9999>; Float
	 
	 
	 

	Price
	<ISOTEDATA/Trade/ProfileData/Data/@value>
(pokud <ProfileData profile-role="BP##">)
	16,4
	<-9999999999999999.9999; 9999999999999999.9999>; Float
	 
	 
	 

	Block 1 volume divisibility (A-yes, N-no)
	<ISOTEDATA/Trade/ProfileData/Data/@splitting>
	1
	Char
	 
	 
	 

	Bid block  ID
	<ISOTEDATA/Trade/ProfileData/@profile-role>
(hodnoty: BC01-25, BP01-25)
	4
	Char
	 
	 
	 

	
	
	
	
	
	
	

	
	Mandatory field
	
	
	
	
	


5.8.2 Requirement structure overview  – ISOTEREQ

	Gas DM description
	XML location (ISOTEREQ)
	Size
	Value/Type
	Own bid data (status request) 

	Message code
	ISOTEREQ/@message_code
	3
	Varchar
	GD7

	Gas day (format: YYYY-MM-DD)
	ISOTEREQ/Trade/@trade-day
	10
	Varchar ("2009-01-03")
	 

	Bid ID
	ISOTEREQ/Trade/@id
	10
	<1;9999999999>; Integer
	 

	Bid version
	ISOTEREQ/Trade/@version
	10
	<1;9999999999>; Integer
	 

	Session
	ISOTEREQ/Trade/@trade-session
	1
	Integer
	 

	
	
	
	
	

	
	Mandatory field
	
	
	


5.9 Gas settlement commands

5.9.1 Command and requirement structure overview  – ISOTEDATA and ISOTEREQ

	Results description
	ISOTEREQ (request)
	ISOTEDATA (data transcript)
	Size
	Value/Type
	Request - Marginal prices of Gas DM
	Data transcript - Marginal prices of Gas DM
	Request - Daily settlement
	Data transcript - Daily settlement

	Message code
	ISOTEREQ/@message_code
	ISOTEDATA/@message_code
	3
	Integer
	GDD
	GDF
	GSD
	GSF

	Participant (EIC)
	 
	ISOTEDATA/Trade/Party/@id
	16
	<1;9999999999999>; Integer
	 
	 
	 
	 

	Date (format: YYYY-MM-DD)
	ISOTEREQ/Trade/@trade-day
	<ISOTEDATA/Trade trade-day="2004-03-19">
	10
	Varchar
	 
	 
	 
	 

	Settlement version: 9 - Gas DM morning session, 10 - Gas DM afternoon session, 11 - Monthly settlement with gas, 12 - Final monthly settlement with gas, 13 - Daily settlement Gas IM
	 
	ISOTEDATA/Trade/@version
	5
	<0;99999>; Integer
	 
	 
	 
	 

	Session (1 - morning, 2 - afternoon)
	 
	<ISOTEDATA/Trade/@trade-session
	5
	Integer
	 
	 
	 
	 

	Period (for gas always 1)
	 
	<ISOTEDATA/Trade/ProfileData/Data period="1">
	1
	<1>; Integer
	 
	 
	 
	 

	Volume
	 
	<ISOTEDATA/Trade/ProfileData profile-role="SC02"/Data value="10,5">
	16,4
	<-9999999999999999.9999; 9999999999999999.9999>; Float
	 
	 
	 
	 

	Price
	 
	<ISOTEDATA/Trade/ProfileData profile-role=" SP02"/Data value="899">
	16,4
	<-9999999999999999.9999; 9999999999999999.9999>; Float
	 
	 
	 
	 

	Currency code (CZK, EUR)
	 
	<ISOTEDATA/Trade/ProfileData Data unit="EUR">
	3
	Char
	 
	 
	 
	 

	Profile identification: 
Marginal prices: Sx20

Daily settlement: Sx02;Sx03; Sx05;Sx15;Sx16;Sx33;Sx34;Sx35
	 
	<ISOTEDATA/Trade/ProfileData profile-role="SP50">
	4
	Char
	 
	 
	 
	 

	
	
	
	
	
	
	
	
	

	
	Mandatory field
	
	
	
	
	
	
	


5.10 General commands 

5.10.1 Response structure review – RESPONSE

	L.I.
	Description
	XML view

	1
	Message code
	RESPONSE/@message-code="881"

	2
	Bid/order ID
	RESPONSE/Reason/@trade-id="1111"

	3
	Bid/order version
	RESPONSE/Reason version="1"

	4
	Descriptive message to the recipient /Mail body (mail body text only)
	RESPONSE/Reason (element value)

	5
	Error code
	RESPONSE/Reason/@code="5504"

	6
	Error type
	RESPONSE/Reason/@type="A04" or "A03" or "A02" 

	7
	Sender ID
	RESPONSE/SenderIdentification/@id="8591824000007"

	8
	Recipient ID
	RESPONSE/ReceiverIdentification/@id="8591824000007"

	9
	Message ID (is used for a service request for processing results in case of klient-server communication architecture)
	RESPONSE/@id="11111111"


5.11 Notification

5.11.1 Summary of notification structure – RESPONSE
	L.I.
	DM description
	XML location (ISOTEDATA)
	Size
	Value/Type
	Notification about change (shift) of gate closure time
	 
	 

	1
	Message identifier
	RESPONSE/@id
	15
	Integer
	981
	 
	 

	2
	Message code
	RESPONSE/@message-code
	3
	Varchar
	 
	 
	 

	3
	Message create time
	RESPONSE/@date-time
	19
	Varchar
	 
	 
	 

	4
	Sender Identification
	RESPONSE/SenderIdentification/@id
	16
	Varchar
	 
	 
	 

	5
	Receiver Identification
	RESPONSE/ReceiverIdentification/@id
	16
	Varchar
	 
	 
	 

	6
	Reason (message body)
	RESPONSE/Reason 
	500
	Varchar
	 
	 
	 

	7
	Reason Code
	RESPONSE/Reason/@code
	4
	Varchar
	 
	 
	 

	8
	Reason Type
	RESPONSE/Reason/@type
	3
	Varchar
	 
	 
	 

	
	
	
	
	
	
	
	

	 
	Mandatory field
	
	
	
	
	
	


Commands in ETSO format

5.11.2 Messages in ETSO ECAN Capacity Document structure

	 
	 
	 
	 
	MCC for DM
	 
	 
	MCC for DM

	
	L.I.
	Description
ECAN CapacityDocument
	CapacityDocument ==> CD
	Value
	Size
	Value/Type
	 

	 
	1
	DocumentIdentification
	CD/DocumentIdentification/@v
	20090501_A13_27XOTE-CZECHREPB
	35
	Varchar
	 

	 
	2
	DocumentVersion
	CD/DocumentVersion/@v
	1
	3
	<1;999>; Integer
	 

	
	3
	DocumentType
	CD/DocumentType/@v
	A13
	3
	Varchar
	 

	
	4
	ProcessType
	CD/ProcessType/@v
	A07 
	3
	Varchar
	 

	
	5
	SenderIdentification
	CD/SenderIdentification/@v
	10XSK-SEPS-GRIDB
	16
	Varchar
	 

	
	6
	SenderIdentification.codingScheme
	CD/SenderIdentification/@codingScheme
	A01
	3
	Varchar
	 

	
	7
	SenderRole
	CD/SenderRole/@v
	A04
	3
	Varchar
	 

	
	8
	ReceiverIdentification
	CD/ReceiverIdentification/@v
	27XOTE-CZECHREPB
	16
	Varchar
	 

	
	9
	ReceiverIdentification.codingScheme
	CD/ReceiverIdentification/@codingScheme
	A01
	3
	Varchar
	 

	
	10
	ReceiverRole
	CD/ReceiverRole/@v
	A07 
	3
	Varchar
	 

	
	11
	CreationDateTime v UCT 
(ve tvaru YYYY-MM-DDThh:mm:ssZ)
	CD/CreationDateTime/@v
	2009-04-30T06:30:30Z
	20
	Varchar
	 

	
	12
	CapacityTimeInterval v UCT
(ve tvaru YYYY-MM-DDThh:00Z/YYYY-MM-DD+1Thh:00Z)
	CD/CapacityTimeInterval/@v
	2009-04-30T22:00Z/2009-05-01T22:00Z
	35
	Varchar
	 

	
	13
	Domain
	CD/Domain/@v
	10YDOM-CZ-DE-SKK
	16
	Varchar
	 

	
	14
	Domain.codingScheme
	CD/Domain/@codingScheme
	A01
	3
	Varchar
	 

	
	15
	TimeSeriesIdentification
	CD/CapacityTimeSeries/TimeSeriesIdentification/@v
	TS_001
	35
	Varchar
	 

	
	16
	BusinesType
	CD/CapacityTimeSeries/BusinessType/@v
	A31
	3
	Varchar
	 

	
	17
	Product
	CD/CapacityTimeSeries/Product/@v
	8716867000016
	13
	Integer
	 

	
	18
	InArea
	CD/CapacityTimeSeries/InArea/@v
	{10YSK-SEPS-----K ; 
10YCZ-CEPS-----N}
	18
	Varchar
	 

	
	19
	InArea.codingScheme
	CD/CapacityTimeSeries/InArea/@codingScheme
	A01
	3
	Varchar
	 

	
	20
	OutArea
	CD/CapacityTimeSeries/OutArea/@v
	{10YCZ-CEPS-----N ;
10YSK-SEPS-----K}
	18
	Varchar
	 

	
	21
	OutArea.codingScheme
	CD/CapacityTimeSeries/OutArea/@codingScheme
	A01
	3
	Varchar
	 

	
	22
	MeasurementUnit
	CD/CapacityTimeSeries/MeasureUnit/@v
	MAW
	5
	Varchar
	 

	
	23
	TimeInterval  v UCT
(ve tvaru YYYY-MM-DDThh:00Z/YYYY-MM-DD+1Thh:00Z)
	CD/CapacityTimeSeries/Period/TimeInterval/@v
	2009-04-30T22:00Z/2009-05-01T22:00Z
	35
	Varchar
	 

	
	24
	Resolution
	CD/CapacityTimeSeries/Period/Resolution/@v
	PT60M
	15
	Varchar
	 

	
	25
	Interval - Pos
	CD/CapacityTimeSeries/Period/Interval/Pos/@v
	23
	6
	<1;999999>; Integer
	 

	
	26
	Interval - Qty
	CD/CapacityTimeSeries/Period/Interval/Qty/@v
	70
	16,4
	<-9999999999999999.9999; 9999999999999999.9999>; Float
	 

	
	
	
	
	
	
	
	

	
	
	
	Mandatory field
	
	
	
	

	
	
	TS_001
	Example of valid value
	
	
	
	

	
	
	{10YSK-SEPS-----K ;
10YCZ-CEPS-----N}
	Enumeration of possible values (constants)
	
	
	
	

	
	
	A01
	Constant value
	
	
	
	

	
	
	
	
	
	
	
	


5.11.3 Messages in ETSO ECAN ImplicitAuctionResult Document structure

	 
	 
	 
	 
	Results of implicit auction
	 
	 
	Results of implicit auction

	 
	L.I.
	Description
ECAN ImplicitAuctionResultDocument
	ImplicitAuction
ResultDocument ==> IARD
	Value
	Size
	Value/Type
	 

	 
	1
	DocumentIdentification
	IARD/DocumentIdentification/@v
	20090401_A25_10XSK-SEPS-GRIDB
	35
	Varchar
	 

	
	2
	DocumentVersion
	IARD/DocumentVersion/@v
	1
	3
	<1;999>; Integer
	 

	
	3
	DocumentType
	IARD/DocumentType/@v
	A25
	3
	Varchar
	 

	
	4
	SenderIdentification
	IARD/SenderIdentification/@v
	{ 27XOTE-CZECHREPB ;
 24X-OT-SK------V }
	16
	Varchar
	 

	
	5
	SenderIdentification.codingScheme
	IARD/SenderIdentification/@codingScheme
	A01
	3
	Varchar
	 

	
	6
	SenderRole
	IARD/SenderRole/@v
	A07
	3
	Varchar
	 

	
	7
	ReceiverIdentification
	IARD/ReceiverIdentification/@v
	{10XCZ-CEPS-GRIDE ;
10XSK-SEPS-GRIDB }
	16
	Varchar
	 

	
	8
	ReceiverIdentification.codingScheme
	IARD/ReceiverIdentification/@codingScheme
	A01
	3
	Varchar
	 

	
	9
	ReceiverRole
	IARD/ReceiverRole/@v
	A04
	3
	Varchar
	 

	
	10
	CreationDateTime v UCT
(ve tvaru YYYY-MM-DDThh:mm:ssZ)
	IARD/CreationDateTime/@v
	2009-04-01T09:30:40Z
	20
	Varchar
	 

	
	11
	PublicationTimeInterval v UCT-
(ve tvaru YYYY-MM-DDThh:00Z/YYYY-MM-DD+1Thh:00Z)
	IARD/PublicationTimeInterval/@v
	2009-04-30T22:00Z/2009-05-01T22:00Z
	35
	Varchar
	 

	
	12
	Domain
	IARD/Domain/@v
	10YDOM-CZ-DE-SKK
	16
	Varchar
	 

	
	13
	Domain.codingScheme
	IARD/Domain/@codingScheme
	A01
	3
	Varchar
	 

	
	14
	TimeSeriesIdentification
	IARD/ResultTimeSeries/SendersTimeSeriesIdentification/@v
	TS_001
	35
	Varchar
	 

	
	15
	AllocationType
	IARD/ResultTimeSeries/AllocationType/@v
	A01
	3
	Varchar
	 

	
	16
	BusinessType
	IARD/ResultTimeSeries/BusinessType/@v
	A47
	3
	Varchar
	 

	
	17
	InArea
	IARD/ResultTimeSeries/InArea/@v
	{10YSK-SEPS-----K ;
10YCZ-CEPS-----N}
	18
	Varchar
	 

	
	18
	InArea.codingScheme
	IARD/ResultTimeSeries/InArea/@codingScheme
	A01
	3
	Varchar
	 

	
	19
	OutArea
	IARD/ResultTimeSeries/OutArea/@v
	{10YSK-SEPS-----K ;
10YCZ-CEPS-----N}
	18
	Varchar
	 

	
	20
	OutArea.codingScheme
	IARD/ResultTimeSeries/OutArea/@codingScheme
	A01
	3
	Varchar
	 

	
	21
	ContractType
	IARD/ResultTimeSeries/ContractType/@v
	A01
	5
	Varchar
	 

	
	22
	MeasureUnitQuantity
	IARD/ResultTimeSeries/MeasureUnitQuantity/@v
	MAW
	5
	Varchar
	 

	
	23
	Currency
	IARD/ResultTimeSeries/Currency/@v
	EUR
	5
	Varchar
	 

	
	24
	MeasureUnitPrice
	IARD/ResultTimeSeries/MeasureUnitPrice/@v
	MAW
	5
	Varchar
	 

	
	25
	TimeInterval  v UCT
(ve tvaru YYYY-MM-DDThh:00Z/YYYY-MM-DD+1Thh:00Z)
	IARD/ResultTimeSeries/Period/TimeInterval/@v
	2009-04-30T22:00Z/2009-05-01T22:00Z
	35
	Varchar
	 

	
	26
	Resolution
	IARD/ResultTimeSeries/Period/Resolution/@v
	PT60M
	15
	Varchar
	 

	
	27
	Interval - Pos
	IARD/ResultTimeSeries/Period/Interval/Pos/@v
	18
	6
	<1;999999>; Integer
	 

	
	28
	Interval - Qty
	IARD/ResultTimeSeries/Period/Interval/Qty/@v
	24.2
	16,4
	<-9999999999999999.9999; 9999999999999999.9999>; Float
	 

	
	29
	Interval - Price
	IARD/ResultTimeSeries/Period/Interval/Price/@v
	31.38
	16,4
	<-9999999999999999.9999; 9999999999999999.9999>; Float
	 

	
	
	
	
	
	
	
	

	
	
	
	Mandatory field
	
	
	
	

	
	
	TS_001
	Example of valid value
	
	
	
	

	
	
	{10YSK-SEPS-----K ;
10YCZ-CEPS-----N}
	Enumeration of possible values (constants)
	
	
	
	

	
	
	A01
	Constant value
	
	
	
	


5.11.4 Messages in ETSO ESS Schedule Message structure

	 
	 
	 
	Out-of-limit DM exchange
	RD entry
	 
	 
	Out-of-limit DM exchange
	RD entry

	L.I.
	Description
ESS Schedule message
	ScheduleMessage ==> SM
	Value
	Value
	Size
	Value/Type
	 
	 

	1
	MessageIdentification
	SM/MessageIdentification/@v
	20090401_A02_10XCZ-CEPS-GRIDE
	20080905_A01_10XCZ-CEPS-GRIDE_1
	35
	Varchar
	 
	 

	2
	MessageVersion
	SM/MessageVersion/@v
	1
	1
	3
	<1;999>; Integer
	 
	 

	3
	MessageType
	SM/MessageType/@v
	A02
	{A01; A09}
	3
	Varchar
	 
	 

	4
	ProcessType
	SM/ProcessType/@v
	A01
	{A01; A02; A12}
	3
	Varchar
	 
	 

	5
	ScheduleClassificationType
	SM/ScheduleClassificationType/@v
	A01
	A01
	3
	Varchar
	 
	 

	6
	SenderIdentification
	SM/SenderIdentification/@v
	{27XOTE-CZECHREPB ;
24X-OT-SK------V}
	8591824010402
	16
	Varchar
	 
	 

	7
	SenderIdentification.codingScheme
	SM/SenderIdentification/@codingScheme
	A01
	A10
	3
	Varchar
	 
	 

	8
	SenderRole
	SM/SenderRole/@v
	A07
	{A01; A04; A11}
	3
	Varchar
	 
	 

	9
	ReceiverIdentification
	SM/ReceiverIdentification/@v
	{10XCZ-CEPS-GRIDE ;
10XSK-SEPS-GRIDB}
	8591824000007
	16
	Varchar
	 
	 

	10
	ReceiverIdentification.codingScheme
	SM/ReceiverIdentification/@codingScheme
	A01
	A10
	3
	Varchar
	 
	 

	11
	ReceiverRole
	SM/ReceiverRole/@v
	A04
	A05
	3
	Varchar
	 
	 

	12
	MessageDateTime v UCT
(ve tvaru YYYY-MM-DDThh:mm:ssZ)
	SM/MessageDateTime/@v
	2009-04-01T09:30:30Z
	2009-04-01T09:30:30Z
	20
	Varchar
	 
	 

	13
	ScheduleTimeInterval v UCT
(ve tvaru YYYY-MM-DDThh:00Z/YYYY-MM-DD+1Thh:00Z)
	SM/ScheduleTimeInterval/@v
	2009-04-30T22:00Z/2009-05-01T22:00Z
	2009-04-30T22:00Z/2009-05-01T22:00Z
	35
	Varchar
	 
	 

	14
	Domain
	SM/Domain/@v
	10YDOM-CZ-DE-SKK
	10YDOM-CZ-DE-SKK
	16
	Varchar
	 
	 

	15
	Domain.codingScheme
	SM/Domain/@codingScheme
	A01
	A01
	3
	Varchar
	 
	 

	16
	SubjectParty
	SM/SubjectParty/@v
	{27XOTE-CZECHREPB ;
24X-OT-SK------V}
	8591824010402
	16
	Varchar
	 
	 

	17
	SubjectParty.codingScheme
	SM/SubjectParty/@codingScheme
	A01
	A10
	3
	Varchar
	 
	 

	18
	SubjectRole
	SM/SubjectRole/@v
	{A07; A11}
	A01
	5
	Varchar
	 
	 

	19
	MatchingPeriod
	SM/MatchingPeriod/@v
	n/a
	2009-04-30T22:00Z/2009-05-01T22:00Z
	35
	Varchar
	 
	 

	20
	SendersTimeSeriesIdentification
	SM/ScheduleTimeSeries/SendersTimeSeriesIdentification/@v
	TS_001
	TS_001
	35
	Varchar
	 
	 

	21
	SendersTimeSeriesVersion
	SM/ScheduleTimeSeries/SendersTimeSeriesVersion/@v
	1
	1
	3
	Integer
	 
	 

	22
	BusinesType
	SM/ScheduleTimeSeries/BusinessType/@v
	A06
	{A02; A06}
	3
	Varchar
	 
	 

	23
	Product
	SM/ScheduleTimeSeries/Product/@v
	8716867000016
	8716867000016
	13
	Integer
	 
	 

	24
	ObjectAgregation
	SM/ScheduleTimeSeries/ObjectAggregation/@v
	A03
	A03
	3
	Varchar
	 
	 

	25
	InArea
	SM/ScheduleTimeSeries/InArea/@v
	{10YCZ-CEPS-----N ;
10YSK-SEPS-----K}
	10YCZ-CEPS-----N
	18
	Varchar
	 
	 

	26
	InArea.codingScheme
	SM/ScheduleTimeSeries/InArea/@codingScheme
	A01
	A01
	3
	Varchar
	 
	 

	27
	OutArea
	SM/ScheduleTimeSeries/OutArea/@v
	{10YCZ-CEPS-----N ;
10YSK-SEPS-----K}
	10YCZ-CEPS-----N
	18
	Varchar
	 
	 

	28
	OutArea.codingScheme
	SM/ScheduleTimeSeries/OutArea/@codingScheme
	A01
	A01
	3
	Varchar
	 
	 

	29
	InParty
	SM/ScheduleTimeSeries/InParty/@v
	{27XOTE-CZECHREPB ;
24X-OT-SK------V}
	8591824010402
	16
	Varchar
	 
	 

	30
	InParty.codingScheme
	SM/ScheduleTimeSeries/InParty/@codingScheme
	A01
	A10
	3
	Varchar
	 
	 

	31
	OutParty
	SM/ScheduleTimeSeries/OutParty/@v
	{27XOTE-CZECHREPB ;
24X-OT-SK------V}
	8591824010402
	16
	Varchar
	 
	 

	32
	OutParty.codingScheme
	SM/ScheduleTimeSeries/OutParty/@codingScheme
	A01
	A10
	3
	Varchar
	 
	 

	33
	CapacityContractType
	SM/ScheduleTimeSeries/CapacityContractType/@v
	A01
	n/a
	5
	Varchar
	 
	 

	34
	MeasurementUnit
	SM/ScheduleTimeSeries/MeasurementUnit/@v
	MAW
	MAW
	5
	Varchar
	 
	 

	35
	TimeInterval  v UCT
(ve tvaru YYYY-MM-DDThh:00Z/YYYY-MM-DD+1Thh:00Z)
	SM/ScheduleTimeSeries/Period/TimeInterval/@v
	2009-04-30T22:00Z/2009-05-01T22:00Z
	2009-04-30T22:00Z/2009-05-01T22:00Z
	35
	Varchar
	 
	 

	36
	Resolution
	SM/ScheduleTimeSeries/Period/Resolution/@v
	PT60M
	PT60M
	15
	Varchar
	 
	 

	37
	Interval - Pos
	SM/ScheduleTimeSeries/Period/Interval/Pos/@v
	7
	7
	6
	<1;999999>; Integer
	 
	 

	38
	Interval - Qty
	SM/ScheduleTimeSeries/Period/Interval/Qty/@v
	41
	41
	16,4
	<-9999999999999999.9999; 9999999999999999.9999>; Float
	 
	 

	
	
	
	
	
	
	
	
	

	
	 
	Mandatory field
	
	
	
	
	
	

	
	TS_001
	Example of valid value
	
	
	
	
	
	

	
	{10YSK-SEPS-----K ;
10YCZ-CEPS-----N}
	Enumeration of possible values (constants)
	
	
	
	
	
	

	
	A01
	Constant value
	
	
	
	
	
	


5.11.5 Messages in ETSO ESS Anomaly Report structure

	 
	 
	 
	 
	 
	 

	L.I.
	Description 
ESS Anomaly Report
	AnomalyReport ==> AR
	Value
	Size
	Value/Type

	1
	MessageIdentification
	AR/MessageIdentification/@v
	20090401_A02_10XCZ-CEPS-GRIDE
	35
	Varchar

	2
	MessageDateTime v UCT
(ve tvaru YYYY-MM-DDThh:mm:ssZ)
	AR/MessageDateTime/@v
	2009-04-01T09:30:30Z
	20
	Varchar

	3
	SenderIdentification
	AR/SenderIdentification/@v
	8591824000007
	16
	Varchar

	4
	SenderIdentification.codingScheme
	AR/SenderIdentification/@codingScheme
	A10
	3
	Varchar

	5
	SenderRole
	AR/SenderRole/@v
	A05
	3
	Varchar

	6
	ReceiverIdentification
	AR/ReceiverIdentification/@v
	8591824010402
	16
	Varchar

	7
	ReceiverIdentification.codingScheme
	AR/ReceiverIdentification/@codingScheme
	A10
	3
	Varchar

	8
	ReceiverRole
	AR/ReceiverRole/@v
	{A01; A04; A11}
	3
	Varchar

	9
	ScheduleTimeInterval v UCT
(ve tvaru YYYY-MM-DDThh:00Z/YYYY-MM-DD+1Thh:00Z)
	AR/ScheduleTimeInterval/@v
	2009-04-30T22:00Z/2009-05-01T22:00Z
	35
	Varchar

	10
	MessageSenderIdentification
	AR/TimeSeriesAnomaly/MessageSenderIdentification/@v
	8591824010402
	16
	Varchar

	11
	MessageSenderIdentification.codingScheme
	AR/TimeSeriesAnomaly/MessageSenderIdentification/@codingScheme
	A10
	3
	Varchar

	 
	SendersMessageIdentification
	AR/TimeSeriesAnomaly/SendersMessageIdentification/@v
	20090401_A01_10XCZ-XXX-YYY_001
	35
	Varchar

	12
	SendersMessageVersion
	AR/TimeSeriesAnomaly/SendersMessageVersion/@v
	1
	3
	Integer

	13
	SendersTimeSeriesIdentification
	AR/TimeSeriesAnomaly/SendersTimeSeriesIdentification/@v
	TS_001
	35
	Varchar

	14
	SendersTimeSeriesVersion
	AR/TimeSeriesAnomaly/SendersTimeSeriesVersion/@v
	1
	3
	Integer

	15
	BusinesType
	AR/TimeSeriesAnomaly/BusinessType/@v
	{A02; A06}
	3
	Varchar

	16
	Product
	AR/TimeSeriesAnomaly/Product/@v
	8716867000016
	13
	Integer

	17
	ObjectAgregation
	AR/TimeSeriesAnomaly/ObjectAggregation/@v
	A03
	3
	Varchar

	18
	InArea
	AR/TimeSeriesAnomaly/InArea/@v
	10YCZ-CEPS-----N
	16
	Varchar

	19
	InArea.codingScheme
	AR/TimeSeriesAnomaly/InArea/@codingScheme
	A01
	3
	Varchar

	20
	OutArea
	AR/TimeSeriesAnomaly/OutArea/@v
	10YCZ-CEPS-----N
	16
	Varchar

	21
	OutArea.codingScheme
	AR/TimeSeriesAnomaly/OutArea/@codingScheme
	A01
	3
	Varchar

	18
	InParty
	AR/TimeSeriesAnomaly/InParty/@v
	8591824010402
	16
	Varchar

	19
	InParty.codingScheme
	AR/TimeSeriesAnomaly/InParty/@codingScheme
	A10
	3
	Varchar

	20
	OutParty
	AR/TimeSeriesAnomaly/OutParty/@v
	8591824010402
	16
	Varchar

	21
	OutParty.codingScheme
	AR/TimeSeriesAnomaly/OutParty/@codingScheme
	A10
	3
	Varchar

	22
	MeasurementUnit
	AR/TimeSeriesAnomaly/MeasurementUnit/@v
	MAW
	5
	Varchar

	23
	TimeInterval  v UCT
(ve tvaru YYYY-MM-DDThh:00Z/YYYY-MM-DD+1Thh:00Z)
	AR/TimeSeriesAnomaly/Period/TimeInterval/@v
	2009-04-30T22:00Z/2009-05-01T22:00Z
	35
	Varchar

	24
	Resolution
	AR/TimeSeriesAnomaly/Period/Resolution/@v
	PT60M
	15
	Varchar

	25
	Interval - Pos
	AR/TimeSeriesAnomaly/Period/Interval/Pos/@v
	7
	6
	<1;999999>; Integer

	26
	Interval - Qty
	AR/TimeSeriesAnomaly/Period/Interval/Qty/@v
	41
	16,4
	<-9999999999999999.9999; 9999999999999999.9999>; Float

	27
	ReasonCode
	AR/TimeSeriesAnomaly/Reason/ReasonCode/@v
	A08
	3
	Varchar

	
	
	
	
	
	

	
	
	Mandatory field
	
	
	

	
	TS_001
	Example of valid value
	
	
	

	
	{10YSK-SEPS-----K ;
10YCZ-CEPS-----N}
	Enumeration of possible values (constants)
	
	
	

	
	A01
	Constant value
	
	
	


5.11.6 Messages in ETSO ESS Confirmation Report structure

	 
	 
	 
	 
	 
	 

	L.I.
	Description 
ESS Confirmation Report
	ConfirmationReport ==> CR
	Value
	Size
	Value/Type

	1
	MessageIdentification
	CR/MessageIdentification/@v
	20090401_A02_10XCZ-CEPS-GRIDE
	35
	Varchar

	2
	MessageType
	CR/MessageType/@v
	{A01; A09}
	3
	Varchar

	3
	MessageDateTime v UCT
(ve tvaru YYYY-MM-DDThh:mm:ssZ)
	CR/MessageDateTime/@v
	2009-04-01T09:30:30Z
	20
	Varchar

	4
	SenderIdentification
	CR/SenderIdentification/@v
	8591824000007
	16
	Varchar

	5
	SenderIdentification.codingScheme
	CR/SenderIdentification/@codingScheme
	A10
	3
	Varchar

	6
	SenderRole
	CR/SenderRole/@v
	A05
	3
	Varchar

	7
	ReceiverIdentification
	CR/ReceiverIdentification/@v
	8591824010402
	16
	Varchar

	8
	ReceiverIdentification.codingScheme
	CR/ReceiverIdentification/@codingScheme
	A10
	3
	Varchar

	9
	ReceiverRole
	CR/ReceiverRole/@v
	{A01; A04; A11}
	3
	Varchar

	10
	ScheduleTimeInterval v UCT
(ve tvaru YYYY-MM-DDThh:00Z/YYYY-MM-DD+1Thh:00Z)
	CR/ScheduleTimeInterval/@v
	2009-04-30T22:00Z/2009-05-01T22:00Z
	35
	Varchar

	11
	ConfirmedMessageIdentification
	CR/ConfirmedMessageIdentification/@v
	20080905_A01_10XCZ-CEPS-GRIDE_1
	35
	Varchar

	12
	ConfirmedMessageVersion
	CR/ConfirmedMessageVersion/@v
	1
	3
	Integer

	13
	Domain
	CR/Domain/@v
	10YDOM-CZ-DE-SKK
	18
	Varchar

	14
	Domain.codingScheme
	CR/Domain/@codingScheme
	A01
	3
	Varchar

	15
	SubjectParty
	CR/SubjectParty/@v
	8591824010402
	16
	Varchar

	16
	SubjectParty.codingScheme
	CR/SubjectParty/@codingScheme
	A10
	3
	Varchar

	17
	SubjectRole
	CR/SubjectRole/@v
	{A01; A04; A11}
	3
	Varchar

	18
	ProcessType
	CR/ProcessType/@v
	{A01; A02; A12}
	3
	Varchar

	19
	ReasonCode
	CR/Reason/ReasonCode/@v
	A06
	3
	Varchar

	20
	ReasonText
	CR/Reason/ReasonText/@v
	Schedule Accepted
	 
	Varchar

	21
	SendersTimeSeriesIdentification
	CR/TimeSeriesConfirmation/SendersTimeSeriesIdentification/@v
	TS_001
	35
	Varchar

	22
	SendersTimeSeriesVersion
	CR/TimeSeriesConfirmation/SendersTimeSeriesVersion/@v
	1
	3
	Integer

	23
	BusinesType
	CR/TimeSeriesConfirmation/BusinessType/@v
	{A02; A06}
	3
	Varchar

	24
	Product
	CR/TimeSeriesConfirmation/Product/@v
	8716867000016
	13
	Integer

	25
	ObjectAgregation
	CR/TimeSeriesConfirmation/ObjectAggregation/@v
	A03
	3
	Varchar

	26
	InArea
	CR/TimeSeriesConfirmation/InArea/@v
	10YCZ-CEPS-----N
	16
	Varchar

	27
	InArea.codingScheme
	CR/TimeSeriesConfirmation/InArea/@codingScheme
	A01
	3
	Varchar

	28
	OutArea
	CR/TimeSeriesConfirmation/OutArea/@v
	10YCZ-CEPS-----N
	16
	Varchar

	29
	OutArea.codingScheme
	CR/TimeSeriesConfirmation/OutArea/@codingScheme
	A01
	3
	Varchar

	30
	InParty
	CR/TimeSeriesConfirmation/InParty/@v
	8591824010402
	16
	Varchar

	31
	InParty.codingScheme
	CR/TimeSeriesConfirmation/InParty/@codingScheme
	A10
	3
	Varchar

	32
	OutParty
	CR/TimeSeriesConfirmation/OutParty/@v
	8591824010402
	16
	Varchar

	33
	OutParty.codingScheme
	CR/TimeSeriesConfirmation/OutParty/@codingScheme
	A10
	3
	Varchar

	34
	MeasurementUnit
	CR/TimeSeriesConfirmation/MeasurementUnit/@v
	MAW
	5
	Varchar

	35
	ReasonCode
	CR/TimeSeriesConfirmation/Reason/ReasonCode/@v
	A88
	3
	Varchar

	36
	ReasonText
	CR/TimeSeriesConfirmation/Reason/ReasonText/@v
	The time series has been successfully matched.
	 
	Varchar

	37
	TimeInterval  v UCT
(ve tvaru YYYY-MM-DDThh:00Z/YYYY-MM-DD+1Thh:00Z)
	CR/TimeSeriesConfirmation/Period/TimeInterval/@v
	2009-04-30T22:00Z/2009-05-01T22:00Z
	35
	Varchar

	38
	Resolution
	CR/TimeSeriesConfirmation/Period/Resolution/@v
	PT60M
	15
	Varchar

	39
	Interval - Pos
	CR/TimeSeriesConfirmation/Period/Interval/Pos/@v
	7
	6
	<1;999999>; Integer

	40
	Interval - Qty
	CR/TimeSeriesConfirmation/Period/Interval/Qty/@v
	41
	16,4
	<-9999999999999999.9999; 9999999999999999.9999>; Float

	
	
	
	
	
	

	
	
	Mandatory field
	
	
	

	
	TS_001
	Example of valid value
	
	
	

	
	11XSEBRATISLAVA4 or 8591824010402
	Example of valid values
	
	
	

	
	{10YSK-SEPS-----K ;
10YCZ-CEPS-----N}
	Enumeration of possible values (constants)
	
	
	

	
	A01
	Constant value
	
	
	


5.11.7 Messages in ETSO Status Request structure

	 
	 
	 
	MCC enquiry
	RD enquiry
	 
	 
	MCC enquiry
	RD enquiry

	L.I.
	Description
ETSO StatusRequest
	StatusRequest ==> SR
	Value
	Value
	Size
	Value/Type
	 
	 

	1
	MessageIdentification
	SR/MessageIdentification/@v
	20080905_A02_8591824010402_1
	20080905_A02_8591824010402_1
	35
	Varchar
	 
	 

	2
	MessageType
	SR/MessageType/@v
	 A13
	{A01; A09; A13}
	3
	Varchar
	 
	 

	3
	ProcessType
	SR/ProcessType/@v
	A07
	{A01; A02; A07; A12; A18}
	3
	Varchar
	 
	 

	4
	SenderIdentification
	SR/SenderIdentification/@v
	11XSEBRATISLAVA4 or 8591824010402
	8591824010402
	16
	Varchar
	 
	 

	5
	SenderIdentification.codingScheme
	SR/SenderIdentification/@codingScheme
	{A01; A10}
	A10
	3
	Varchar
	 
	 

	6
	SenderRole
	SR/SenderRole/@v
	{A07; A08; A11}
	{A01; A04; A11}
	3
	Varchar
	 
	 

	7
	ReceiverIdentification
	SR/ReceiverIdentification/@v
	27XOTE-CZECHREPB or
8591824010402
	8591824010402
	16
	Varchar
	 
	 

	8
	ReceiverIdentification.codingScheme
	SR/ReceiverIdentification/@codingScheme
	{A01; A10}
	A10
	3
	Varchar
	 
	 

	9
	ReceiverRole
	SR/ReceiverRole/@v
	A05
	A05
	3
	Varchar
	 
	 

	10
	MessageDateTime v UCT
(ve tvaru YYYY-MM-DDThh:mm:ssZ)
	SR/MessageDateTime/@v
	2009-05-01T07:10:30Z
	2009-05-01T07:10:30Z
	20
	Varchar
	 
	 

	11
	RequestedTimeInterval v UCT
(ve tvaru YYYY-MM-DDThh:00Z/YYYY-MM-DD+1Thh:00Z)
	SR/RequestedTimeInterval/@v
	2009-04-30T22:00Z/2009-05-01T22:00Z
	2009-04-30T22:00Z/2009-05-01T22:00Z
	35
	Varchar
	 
	 

	12
	ReqSenderIdentification
	SR/ReqSender/@v
	 
	8591824010402
	16
	Varchar
	 
	 

	13
	ReqSenderIdentification.codingScheme
	SR/ReqSubjectParty/@codingScheme
	 
	A10
	3
	Varchar
	 
	 

	14
	ReqSenderRole
	SR/ReqSenderRole/@v
	 
	{A01; A04; A11}
	3
	Varchar
	 
	 

	15
	ReqSubjectParty
	SR/ReqSubjectParty/@v
	 
	8591824010402
	16
	Varchar
	 
	 

	16
	ReqSubjectParty.codingScheme
	SR/ReqSubjectParty/@codingScheme
	 
	A10
	3
	Varchar
	 
	 

	17
	ReqSubjectRole
	SR/ReqSubjectRole/@v
	 
	A01
	3
	Varchar
	 
	 

	18
	ReqMatchingPeriod
	SR/ReqMatchingPeriod/@v
	 
	2009-04-30T22:00Z/2009-05-01T22:00Z
	35
	Varchar
	 
	 

	19
	ReqCounterparty
	SR/ReqCounterparty/@v
	 
	8591824010402
	 
	 
	 
	 

	 
	ReqCounterparty.codingScheme
	SR/ReqCounterparty/@codingScheme
	 
	A10
	 
	 
	 
	 

	20
	ReqBusinessType
	SR/BusinessType/@v
	 
	{A02; A06}
	3
	Varchar
	 
	 

	21
	ReqMessageIdentification
	SR/ReqMessageIdentification/@v
	 
	20080905_A02_8591824010402_1
	35
	Varchar
	 
	 

	22
	ReqMessageVersion
	SR/ReqMessageVersion/@v
	 
	1
	3
	Varchar
	 
	 

	
	
	
	
	
	
	
	
	

	
	 
	Field above ETSO specification
	
	
	
	
	
	

	
	 
	Mandatory field
	
	
	
	
	
	

	
	 
	Mandatory field (under some circumstances)
	
	
	
	
	
	

	
	TS_001
	Example of valid value
	
	
	
	
	
	

	
	11XSEBRATISLAVA4 or 8591824010402
	Example of valid values
	
	
	
	
	
	

	
	{A01; A10}
	Enumeration of possible values (constants)
	
	
	
	
	
	

	
	A05
	Constant value
	
	
	
	
	
	


5.11.8 Messages in ETSO Acknowledgement Document structure

	 
	 
	 
	 
	 
	 

	L.I.
	Description EAD
	AcknowledgementDocument ==> AD
	Value
	Size
	Value/Type

	1
	DocumentIdentification
	AD/DocumentIdentification/@v
	20090501_A13_27XOTE-CZECHREPB_1
	35
	Varchar

	2
	DocumentDateTime v UCT
(ve tvaru YYYY-MM-DDThh:mm:ssZ)
	AD/DocumentDateTime/@v
	2009-05-01T07:10:30Z
	20
	Varchar

	3
	SenderIdentification
	AD/SenderIdentification/@v
	8591824000007
	16
	Varchar

	4
	SenderIdentification.codingScheme
	AD/SenderIdentification/@codingScheme
	{A01; A10}
	3
	Varchar

	5
	SenderRole
	AD/SenderRole/@v
	A05
	3
	Varchar

	6
	ReceiverIdentification
	AD/ReceiverIdentification/@v
	8591824010402
	16
	Varchar

	7
	ReceiverIdentification.codingScheme
	AD/ReceiverIdentification/@codingScheme
	{A01; A10}
	3
	Varchar

	8
	ReceiverRole
	AD/ReceiverRole/@v
	{A07; A08; A11}
	3
	Varchar

	9
	ReceivingDocumentIdentification
	AD/ReceivingDocumentIdentification/@v
	20090501_A13_27XOTE-CZECHREPB
	35
	Varchar

	10
	ReceivingDocumentVersion
	AD/ReceivingDocumentVersion/@v
	01
	3
	<1;999>; Integer

	11
	ReceivingDocumentType
	AD/ReceivingDocumentType/@v
	A13
	3
	Varchar

	12
	DateTimeReceivingDocument v UCT
(ve tvaru YYYY-MM-DDThh:mm:ssZ)
	AD/DateTimeReceivingDocument/@v
	2009-05-01T07:10:30Z
	35
	Varchar

	13
	SendersTimeSeriesIdentification
	AD/TimeSeriesRejection/SendersTimeSeriesIdentification/@v
	TS_001
	35
	Varchar

	14
	SendersTimeSeriesVersion
	AD/TimeSeriesRejection/SendersTimeSeriesVersion/@v
	01
	3
	Integer

	15
	ReasonCode (Series)
	AD/TimeSeriesRejection/Reason/ReasonCode/@v
	A01
	3
	Varchar

	16
	QuantityTimeInterval
	AD/TimeSeriesRejection/TimeIntervalError/QuantityTimeInterval/@v
	2009-04-30T22:00Z/2009-05-01T22:00Z
	35
	Varchar

	17
	ReasonCode (Interval)
	AD/TimeSeriesRejection/TimeIntervalError/Reason/ReasonCode/@v
	A01
	3
	Varchar

	18
	ReasonCode (Document)
	AD/Reason/ReasonCode/@v
	A01
	3
	Varchar

	
	
	
	
	
	

	
	
	Mandatory field
	
	
	

	
	TS_001
	Example of valid value
	
	
	

	
	11XSEBRATISLAVA4 or 8591824010402
	Example of valid values
	
	
	

	
	{A01; A10}
	Enumeration of possible values (constants)
	
	
	

	
	A05
	Constant value
	
	
	


5.12 Allocation of profiles to IS OTE data 

The table below defines the method of individual payments/charges identification and related categories or type sof types energy in terms of external systems.

Column 1 – Payments/charges identification shortcut

Column 2 – Records identification with nternal interface tools of the IS OTE/CDS system

Column 3 – Payments/charges description 

Column 4 – Shows whether within 1 trading hour the payment/charge may be made either to the debit or to the benefit of the SS (yes – the dual status may become valid). For daily settlement information the whole matter is related to an imaginary „zero“ hour.

Column 5 – Specification of energy types and profile roles (see XML files structure) (N/A – no energy value is indicated; demand – buying (buy); supply – selling (sell); abs – absolute energy value), complete profile role description (including input and output values for separate commands) is specified in the table Profile role mapping for separate message codes (MSG_code) 

Column 6 – Payment and profile types description (see XML files structure)  (- payment; + automatic debit; +/- automatic debit is possible, but for one type per one trading hour), complete description of profile roles (including input and output values for separate commands) is specified in the table Profile role mapping for separate message codes (MSG_code)

Columns 7 to 9 – identically to columns 4 to 6

	 
	 
	Settlement
	Hourly data
	Daily data
	 Comment

	 
	 
	 
	 +/- prices in one hour
	energy
	price -  the sign is in terms of the SS part, but not the OTE
	 +/- prices in one hour (all Hour 0)
	energy
	price - the sign is in terms of the SS part, but not the OTE
	 

	AF
	Sx15
	Admission Fee – charge for the access to CDS
	no
	N/A
	- (ST15)
	No
	N/A
	- (ST15)
	Since February 2003 

	CF
	Sx01
	Consumption Fee – charge for consumption
	no
	demand (SC01)
	- (SP01)
	no
	demand (SC01)
	- (SP01)
	 

	DMS
	Sx02
	Day-ahead market Settlement (buy) - negative energy (spot bids)
	no
	demand (SC02)
	- (SP02)
	no
	demand (SC02)
	- (SP02)
	 

	
	Sx03
	Day-ahead market Settlement (sell) - positive energy (spot bids)
	no
	supply (SC03)
	+ (SP03)
	no
	supply (SC03)
	+ (SP03)
	 

	
	Sx36
	Day-ahead Market Settlement (buy) - settlement DM negative energy (bids FS)
	no
	demand (SC36)
	- (SP36)
	no
	demand (SC36)
	- (SP36)
	 Since January 2011

	
	Sx37
	Day-ahead Market Settlement (sell)- settlement DM positive energy (bids FS)
	no
	supply (SC37)
	+ (SP37)
	no
	supply (SC37)
	+ (SP37)
	 Since January 2011

	PXE
	Sx11
	Day-ahead market Settlement PXE buying – accumulated position PXE negative energy (spot market)
	no
	demand (SC11)
	- (SP11)
	no
	demand (SC11)
	- (SP11)
	Since February 2009

	
	Sx12
	Day-ahead market Settlement PXE selling – accumulated position PXE positive energy (spot market)
	no
	supply (SC12)
	+ (SP12)
	no
	supply (SC12)
	+ (SP12)
	Since February 2009

	
	Sx77
	Day-ahead market Settlement PXE buying – accumulated position PXE negative energy (futures)
	no
	demand (SC77)
	- (SP77)
	no
	demand (SC77)
	- (SP77)
	Since January 2011

	
	Sx78
	Day-ahead market Settlement PXE selling – accumulated position PXE positive energy (futures)
	no
	supply (SC78)
	+ (SP78)
	no
	supply (SC78)
	+ (SP78)
	Since January 2011

	EC
	Sx04
	Extra Cost – additional cost value
	no
	abs (SC04)
	+ (SP04)
	yes
	abs (SC04)
	+ (SP04)
	 

	
	Sx54
	
	
	abs (SC54)
	- (SP54)
	
	abs (SC54)
	- (SP54)
	 

	EI
	ST17
	Extra imbalance RE - RE settlement surplus amount
	no
	N/A
	+(ST17)
	no
	N/A
	+(ST17)
	Since January 2007

	FMD
	Sx05
	Day-ahead market Fee
	no
	abs (SC05)
	- (SP05)
	no
	abs (SC05)
	- (SP05)
	 

	IEM
	Sx06
	Consolidate Imbalance Minus – Consolidated negative deviation
	no
	demand (SC06)
	+ (SP06)
	yes
	demand (SC06)
	+ (SP06)
	Since February - April 2003 depending on settlement version

	
	Sx56
	
	
	demand (SC56)
	- (SP56)
	
	demand (SC56)
	- (SP56)
	

	IEP
	Sx07
	Consolidate Imbalance Plus - Consolidated positive deviation
	no
	supply (SC07)
	+ (SP07)
	yes
	supply (SC07)
	+ (SP07)
	

	
	Sx57
	
	
	supply (SC57)
	- (SP57)
	
	supply (SC57)
	- (SP57)
	

	IESM
	Sx55
	Aggregated Imbalance SSS Minus
	no
	demand (XC02)
	+ (XP02)
	yes
	demand (XC02)
	+ (XP02)
	generated only for SSS

	
	Sx52
	
	
	demand (XC52)
	- (XP52)
	
	demand (XC52)
	- (XP52)
	

	IESP
	Sx53
	Aggregated Imbalance SSS Plus
	no
	supply (XC01)
	+ (XP01)
	yes
	supply (XC01)
	+ (XP01)
	

	
	Sx60
	
	
	supply (XC51)
	- (XP51)
	
	supply (XC51)
	- (XP51)
	

	IFF
	Sx14
	Intraday Balance Fee (price)
	no
	N/A
	- (ST14)
	no
	N/A
	- (ST14)
	Not activated

	IMM
	Sx08
	Intraday Market Minus - negative energy
	yes
	demand (SC08)
	+ (SP08)
	yes
	demand (SC08)
	+ (SP08)
	 

	
	Sx58
	
	
	demand (SC58)
	- (SP58)
	
	demand (SC58)
	- (SP58)
	 

	IMP
	Sx09
	Intraday Market Plus - positive energy
	yes
	supply (SC09)
	+ (SP09)
	yes
	supply (SC09)
	+ (SP09)
	 

	
	Sx59
	
	
	supply (SC59)
	- (SP59)
	
	supply (SC59)
	- (SP59)
	 

	IMF
	Sx10
	Intraday Market Fee
	no
	abs (SC10)
	- (SP10)
	no
	abs (SC10)
	- (SP10)
	Not activated

	IS
	Sx17
	Imbalance Settlement – Positive deviation
	no
	supply (SC17)
	+/- (SP17)
	not used
	

	
	Sx18
	Imbalance Settlement – Negative deviation
	no
	demand (SC18)
	+/- (SP18)
	not used
	

	OF
	Sx16
	Monthly Fee - Monthly fee (for SS) - negative price
	no
	N/A
	- (ST16)
	no
	N/A 
	- (ST16)
	 

	SSM
	Sx12
	Auxiliary Services Minus - Negative energy support services
	no
no
	demand (SF12)
	+ (SG12)
	yes
	demand (SF12)
	+ (SG12)
	Is generated only if energy value <> 0

	
	Sx62
	
	
	demand (SF62)
	- (SG62)
	
	demand (SF62)
	- (SG62)
	

	SSP
	Sx11
	Auxiliary Services Plus - Positive energy support services
	no
	supply (SF11)
	+ (SG11)
	yes
	supply (SF11)
	+ (SG11)
	Is generated only if energy value <> 0

	
	Sx61
	
	
	supply (SF61)
	- (SG61)
	
	supply (SF61)
	- (SG61)
	

	EM+
	Sx29
	Emergency supply
	no
no
	supply (SC29)
	+ (SP29)
	yes*
	supply (SC29)
	+ (SP29)
	* Provided the unit price value would be negative

	
	Sx79
	
	
	supply (SC79)*
	- (SP79)*
	
	supply (SC79)*
	- (SP79)*
	

	EM-
	Sx30
	Emergency demand
	no
	demand (SC30)
	- (SP30)
	yes*
	demand (SC30)
	- (SP30)
	* Provided the unit price value would be negative

	
	Sx80
	
	
	demand (SC80)*
	+ (SP80)*
	
	demand (SC80)*
	+ (SP80)*
	

	LP
	Sx27
	Clearing LP Minus - LP negative energy settlement
	not used
	no
	demand (SC27)
	- (SP27)
	 
 

	
	Sx28
	Clearing LP Plus - LP positive energy settlement
	
	
	supply (SC28)
	+ (SP28)
	

	BM
	Sx33
	Block Market Settlement buy - negative energy
	not used
	no
	demand (SC33)
	- (SP33)
	Since February 2008

	
	Sx34
	Block Market Settlement buy - positive energy
	
	no
	supply (SC34)
	+ (SP34)
	

	BMF
	Sx35
	Block Market Fee
	not used
	no
	abs (SC35)
	- (SP35)
	Since February 2008

	GDS
	Sx02
	Gas Day-ahead market Settlement - buy – negative energy
	not used
	no
	demand (SC02)
	- (SP02)
	since 1.1.2010

	
	Sx03
	Gas Day-ahead market Settlement - sell – positive energy
	
	no
	supply (SC03)
	+ (SP03)
	

	GDF
	Sx05
	Gas Day-ahead market Fee
	not used
	no
	abs (SC05)
	- (SP05)
	since 1.1.2010

	GMF
	Sx16
	Gas Monthly Fee – negative price
	not used
	no
	not used
	- (ST16)
	since 1.1.2010

	GCF
	Sx15
	Gas Metering Data Fee – negative price
	not used
	no
	not used
	- (ST15)
	since 1.1.2010

	GIS
	Sx33
	Gas Intraday market Settlement – buy – negative energy
	not used
	no
	demand (SC33)
	- (SP33)
	since 1.4.2010

	
	Sx34
	Gas Intraday market Settlement - sell – positive energy
	
	no
	supply (SC34)
	+ (SP34)
	

	GIF
	Sx35
	Gas Intraday market Fee
	not used
	no
	abs (SC35)
	- (SP35)
	since 1.4.2010

	 
	 
	Final plan (always hourly value)
	 +/- price within one hour
	energy
	price – the sign is in terms of the SS part, but not the OTE
	not used
	 

	ERD
	Sx23
	Daily RD - buy 
	yes*
	demand (SC23)
	- (SP23)*
	
	* Provided the RRD clearing will be used.

	
	Sx73
	
	
	demand (SC73)*
	+ (SP73)*
	
	

	
	Sx24
	Daily RD - sell 
	yes*
	supply (SC24)
	- (SP24)*
	
	

	
	Sx74
	
	
	supply (SC74)*
	+ (SP74)*
	
	

	
	Sx25
	External RD - buy 
	yes*
	demand (SC25)
	- (SP25)*
	
	

	
	Sx75
	
	
	demand (SC75)*
	+ (SP75)*
	
	

	
	Sx26
	External RD - sell 
	yes*
	supply (SC26)
	- (SP26)*
	
	

	
	Sx76
	
	
	supply (SC76)*
	+ (SP76)*
	
	

	OKO
	Sx19
	DM - buy (spot bid)
	no
	demand (SC19)
	- (SP19)
	
	 

	
	Sx20
	DM - sell (spot bid)
	no
	supply (SC20)
	+ (SP20)
	
	

	
	Sx50
	DM - buy (FS bid)
	no
	demand (SC50)
	not used
	
	

	
	Sx51
	DM - sell (FS bid)
	no
	supply (SC51)
	not used
	
	 

	VDT
	Sx21
	Intraday Market - buy 
	yes
	demand (SC21)
	+ (SP21)
	
	 

	
	Sx71
	
	
	demand (SC71)
	- (SP71)
	
	 

	
	Sx22
	Intraday Market - sell 
	yes
	supply (SC22)
	+ (SP22)
	
	 

	
	Sx72
	
	
	supply (SC72)
	- (SP72)
	
	 

	BM
	Sx31
	BM - buy 
	no
	demand (SC31)
	- (SP31)
	
	Since February 2008

	
	Sx32
	BM - sell
	no
	supply (SC32)
	+ (SP32)
	
	

	 
	 
	Statistical data of imbalance settlement (always values per hour)
	 +/- prices in one hour
	energy
	price 
	not used
	 

	
	SS13
	System imbalance
	no
	+/- (SC13)
	not used
	
	 

	
	SS17
	Positive imbalances
	no
	+ (SC17)
	not used
	
	 

	
	SS18
	Negative imbalances
	no
	- (SC18)
	not used
	
	 

	
	SS50
	Settlement price
	yes
	not used
	+/- (SP50)
	
	 

	
	SS14
	Expenses RE
	yes
	not used
	+/- (SP14)
	
	 

	
	SS15
	Volume RE+
	no
	+ (SC15)
	not used
	
	 

	
	
	Expenses RE+
	no
	not used
	+ (SP15)
	
	 

	
	SS16
	Volume RE-
	no
	- (SC16)
	not used
	
	 

	
	
	Expenses RE-
	yes
	not used
	+/- (SP16)
	
	 

	
	SS51
	Price of contrary imbalance
	yes
	not used
	+/- (SP51)
	
	since 1.1.2010

	
	SS52
	Volume RE+ from BalM
	no
	+ (SC52)
	not used
	
	 

	
	
	Expenses RE+ from BalM
	no
	not used
	+ (SP52)
	
	 

	
	SS53
	Volume RE- from BalM
	no
	- (SC53)
	not used
	
	

	
	
	Expenses RE- from BalM
	yes
	not used
	+/- (SP53)
	
	

	
	SS55
	Rounding of imbalances
	no
	+/- (SC55)
	+/- (SP55)
	
	

	 
	
	
	
	
	
	
	
	
	 

	 
	
	
	
	
	
	
	
	
	 

	 
	 
	DM and Gas DM marginal prices
	
	
	price 
	not used
	 

	 OKO
	Sx20
	Marginal price 
	no
	
	+ (SP20)
	
	 

	 
	
	
	
	
	
	
	
	
	 

	 
	
	
	
	
	
	
	
	
	 

	 
	 
	RD - trade
	 
	energy
	price
	not used
	 

	ERD
	xx25
	RD - buy 
	no
	demand (C25)
	+/- (P25)*
	
	* Provided the RRD clearing will be used. Profile  C26 is used for Exchange market trade.

	
	xx26
	RD - sell 
	no
	supply (C26)
	+/- (P26)*
	
	

	Xxx
	xx13
	Default trade cancellation date
	 
	 
	 
	
	T13


Profile role mapping for separate message codes (MSG_code)

	Role in external interface
	  Description
	Msg_code

	BC01-25
	Trading block identification (block 1 to 25) – volume
	811,813,821,823,833, GD1, GD3, GD6, GD9

	BP01-25
	Trading block identification (block 1 až 25) - price
	811,813,821,823,833, GD1, GD3, GD6, GD9

	C25
	Bilateral contracts – buying (energy buy)
	741, 743, 753, 763, 733, 783

	C26
	Bilateral contracts – selling (energy sell)
	741, 743, 753, 763, 733, 783

	C71
	Traded volume – buy (IM&BalM)
	851, 871, 853, 863, 873, 883, 893, 903, 933

	C72
	Traded volume – sell  (IM&BalM)
	851, 871, 853, 863, 873, 883, 893, 903

	C73
	Accepted at IM – buy
	853, 863, 873, 883

	C74
	Accepted at IM – sell
	853, 863, 873, 883

	C75
	Accepted at BalM – buy
	853, 863, 873, 883

	C76
	Accepted at BalM - sell
	853, 863, 873, 883

	P25
	Bilateral contracts – buy (price)
	741, 743, 753, 763, 733, 783

	P26
	Bilateral contracts - sell (price)
	741, 743, 753, 763, 733, 783

	P71
	Traded volume price – buy
	851, 871, 853, 863, 873, 883, 893, 903, 933

	P72
	Traded volume price – sell
	851, 871, 853, 863, 873, 883, 893, 903, 933

	R01
	Settlement OTE rate
	427

	SC01
	Consumption Fee - negative energy for negative price value consumption charge
	953, 963

	SC02
	Day-ahead market, Gas DM Settlement buy - negative energy for negative price value (spot bids)
	953, 963, GSF

	SC03
	Day-ahead market, Gas DM Settlement sell - positive energy for positive price value (spot bids)
	953, 963, GSF

	SC04
	Extra Cost – additional cost value - energy for positive price value
	953, 963

	SC05
	Day-ahead market, Gas DM Fee - energy for negative price value
	953, 963, GSF

	SC06
	Consolidate Imbalance Minus – Consolidated deviation - negative energy for positive price value (deviation + EC)
	953, 963

	SC07
	Consolidate Imbalance Plus - Consolidated deviation - positive energy for positive price value (deviation + EC)
	953, 963

	SC08
	Intraday Market Minus - negative energy for positive price value
	953, 963

	SC09
	Intraday Market Plus - positive energy for positive price value
	953, 963

	SC10
	Intraday Market Fee - energy for negative price value
	953, 963

	SC11
	Day-ahead market settlement PXE – buy

Matching  volumes of PXE-spot market purchase bids
	953, 963

	SC12
	Day-ahead market settlement PXE – sell

Matching  volumes of PXE-spot market sales bids
	953, 963

	SC13
	Statistical data of imbalance settlement - System imbalance
	966

	SC15
	Statistical data of imbalance settlement - Volume RE+
	966

	SC16
	Statistical data of imbalance settlement - Volume RE-
	966

	SC17
	Imbalance Settlement – Deviation - positive energy
	953, 966

	SC18
	Imbalance Settlement – Deviation – negative energy
	953, 966

	SC19
	Final plan – DM - negative energy for negative price value (spot bids)
	943

	SC20
	Final plan – DM – positive energy for positive price value (spot bids)
	943

	SC21
	Final plan – IM - negative energy for positive price value
	943

	SC22
	Final plan – IM - positive energy for positive price value
	943

	SC23
	Final plan – daily RD - negative energy for negative price value
	943

	SC24
	Final plan – daily RD - positive energy for negative price value
	943

	SC25
	Final plan – external RD - negative energy for negative price value
	943

	SC26
	Final plan – external RD - positive energy for negative price value
	943

	SC27
	Clearing LP Minus - LP settlement - negative energy for negative price value
	953, 963

	SC28
	Clearing LP Plus - LP settlement - positive energy for positive price value
	953, 963

	SC29
	Emergency supply - positive energy for positive price value
	953, 963

	SC30
	Emergency demand - negative energy for negative price value
	953, 963

	SC31
	Final plan – BM - negative energy for negative price value
	943

	SC32
	Final plan – BM – positive energy for positive price value
	943

	SC33
	Block Market and Gas IM Settlement buy - negative energy for negative price value (summarized for all instance types)
	953, 963, GSF

	SC34
	Block Market and Gas IM Settlement sell - positive energy for positive price value (summarized for all instance types)
	953, 963, GSF

	SC35
	Block Market and Gas IM Fee - energy for negative price value
	953, 963, GSF

	SC36
	Day-ahead Market Settlement Buy – Settlement DM (FS bids) – negative energy
	953, 963

	SC37
	Day-ahead Market Settlement Sell - Settlement DM (FS bids) – positive energy
	953, 963

	SC40
	Block Market, Gas IM – Trading Screen – negative energy for negative price value
	869, GVK

	SC41
	Block Market, Gas IM – Trading Screen – positive energy for positive price value
	869, GVK

	SC42
	Block Market, Gas IM – Trading Screen – Number of contracts traded during the current day
	869, GVK

	SC44
	Block Market, Gas IM – Trading Screen – Number of contracts traded during the entire instance (product) trading period
	869, GVK

	SC46
	Number of BM and Gas IM order contracts - buy
	854, 856, 859, 866, GV1, GV3, GV6, GV9

	SC47
	Number of traded BM and Gas IM order contracts - buy
	854, 856, 859, 866, GV1, GV3, GV6, GV9

	SC48
	Number of BM and Gas IM trading contracts – buy 
	874, 876, GVE

	SC49
	BM and Gas IM trading volume – buy
	874, 876, GVE

	SC50
	Final plan – DM – negative energy (FS bids)
	943

	SC51
	Final plan – DM – positive energy (FS bids)
	943

	SC54
	Extra Cost – energy for negative price value
	953, 963

	SC56
	Consolidate Imbalance Minus - Consolidated deviation - negative energy for negative price value (deviation + EC)
	953, 963

	SC57
	Consolidate Imbalance Plus - Consolidated deviation - positive energy for negative price value (deviation + EC)
	953, 963

	SC58
	Intraday Market Minus - negative energy for negative price value
	953, 963

	SC59
	Intraday Market Plus - positive energy for negative price value
	953, 963

	SC60
	DM volume - area CZ - sell
	936

	SC61
	DM volume - area SK - buy
	936

	SC62
	DM volume - flow CZ - SK
	936

	SC63
	DM price area SK
	936

	SC64
	DM volume - area SK - buy
	936

	SC65
	DM volume - Flow SK - CZ
	936

	SC66
	DM - total volume
	936, 939

	SC67
	DM – system volume 
	936

	SC68
	DM – required flow CZ-SK
	936

	SC69
	DM - required flow SK-CZ
	936

	SC71
	Final plan – IM - negative energy for negative price value
	943

	SC72
	Final plan – IM - positive energy for negative price value
	943

	SC73
	Final plan – BC - negative energy for positive price value
	943

	SC74
	Final plan – BC - positive energy for positive price value
	943

	SC77
	Day-ahead Market settlement PXE – buy (bids FS)

Matching  volumes of PXE-futures purchase bids
	953, 963

	SC78
	Day-ahead Market settlement PXE – sell (bids FS)

Matching volumes of PXE-futures sales bids
	953, 963

	SC79
	Emergency supply - positive energy for negative price value
	953, 963

	SC80
	Emergency demand - negative energy for positive price value
	953, 963

	SC96
	Number of BM / Gas IM order contracts - sell
	854, 856, 859, 866, GV1, GV3, GV6, GV9

	SC97
	Number of traded BM / Gas IM order contracts - sell
	854, 856, 859, 866, GV1, GV3, GV6, GV9

	SC98
	Number of BM / Gas IM traiding contracts – sell
	874, 876, GVE

	SC99
	BM / Gas IM trading volume – sell
	874, 876, GVE

	SF11
	Auxiliary Services Plus - Support services - positive energy for positive price value
	953, 963

	SF12
	Auxiliary Services Minus - Support services - negative energy for positive price value
	953, 963

	SF61
	Auxiliary Services Plus - Support services - positive energy for negative price value
	953, 963

	SF62
	Auxiliary Services Minus - Support services - negative energy for negative price value
	953, 963

	SG11
	Auxiliary Services Plus - Support services - positive price for positive energy–
	953, 963

	SG12
	Auxiliary Services Minus - Support services - positive price for negative energy
	953, 963

	SG61
	Auxiliary Services Plus - Support services – negative price for positive energy
	953, 963

	SG62
	Auxiliary Services Minus - Support services - negative price for negative energy
	953, 963

	SP01
	Consumption Fee - consumption charge - negative price for negative energy
	953, 963

	SP02
	Day-ahead market / Gas DM Settlement buy - negaive price for negative energy (spot bids)
	953, 963, GSF

	SP03
	Day-ahead market / Gas DM Settlement sell - positive price for positive energy (spot bids)
	953, 963, GSF

	SP04
	Extra Cost – additional cost value - positive price
	953, 963

	SP05
	Day-ahead market / Gas DM Fee - negative price
	953, 963, GSF

	SP06
	Consolidate Imbalance Minus - Consolidated deviation - positive price for negative energy (deviation + EC)
	953, 963

	SP07
	Consolidate Imbalance Plus - Consolidated deviation - positive price for positive energy (deviation + EC)
	953, 963

	SP08
	Intraday Market Minus - positive price for negative energy
	953, 963

	SP09
	Intraday Market Plus - positive price for positive energy
	953, 963

	SP10
	Intraday Market Fee - negative price
	953, 963

	SP11
	Day-ahead market settlement PXE – buy

Negative price of matching volumes of PXE-spot market bids
	953, 963

	SP12
	Day-ahead market settlement PXE – sell

Positive price of matching volumes of PXE-spot market bids
	953, 963

	SP17
	Imbalance Settlement – Deviation - price for positive energy
	953

	SP18
	Imbalance Settlement – Deviation - price for negative energy
	953

	SP19
	Final plan – DM – negative price for negative energy
	943

	SP20
	Final plan – DM – positive price for positive energy; DM / Gas DM marginal prices
	943, 946, GDF

	SP21
	Final plan – IM - positive price for negative energy
	943

	SP22
	Final plan – IM - positive price for positive energy
	943

	SP23
	Final plan – daily RD - negative price for negative energy
	943

	SP24
	Final plan – daily RD - negative price for positive energy
	943

	SP25
	Final plan – external RD - negative price for negative energy
	943

	SP26
	Final plan – external RD - negative price for positive energy
	943

	SP27
	Clearing LP Minus - LP settlement - negative price for negative energy
	953, 963

	SP28
	Clearing LP Plus - LP settlement - positive price for positive energy
	953, 963

	SP29
	Emergency supply - positive price for positive energy
	953, 963

	SP30
	Emergency demand - negative price for negative energy
	953, 963

	SP31
	Final plan – BM – negative price negative energy
	943

	SP32
	Final plan – BM – positive price for positive energy
	943

	SP33
	Block Market / Gas IM Settlement buy - negative price for negative energy (summarized for all instance types)
	953, 963, GSF

	SP34
	Block Market / Gas IM Settlement sell - positive price for positive energy (s summarized for all instance types)
	953, 963, GSF

	SP35
	Block Market / Gas IM Fee - negative price
	953, 963, GSF

	SP36
	Day-ahead Market Settlement Buy – Settlement DM (FS bids) – negative price for negative energy
	953, 963

	SP37
	Day-ahead Market Settlement Sell - Settlement DM (FS bids) – positive price for positive energy
	953, 963

	SP40
	Block Market / Gas IM – negative price for negative energy
	869, GVK

	SP41
	Block Market / Gas IM – Trading Screen – positive price for positive energy
	869, GVK

	SP42
	Block Market / Gas IM – Trading Screen – Bottom price of the current day
	869, GVK

	SP43
	Block Market / Gas IM – Trading Screen – Ceiling price of the current day
	869, GVK

	SP44
	Block Market / Gas IM – Trading Screen – Bottom price of the entire instance (product) trading period
	869, GVK

	SP45
	Block Market / Gas IM – Trading Screen – Ceiling price of the entire instance (product) trading period
	869, GVK

	SP46
	Order limited prices – buy
	854, 856, 859, 866, GV1, GV3, GV6, GV9

	SP48
	Trading limited prices – buy 
	874, 876, GVE

	SP49
	Total trade amount – buy 
	874, 876, GVE

	SP54
	Extra Cost - negative price
	953, 963

	SP56
	Consolidate Imbalance Minus - Consolidated deviation - negative price for negative energy (deviation + EC)
	953, 963

	SP57
	Consolidate Imbalance Plus - Consolidated deviation - negative price for positive energy (deviation + EC)
	953, 963

	SP58
	Intraday Market Minus - negative price for negative energy
	953, 963

	SP59
	Intraday Market Plus - negative price for positive energy
	953, 963

	SP60
	Area CZ DM price
	936

	SP63
	Area SK DM price 
	936

	SP67
	DM – system price
	936

	SP71
	Final plan – IM - negative price for negative energy
	943

	SP72
	Final plan – IM - negative price for positive energy
	943

	SP73
	Final plan – daily RD - positive price for negative energy
	943

	SP74
	Final plan – daily RD - positive price for positive energy
	943

	SP75
	Final plan – external RD - positive price for negative energy
	943

	SP76
	Final plan – external RD - positive price for positive energy
	943

	SP77
	Day-ahead market settlement PXE – buy (bids FS)

Negative price of matching volumes of PXE-futures market bids
	953, 963

	SP78
	Day-ahead market settlement PXE – sell (bids FS)

Positive price of matching volumes of PXE-futures market bids
	953, 963

	SP79
	Emergency supply - negative price for positive energy
	953, 963

	SP80
	Emergency demand - positive price for negative energy
	953, 963

	SP96
	Order limit price - sell
	854, 856, 859, 866, GV1, GV3, GV6, GV9

	SP98
	Trading limit price – sell
	874, 876, GVE

	SP99
	Total trade amount – sell 
	874, 876, GVE

	ST14
	Intraday Balance Fee - Market regulation fee - negative price
	953, 963

	ST15
	Admission Fee - charge for the access to CDS – negative price
	953, 963, GSF

	ST16
	Monthly Fee - Monthly charge (for SS) – negative price
	953, 963, GSF

	ST17
	RE settlement surplus 
	953, 963

	T11
	Trading hours opening time (date and hour)
	913

	T12
	Trading hours closing time (date and hour)
	913

	T13
	Default trade cancellation time (date and time)
	793

	XC01
	Aggregated Imbalance SSS Plus - positive energy for positive price value (MWh)
	953, 963

	XC02
	Aggregated Imbalance SSS Minus - negative energy for positive price value (MWh)
	953, 963

	XC51
	Aggregated Imbalance SSS Plus - positive energy for negative price value (MWh)
	953, 963

	XC52
	Aggregated Imbalance SSS Minus - negative energy for negative price value (MWh)
	953, 963

	XP01
	Payments for Aggregated Imbalance SSS Plus - positive price for positive energy (CZK)
	953, 963

	XP02
	Payments for Aggregated Imbalance SSS Minus - positive price for negative energy (CZK)
	953, 963

	XP51
	Payments for Aggregated Imbalance SSS Plus - negative price for positive energy (CZK)
	953, 963

	XP52
	Payments for Aggregated Imbalance SSS Minus - negative price for negative energy (CZK)
	953, 963


The report message 869 consists of 12 records according to the trading hours indexes:

· Records 1 to 5 contain five top orders (buy) of the day

· Records 6 to 10 contain five top orders (sell) of the day

· Record 11 contains daily statistics related to instance (product) trading

· Record 12 contains statistics related to the entire instance (product) trading period
The report message 876 consists of 2 records according to the trading hours indexes:

· Record 1 contains information about the trading price and  the number of contracts (interface items 4 and 7)

· Record 2 contains information about the volume and the total trading amount (interface items 3 and 4)

Explanatory note:

Alphabetic character S, X means the SS total amount (summarised), SSS

Alphabetic character C means traded/planned value 

Alphabetic character P means price – introduced within IM&BalM

Alphabetic character T means a charge/fee independent on energy or date

Alphabetic character F in this case traditionally means RE in CDS

Alphabetic character G in this case traditionally means RE in CDS

Alphabetic character R means currency value rate, ratio
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